{"text_format":"2","workbook":"xlsx","n_sheets":10,"sheets":["Revision","EthConfigData","WifiConfigData","TeleConfigData","SysConfigData","SysInfoData","ChargingInfoData","PSU","Chademo","OCPP"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Revision","index":0,"n_rows":10,"n_cols":19,"rows_kept":10,"cut":false,"hidden":false,"merged":[[2,4,5,21],[7,2,7,21],[8,2,8,3],[8,4,8,7],[8,8,8,17],[8,18,8,21],[9,2,9,3],[10,2,10,3],[11,2,11,3],[12,2,12,3],[13,2,13,3],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,2,20,3],[21,2,21,3],[22,2,22,3],[23,2,23,3],[24,2,24,3],[25,2,25,3],[26,2,26,3],[9,4,9,7],[10,4,10,7],[11,4,11,7],[12,4,12,7],[13,4,13,7],[14,4,14,7],[15,4,15,7],[16,4,16,7],[17,4,17,7],[18,4,18,7],[19,4,19,7],[20,4,20,7],[21,4,21,7],[22,4,22,7],[23,4,23,7],[24,4,24,7],[25,4,25,7],[26,4,26,7],[9,8,9,17],[10,8,10,17],[11,8,11,17],[12,8,12,17],[13,8,13,17],[14,8,14,17],[15,8,15,17],[16,8,16,17],[17,8,17,17],[18,8,18,17],[19,8,19,17],[20,8,20,17],[21,8,21,17],[22,8,22,17],[23,8,23,17],[24,8,24,17],[25,8,25,17],[26,8,26,17],[9,18,9,21],[10,18,10,21],[11,18,11,21],[12,18,12,21],[13,18,13,21],[14,18,14,21],[15,18,15,21],[16,18,16,21],[17,18,17,21],[18,18,18,21],[19,18,19,21],[20,18,20,21],[21,18,21,21],[22,18,22,21],[23,18,23,21],[24,18,24,21],[25,18,25,21],[26,18,26,21]]}
[]
[]
[{"$nulls":4},"Define.h file"]
[]
[]
[]
[]
[null,null,"Revision History"]
[null,null,"Rev",null,"Date",null,null,null,"Description",{"$nulls":9},"Editor"]
[null,null,"01",null,"2019-08-08",null,null,null,"First issue",{"$nulls":9},"Alston Lin"]

{"sheet":"EthConfigData","index":1,"n_rows":6,"n_cols":10,"rows_kept":6,"cut":false,"hidden":false,"merged":[[10,0,10,2],[5,0,5,2],[6,0,6,2],[7,0,7,2],[8,0,8,2],[9,0,9,2],[0,0,0,2],[1,0,1,2],[2,0,2,2],[3,0,3,2],[4,0,4,2],[19,0,19,2],[20,0,20,2],[21,0,21,2],[22,0,22,2],[11,0,11,2],[14,0,14,2],[15,0,15,2],[16,0,16,2],[17,0,17,2],[18,0,18,2],[4,9,4,20],[35,0,35,2],[24,0,24,2],[25,0,25,2],[26,0,26,2],[27,0,27,2],[28,0,28,2],[29,0,29,2],[30,0,30,2],[31,0,31,2],[32,0,32,2],[33,0,33,2],[34,0,34,2],[23,0,23,2],[12,0,12,2],[13,0,13,2],[4,3,4,8],[5,3,5,8],[6,3,6,8],[7,3,7,8],[8,3,8,8],[0,3,0,8],[0,9,0,20],[1,3,1,8],[2,3,2,8],[3,3,3,8],[1,9,1,20],[2,9,2,20],[3,9,3,20],[5,9,5,20],[11,3,11,8],[12,3,12,8],[13,3,13,8],[14,3,14,8],[6,9,6,20],[7,9,7,20],[8,9,8,20],[9,9,9,20],[10,9,10,20],[11,9,11,20],[10,3,10,8],[9,3,9,8],[15,3,15,8],[12,9,12,20],[13,9,13,20],[14,9,14,20],[15,9,15,20]]}
["Data type",null,null,"Define",{"$nulls":5},"Comment"]
["unsigned char",null,null,"EthDhcpClient",{"$nulls":5},"0: enable,1: disable"]
["unsigned char",null,null,"EthMacAddress[18]",{"$nulls":5},"default: Null"]
["unsigned char",null,null,"EthIpAddress[16]",{"$nulls":5},"Eth0 default:192.168.0.10\t,Eth1 default:192.168.1.10"]
["unsigned char",null,null,"EthSubmaskAddress[16]",{"$nulls":5},"Eth0 default:255.255.255.0\t,Eth1 default:255.255.255.0"]
["unsigned char",null,null,"EthGatewayAddress[16]",{"$nulls":5},"Eth0 default:192.168.0.254\t,Eth1 default:192.168.1.254"]

{"sheet":"WifiConfigData","index":2,"n_rows":12,"n_cols":10,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,0,0,2],[0,3,0,8],[0,9,0,20],[1,0,1,2],[1,3,1,8],[1,9,1,20],[2,0,2,2],[2,3,2,8],[2,9,2,20],[3,0,3,2],[3,3,3,8],[3,9,3,20],[4,0,4,2],[4,3,4,8],[4,9,4,20],[5,0,5,2],[5,3,5,8],[5,9,5,20],[6,0,6,2],[6,3,6,8],[6,9,6,20],[7,0,7,2],[7,3,7,8],[7,9,7,20],[8,0,8,2],[8,3,8,8],[8,9,8,20],[9,0,9,2],[9,3,9,8],[9,9,9,20],[10,0,10,2],[10,3,10,8],[10,9,10,20],[11,0,11,2],[11,3,11,8],[11,9,11,20],[12,0,12,2],[12,3,12,8],[12,9,12,20],[13,0,13,2],[13,3,13,8],[13,9,13,20],[14,0,14,2],[14,3,14,8],[14,9,14,20],[15,0,15,2],[15,3,15,8],[15,9,15,20]]}
["Data type",null,null,"Define",{"$nulls":5},"Comment"]
["unsigned char",null,null,"WifiMode",{"$nulls":5},"0: disable, 1: Infrastructure client, 2: Infrastructure server, 3: Ad-Hoc"]
["unsigned char",null,null,"WifiSsid[256]",{"$nulls":5},"default: Null"]
["unsigned char",null,null,"WifiPassword[256]",{"$nulls":5},"default: Null"]
["int",null,null,"WifiRssi",{"$nulls":5},"dbm"]
["unsigned char",null,null,"WifiDhcpServer",{"$nulls":5},"0: enable, 1: disable"]
["unsigned char",null,null,"WifiDhcpClient",{"$nulls":5},"0: enable, 1: disable"]
["unsigned char",null,null,"WifiMacAddress[18]",{"$nulls":5},"default: Null"]
["unsigned char",null,null,"WifiIpAddress[16]",{"$nulls":5},"default:192.168.2.10"]
["unsigned char",null,null,"WifiSubmaskAddress[16]",{"$nulls":5},"default:255.255.255.0"]
["unsigned char",null,null,"WifiGatewayAddress[16]",{"$nulls":5},"default:192.168.2.254"]
["unsigned char",null,null,"WifiNetworkConn",{"$nulls":5},"0: disconnected, 1: connected"]

{"sheet":"TeleConfigData","index":3,"n_rows":13,"n_cols":10,"rows_kept":13,"cut":false,"hidden":false,"merged":[[0,0,0,2],[0,3,0,8],[0,9,0,20],[1,0,1,2],[1,3,1,8],[1,9,1,20],[2,0,2,2],[2,3,2,8],[2,9,2,20],[3,0,3,2],[3,3,3,8],[3,9,3,20],[4,0,4,2],[4,3,4,8],[4,9,4,20],[5,0,5,2],[5,3,5,8],[5,9,5,20],[6,0,6,2],[6,3,6,8],[6,9,6,20],[7,0,7,2],[7,3,7,8],[7,9,7,20],[8,0,8,2],[8,3,8,8],[8,9,8,20],[9,0,9,2],[9,3,9,8],[9,9,9,20],[10,0,10,2],[10,3,10,8],[10,9,10,20],[11,0,11,2],[11,3,11,8],[11,9,11,20],[12,0,12,2],[12,3,12,8],[12,9,12,20],[13,0,13,2],[13,3,13,8],[13,9,13,20],[14,0,14,2],[14,3,14,8],[14,9,14,20],[15,0,15,2],[15,3,15,8],[15,9,15,20]]}
["Data type",null,null,"Define",{"$nulls":5},"Comment"]
["unsigned char",null,null,"TelcomModelName[64]",{"$nulls":5},"default: Null"]
["unsigned char",null,null,"TelcomSoftwareVer[64]",{"$nulls":5},"default: Null"]
["unsigned char",null,null,"TelcomApn[256]",{"$nulls":5},"default: Null"]
["int",null,null,"TelcomRssi",{"$nulls":5},"dbm"]
["unsigned char",null,null,"TelcomChapPapId[256]",{"$nulls":5},"default: Null"]
["unsigned char",null,null,"TelcomChapPapPwd[256]",{"$nulls":5},"default: Null"]
["unsigned char",null,null,"TelcomModemImei[16]",{"$nulls":5},"default: Null"]
["unsigned char",null,null,"TelcomSimImsi[16]",{"$nulls":5},"default: Null"]
["unsigned char",null,null,"TelcomSimStatus",{"$nulls":5},"0: no SIM card is found, 1: valid SIM card, 2: invalid SIM card"]
["unsigned char",null,null,"TelcomModemMode",{"$nulls":5},"0: No services, 1: CDMA, 2: GSM/GPRS, 3: WCDMA, 4: GSM/WCDMA, 5: TD_SCDMA mode, 6: Unknow"]
["unsigned char",null,null,"TelcomIpAddress[16]",{"$nulls":5},"default: Null"]
["unsigned char",null,null,"TelcomNetworkConn",{"$nulls":5},"0: disconnected, 1: connected"]

{"sheet":"SysConfigData","index":4,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":false,"merged":[[2,0,2,2],[2,3,2,8],[2,9,2,20],[3,0,3,2],[3,3,3,8],[3,9,3,20],[0,0,0,2],[0,3,0,8],[0,9,0,20],[1,0,1,2],[1,3,1,8],[1,9,1,20],[6,0,6,2],[6,3,6,8],[6,9,6,20],[7,0,7,2],[7,3,7,8],[7,9,7,20],[4,0,4,2],[4,3,4,8],[4,9,4,20],[5,0,5,2],[5,3,5,8],[5,9,5,20],[10,0,10,2],[10,3,10,8],[10,9,10,20],[11,0,11,2],[11,3,11,8],[11,9,11,20],[8,0,8,2],[8,3,8,8],[8,9,8,20],[9,0,9,2],[9,3,9,8],[9,9,9,20],[14,0,14,2],[14,3,14,8],[14,9,14,20],[15,0,15,2],[15,3,15,8],[15,9,15,20],[12,0,12,2],[12,3,12,8],[12,9,12,20],[13,0,13,2],[13,3,13,8],[13,9,13,20],[22,0,22,2],[23,0,23,2],[24,0,24,2],[25,0,25,2],[26,0,26,2],[27,0,27,2],[16,0,16,2],[17,0,17,2],[18,0,18,2],[19,0,19,2],[20,0,20,2],[21,0,21,2],[22,3,22,8],[23,3,23,8],[24,3,24,8],[25,3,25,8],[26,3,26,8],[27,3,27,8],[16,3,16,8],[17,3,17,8],[18,3,18,8],[19,3,19,8],[20,3,20,8],[21,3,21,8],[22,9,22,20],[23,9,23,20],[24,9,24,20],[25,9,25,20],[26,9,26,20],[27,9,27,20],[16,9,16,20],[17,9,17,20],[18,9,18,20],[19,9,19,20],[20,9,20,20],[21,9,21,20],[35,9,35,20],[28,9,28,20],[29,9,29,20],[30,9,30,20],[31,9,31,20],[32,9,32,20],[33,9,33,20],[34,9,34,20],[34,0,34,2],[35,0,35,2],[28,3,28,8],[29,3,29,8],[30,3,30,8],[31,3,31,8],[32,3,32,8],[33,3,33,8],[34,3,34,8],[35,3,35,8],[28,0,28,2],[29,0,29,2],[30,0,30,2],[31,0,31,2],[32,0,32,2],[33,0,33,2]]}
["Data type",null,null,"Define",{"$nulls":5},"Comment"]
["unsigned char",null,null,"ModelName[64]",{"$nulls":5},"charger model name"]
["unsigned char",null,null,"SerialNumber[64]",{"$nulls":5},"charger system serial number"]
["unsigned char",null,null,"SystemId[128]",{"$nulls":5},"charger system ID"]
["unsigned char",null,null,"SystemDateTime[32]",{"$nulls":5},"charger system date and time"]
["unsigned char",null,null,"AuthorisationMode",{"$nulls":5},"0: Phihong RFID tag,  1: OCPP backend,  2: Phihong backend,  3: free mode"]
["unsigned char",null,null,"DefaultLanguage"]
["unsigned char",null,null,"RfidCardNumEndian",{"$nulls":5},"0: little endian,  1: big endian"]
["unsigned short",null,null,"AcPlugInTimes",{"$nulls":5},"0~65535"]
["unsigned short",null,null,"GbPlugInTimes",{"$nulls":5},"0~65535"]
["unsigned short",null,null,"Ccs1PlugInTime",{"$nulls":5},"0~65535"]
["unsigned short",null,null,"Ccs2PlugInTimes",{"$nulls":5},"0~65535"]
["unsigned short",null,null,"ChademoPlugInTimes",{"$nulls":5},"0~65535"]
[]
["unsigned short",null,null,"MaxChargingEnergy",{"$nulls":5},"0: no limit,\t1 ~ 65535\tkWh"]
["unsigned short",null,null,"MaxChargingPower",{"$nulls":5},"0: rating value, 1 ~ RATING_POWER (kW)\""]
["unsigned short",null,null,"MaxChargingCurrent",{"$nulls":5},"0: rating value, 1 ~ RATING_CURRENT (amp)\""]
["unsigned short",null,null,"MaxChargingDuration",{"$nulls":5},"0: no limit,\t1 ~ 65535\tminutes"]
["unsigned char",null,null,"PhaseLossPolicy",{"$nulls":5},"0: charging,  1: stop charging"]
["unsigned char",null,null,"LocalWhiteCard[10][32]",{"$nulls":5},"Max. card quantity is 10"]
["unsigned char",null,null,"UserId[32]",{"$nulls":5},"the user use this ID to trigger charging event, it can be RFID card number, OCPP IdTag, etc."]
[]
["unsigned char",null,null,"FtpServer[32]",{"$nulls":5},"the ftp server for Phihong server to do data transimission"]
["struct EthConfigData",null,null,"Eth0Interface"]
["struct EthConfigData",null,null,"Eth1Interface"]
["struct WifiConfigData",null,null,"AthInterface"]
["struct TeleConfigData",null,null,"TelecomInterface"]
[]
["unsigned int",null,null,"BackendConnTimeout",{"$nulls":5},"default : 300s"]
["unsigned char",null,null,"OfflinePolicy",{"$nulls":5},"0: local list, 1: Phihong RFID tag, 2: free charging, 3: no charging"]
["unsigned short",null,null,"OfflineMaxChargeEnergy",{"$nulls":5},"0: same as MaxChargingEnergy, 1 ~ 65535 kWh"]
["unsigned short",null,null,"OfflineMaxChargeDuration",{"$nulls":5},"0: same as MaxChargeDuration, 1 ~ 65535 minutes"]
["unsigned char",null,null,"OcppServerURL[512]",{"$nulls":5},"http: non-secure OCPP 1.5-S, https: secure OCPP 1.5-S, ws: non-secure OCPP 1.6-J, wss: secure OCPP 1.6-J\""]
["unsigned char",null,null,"ChargeBoxId[128]"]
["unsigned int",null,null,"Checksum",{"$nulls":5},"4 bytes checksum"]

{"sheet":"SysInfoData","index":5,"n_rows":56,"n_cols":10,"rows_kept":56,"cut":false,"hidden":false,"merged":[[3,0,3,2],[3,3,3,8],[3,9,3,20],[0,0,0,2],[0,3,0,8],[0,9,0,20],[1,0,1,2],[1,3,1,8],[1,9,1,20],[5,3,5,8],[5,9,5,20],[10,0,10,2],[10,3,10,8],[10,9,10,20],[6,0,6,2],[6,3,6,8],[6,9,6,20],[7,0,7,2],[7,3,7,8],[7,9,7,20],[4,0,4,2],[4,3,4,8],[4,9,4,20],[5,0,5,2],[2,0,2,2],[2,3,2,8],[2,9,2,20],[11,0,11,2],[11,3,11,8],[11,9,11,20],[8,0,8,2],[8,3,8,8],[8,9,8,20],[9,0,9,2],[9,3,9,8],[9,9,9,20],[14,0,14,2],[14,3,14,8],[14,9,14,20],[15,0,15,2],[15,3,15,8],[15,9,15,20],[12,0,12,2],[12,3,12,8],[12,9,12,20],[13,0,13,2],[13,3,13,8],[13,9,13,20],[34,0,34,2],[22,0,22,2],[23,0,23,2],[24,0,24,2],[25,0,25,2],[26,0,26,2],[27,0,27,2],[16,0,16,2],[17,0,17,2],[18,0,18,2],[19,0,19,2],[20,0,20,2],[21,0,21,2],[16,9,16,20],[17,9,17,20],[18,9,18,20],[19,9,19,20],[20,9,20,20],[21,9,21,20],[30,3,30,8],[31,3,31,8],[32,3,32,8],[16,3,16,8],[17,3,17,8],[18,3,18,8],[19,3,19,8],[20,3,20,8],[21,3,21,8],[22,3,22,8],[23,3,23,8],[28,9,28,20],[29,9,29,20],[30,9,30,20],[31,9,31,20],[32,9,32,20],[24,3,24,8],[25,3,25,8],[34,9,34,20],[22,9,22,20],[23,9,23,20],[24,9,24,20],[25,9,25,20],[26,9,26,20],[27,9,27,20],[41,9,41,20],[33,0,33,2],[33,3,33,8],[33,9,33,20],[34,3,34,8],[36,3,36,8],[26,3,26,8],[27,3,27,8],[28,3,28,8],[29,3,29,8],[35,0,35,2],[36,0,36,2],[28,0,28,2],[29,0,29,2],[30,0,30,2],[31,0,31,2],[32,0,32,2],[35,9,35,20],[36,9,36,20],[37,0,37,2],[38,0,38,2],[39,0,39,2],[40,0,40,2],[37,9,37,20],[38,9,38,20],[39,9,39,20],[40,9,40,20],[35,3,35,8],[42,3,42,8],[43,3,43,8],[44,3,44,8],[42,9,42,20],[43,9,43,20],[42,0,42,2],[43,0,43,2],[41,0,41,2],[37,3,37,8],[38,3,38,8],[39,3,39,8],[40,3,40,8],[41,3,41,8],[55,0,55,2],[55,3,55,8],[55,9,55,20],[54,0,54,2],[54,3,54,8],[54,9,54,20],[53,9,53,20],[44,9,51,20],[52,0,52,2],[52,3,52,8],[52,9,52,20],[44,0,44,2],[53,0,53,2],[53,3,53,8]]}
["Data type",null,null,"Define",{"$nulls":5},"Comment"]
["unsigned char",null,null,"BootingStatus",{"$nulls":5},"0 : booting, 1 : Initializing Complete."]
["unsigned char",null,null,"FactoryConfiguration",{"$nulls":5},"0: normal, 1: trigger, charger will return the configuration to factory default if trigger"]
["float",null,null,"InputVoltageR",{"$nulls":5},"0~655.35 volt"]
["float",null,null,"InputVoltageS",{"$nulls":5},"0~655.35 volt"]
["float",null,null,"InputVoltageT",{"$nulls":5},"0~655.35 volt"]
["unsigned int",null,null,"SystemFanRotaSpeed",{"$nulls":5},"0 ~ 65535 RPM"]
["unsigned int",null,null,"PsuFanRotaSpeed",{"$nulls":5},"0 ~ 65535 RPM"]
["unsigned char",null,null,"AuxPower5V",{"$nulls":5},"0 ~ 255 volt"]
["unsigned char",null,null,"AuxPower12V",{"$nulls":5},"0 ~ 255 volt"]
["unsigned char",null,null,"AuxPower24V",{"$nulls":5},"0 ~ 255 volt"]
["unsigned char",null,null,"AuxPower48V",{"$nulls":5},"0 ~ 255 volt"]
["unsigned char",null,null,"CsuHwRev[32]",{"$nulls":5},"CSU board hardware version"]
["unsigned char",null,null,"CsuBootLoadFwRev[32]",{"$nulls":5},"CSU board bootloader firmware version"]
["unsigned char",null,null,"CsuKernelFwRev[32]",{"$nulls":5},"CSU board OS kernel firmware version"]
["unsigned char",null,null,"CsuRootFsFwRev[32]",{"$nulls":5},"CSU board root file system firmware version"]
["unsigned char",null,null,"CsuPrimFwRev[32]",{"$nulls":5},"CSU board root file system firmware version"]
["unsigned char",null,null,"LcmHwRev[32]",{"$nulls":5},"LCM module hardware version"]
["unsigned char",null,null,"LcmFwRev[32]",{"$nulls":5},"LCM module firmware version"]
["unsigned char",null,null,"PsuHwRev[32]",{"$nulls":5},"PSU hardware version"]
["unsigned char",null,null,"PsuPrimFwRev[32]",{"$nulls":5},"PSU primary firmware version"]
["unsigned char",null,null,"PsuSecFwRev[32]",{"$nulls":5},"PSU secondary firmware version"]
["unsigned char",null,null,"AuxPwrHwRev[32]",{"$nulls":5},"Aux. power module hardware version"]
["unsigned char",null,null,"AuxPwrFwRev[32]",{"$nulls":5},"Aux. power module firmware version"]
["unsigned char",null,null,"FanModuleHwRev[32]",{"$nulls":5},"Fan  module hardware version"]
["unsigned char",null,null,"FanModuleFwRev[32]",{"$nulls":5},"Fan  module firmware version"]
["unsigned char",null,null,"RelayModuleHwRev[32]",{"$nulls":5},"Relay control  module hardware version"]
["unsigned char",null,null,"RelayModuleFwRev[32]",{"$nulls":5},"Relay control  module firmware version"]
["unsigned char",null,null,"TelcomModemFwRev[32]",{"$nulls":5},"the 3G/4G modem firmware version"]
["int",null,null,"SystemAmbientTemp",{"$nulls":5},"-40 ~ 215 degree C"]
["int",null,null,"SystemCriticalTemp",{"$nulls":5},"-40 ~ 216 degree C"]
["int",null,null,"CcsConnectorTemp",{"$nulls":5},"-40 ~ 217 degree C"]
["int",null,null,"PsuAmbientTemp",{"$nulls":5},"-40 ~ 218 degree C"]
[]
["struct ChargingInfoData",null,null,"ChademoChargingData[CHAdeMO_QUANTITY]"]
["struct ChargingInfoData",null,null,"CcsChargingData[CCS_QUANTITY]"]
["struct ChargingInfoData",null,null,"GbChargingData[GB_QUANTITY]"]
["unsigned char",null,null,"CurGunSelected"]
[]
["unsigned char",null,null,"InternetConn",{"$nulls":5},"0: disconnected, 1: connected"]
[]
["unsigned char",null,null,"OcppConnStatus",{"$nulls":5},"0: disconnected, 1: connected"]
[]
["unsigned char",null,null,"WaitForPlugit",{"$nulls":5},"0: none scan, 1: scanning"]
["unsigned char",null,null,"PageIndex",{"$nulls":5},"0 : Initialize\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t1 : idle\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t4 : Authorizing\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t5 : Authorizing complete\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t6 : Authorizing fail\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t7 : Wait for Plug\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t8 : Pre-charge\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t9 : Charging"]
{"$rows_empty":7}
["unsigned char",null,null,"AcContactorStatus",{"$nulls":5},"0 : disconnected, 1 : connected"]
["unsigned char",null,null,"SelfTestSeq"]
["unsigned char",null,null,"ReAssignedFlag",{"$nulls":5},"0 : none, other : gun number"]
["unsigned char",null,null,"FirmwareUpdate",{"$nulls":5},"0 : none, 1 : update"]

{"sheet":"ChargingInfoData","index":6,"n_rows":31,"n_cols":10,"rows_kept":31,"cut":false,"hidden":false,"merged":[[2,0,2,2],[2,3,2,8],[2,9,2,20],[3,0,3,2],[3,3,3,8],[3,9,3,20],[0,0,0,2],[0,3,0,8],[0,9,0,20],[1,0,1,2],[1,3,1,8],[1,9,1,20],[7,0,7,2],[7,3,7,8],[7,9,7,20],[8,0,8,2],[8,3,8,8],[8,9,8,20],[4,0,4,2],[4,3,4,8],[4,9,4,20],[5,0,5,2],[5,3,5,8],[5,9,5,20],[6,0,6,2],[6,3,6,8],[6,9,6,20],[11,0,11,2],[11,3,11,8],[11,9,11,20],[12,0,12,2],[12,3,12,8],[12,9,12,20],[9,0,9,2],[9,3,9,8],[9,9,9,20],[10,0,10,2],[10,3,10,8],[10,9,10,20],[15,0,15,2],[15,3,15,8],[15,9,15,20],[16,0,16,2],[16,3,16,8],[16,9,16,20],[13,0,13,2],[13,3,13,8],[13,9,13,20],[14,0,14,2],[14,3,14,8],[14,9,14,20],[19,0,19,2],[19,3,19,8],[19,9,19,20],[20,0,20,2],[20,3,20,8],[20,9,20,20],[17,0,17,2],[17,3,17,8],[17,9,17,20],[18,0,18,2],[18,3,18,8],[18,9,18,20],[23,0,23,2],[23,3,23,8],[23,9,23,20],[24,0,24,2],[24,3,24,8],[24,9,24,20],[21,0,21,2],[21,3,21,8],[21,9,21,20],[22,0,22,2],[22,3,22,8],[22,9,22,20],[29,3,29,8],[28,9,28,20],[25,0,25,2],[25,3,25,8],[25,9,25,20],[26,0,26,2],[26,3,26,8],[26,9,26,20],[29,9,29,20],[35,0,35,2],[35,3,35,8],[35,9,35,20],[27,0,27,2],[27,3,27,8],[33,0,33,2],[33,3,33,8],[33,9,33,20],[34,0,34,2],[34,3,34,8],[34,9,34,20],[31,0,31,2],[31,3,31,8],[31,9,31,20],[32,0,32,2],[32,3,32,8],[32,9,32,20],[30,0,30,2],[30,3,30,8],[30,9,30,20],[28,0,28,2],[28,3,28,8],[27,9,27,20],[29,0,29,2]]}
["Data type",null,null,"Define",{"$nulls":5},"Comment"]
["unsigned char",null,null,"Index"]
["unsigned char",null,null,"Type",{"$nulls":5},"0 : Chademo, 1 : CCS, 2: GB"]
["unsigned char",null,null,"type_index"]
["unsigned char",null,null,"SystemStatus",{"$nulls":5},"0: Booting, 1: idle, 2: authorizing, 3: preparing, 4: charging, 5: terminating, 6: alarm, 7: fault"]
["unsigned char",null,null,"PreSystemStatus"]
["unsigned char",null,null,"CardNumber[32]"]
["float",null,null,"MaximumChargingVoltage",{"$nulls":5},"0~6553.5 volt"]
["float",null,null,"AvailableChargingCurrent",{"$nulls":5},"0~6553.5 amp"]
["float",null,null,"AvailableChargingPower",{"$nulls":5},"0~6553.5 kW"]
["float",null,null,"PresentChargingVoltage",{"$nulls":5},"0~6553.5 volt"]
["float",null,null,"PresentChargingCurrent",{"$nulls":5},"0~6553.5 amp"]
["float",null,null,"PresentChargingPower",{"$nulls":5},"0~6553.5 kW"]
["float",null,null,"PresentChargedEnergy",{"$nulls":5},"0~6553.5 kWh"]
["int",null,null,"PresentChargedDuration",{"$nulls":5},"second"]
["int",null,null,"RemainChargingDuration",{"$nulls":5},"second"]
["float",null,null,"EvBatteryMaxVoltage",{"$nulls":5},"0~6553.5 volt"]
["float",null,null,"EvBatterytargetVoltage",{"$nulls":5},"0~6553.5 volt"]
["float",null,null,"EvBatterytargetCurrent",{"$nulls":5},"0~200(A) (unit:1A)"]
["int",null,null,"EvBatterySoc",{"$nulls":5},"0~100%"]
["unsigned char",null,null,"ConnectorPlugIn",{"$nulls":5},"0: unplug, 1: Plug-in"]
["unsigned char",null,null,"GunLocked",{"$nulls":5},"0: unlocked 1: locked"]
["float",null,null,"PilotVoltage"]
["unsigned char",null,null,"PilotState",{"$nulls":5},"1:state A, 2:State B1, 3:State B2, 4:State C, 5:State D, 6:State E, 7:State F, 8: Pilot error"]
["unsigned char",null,null,"PilotDuty",{"$nulls":5},"0~100%"]
["unsigned char",null,null,"ConnectorTemp",{"$nulls":5},"0x00: -60¢XC  ~  0xFE: 194"]
["unsigned char",null,null,"ChargingStatus",{"$nulls":5},"0x00 : None, 0x01 : Can Start Charging, 0x02 : Stop Charging"]
["float",null,null,"OutputEnergy",{"$nulls":5},"output energy by per charging"]
["unsigned char",null,null,"RelayK1K2Status",{"$nulls":5},"0x00 : open, 0x01 : close"]
["int",null,null,"TimeoutPid"]
["unsigned char ",null,null,"SmartChargeEnable"]

{"sheet":"PSU","index":7,"n_rows":55,"n_cols":10,"rows_kept":55,"cut":false,"hidden":false,"merged":[[1,0,1,2],[1,3,1,8],[1,9,1,20],[2,0,2,2],[2,3,2,8],[2,9,2,20],[5,0,5,2],[5,3,5,8],[5,9,5,20],[6,0,6,2],[6,3,6,8],[6,9,6,20],[3,0,3,2],[3,3,3,8],[3,9,3,20],[4,0,4,2],[4,3,4,8],[4,9,4,20],[9,0,9,2],[9,3,9,8],[9,9,9,20],[10,0,10,2],[10,3,10,8],[10,9,10,20],[7,0,7,2],[7,3,7,8],[7,9,7,20],[8,0,8,2],[8,3,8,8],[8,9,8,20],[0,0,0,20],[17,0,17,2],[18,0,18,2],[19,0,19,2],[20,0,20,2],[21,0,21,2],[15,0,15,2],[15,3,15,8],[15,9,15,20],[16,0,16,2],[16,3,16,8],[16,9,16,20],[13,0,13,2],[13,3,13,8],[13,9,13,20],[14,0,14,2],[14,3,14,8],[14,9,14,20],[11,0,11,2],[11,3,11,8],[11,9,11,20],[12,0,12,2],[12,3,12,8],[12,9,12,20],[28,0,28,2],[29,0,29,2],[30,0,30,2],[31,0,31,2],[32,0,32,2],[33,0,33,2],[22,0,22,2],[23,0,23,2],[24,0,24,2],[25,0,25,2],[26,0,26,2],[27,0,27,2],[17,9,17,20],[18,9,18,20],[19,9,19,20],[20,9,20,20],[21,9,21,20],[22,9,22,20],[23,9,23,20],[26,3,26,8],[27,3,27,8],[17,3,17,8],[18,3,18,8],[19,3,19,8],[20,3,20,8],[21,3,21,8],[22,3,22,8],[23,3,23,8],[24,3,24,8],[25,3,25,8],[24,9,24,20],[25,9,25,20],[26,9,26,20],[27,9,27,20],[28,9,28,20],[29,9,29,20],[32,3,32,8],[33,3,33,8],[36,3,36,8],[28,3,28,8],[29,3,29,8],[30,3,30,8],[31,3,31,8],[35,3,35,8],[35,9,35,20],[38,0,38,2],[38,3,38,8],[38,9,38,20],[39,0,39,2],[39,3,39,8],[39,9,39,20],[30,9,30,20],[31,9,31,20],[32,9,32,20],[33,9,33,20],[36,9,36,20],[37,0,37,20],[36,0,36,2],[34,0,34,2],[34,3,34,8],[34,9,34,20],[35,0,35,2],[42,0,42,2],[42,3,42,8],[42,9,42,20],[43,0,43,2],[43,3,43,8],[43,9,43,20],[40,0,40,2],[40,3,40,8],[40,9,40,20],[41,0,41,2],[41,3,41,8],[41,9,41,20],[47,0,47,2],[47,3,47,8],[47,9,47,20],[48,3,48,8],[48,9,48,20],[48,0,48,2],[49,0,49,20],[50,0,50,2],[50,3,50,8],[46,0,46,2],[46,3,46,8],[46,9,46,20],[44,0,44,2],[44,3,44,8],[44,9,44,20],[45,0,45,2],[45,3,45,8],[45,9,45,20],[50,9,50,20],[51,0,51,2],[51,3,51,8],[51,9,51,20],[52,0,52,2],[52,3,52,8],[52,9,52,20],[54,0,54,2],[54,3,54,8],[54,9,54,20],[53,0,53,2],[53,3,53,8],[53,9,53,20]]}
["PsuModuleData"]
["Data type",null,null,"Define",{"$nulls":5},"Comment"]
["unsigned char",null,null,"AssignID"]
["unsigned char",null,null,"PhysicalID"]
["unsigned char",null,null,"GroupID"]
["unsigned char",null,null,"Address"]
["unsigned char",null,null,"FwVersion[12]"]
["unsigned char",null,null,"StateMachine",{"$nulls":5},"0: Identification,  1:Operation,  2: Alarm,  3: Failure,  s4:Upgrade"]
["unsigned char",null,null,"OutputPowerSwitch",{"$nulls":5},"0: D.D normal OFF,  1: D.D emergency OFF,  2: D.D ON"]
["unsigned short",null,null,"FanSpeed_1",{"$nulls":5},"RPM"]
["unsigned short",null,null,"FanSpeed_2",{"$nulls":5},"RPM"]
["unsigned short",null,null,"FanSpeed_3",{"$nulls":5},"RPM"]
["unsigned short",null,null,"FanSpeed_4",{"$nulls":5},"RPM"]
["unsigned short",null,null,"InputVoltage_Type",{"$nulls":5},"0x00 = Line to Line Vol, 0x01 = Line to Neutral Vol"]
["unsigned short",null,null,"InputVoltageL1",{"$nulls":5},"abcd=abc.d volt"]
["unsigned short",null,null,"InputVoltageL2",{"$nulls":5},"abcd=abc.d volt"]
["unsigned short",null,null,"InputVoltageL3",{"$nulls":5},"abcd=abc.d volt"]
["unsigned short",null,null,"InputCurrentL1",{"$nulls":5},"abcd=abc.d amp"]
["unsigned short",null,null,"InputCurrentL2",{"$nulls":5},"abcd=abc.d amp"]
["unsigned short",null,null,"InputCurrentL3",{"$nulls":5},"abcd=abc.d amp"]
["unsigned short",null,null,"PresentOutputVoltage",{"$nulls":5},"abcd=abc.d volt"]
["unsigned short",null,null,"PresentOutputCurrent",{"$nulls":5},"abcd=abc.d amps"]
["unsigned short",null,null,"AvailableCurrent",{"$nulls":5},"abcd=abc.d amps"]
["int",null,null,"AvailablePower",{"$nulls":5},"Watt"]
["unsigned char",null,null,"CriticalTemp1",{"$nulls":5},"0x00: -60¢XC  ~  0xFE: 194¢XC, resolution: 1¢XC, offset: -60¢XC, 0xFF: invalid"]
["unsigned char",null,null,"CriticalTemp2",{"$nulls":5},"0x00: -60¢XC  ~  0xFE: 194¢XC, resolution: 1¢XC, offset: -60¢XC, 0xFF: invalid"]
["unsigned char",null,null,"CriticalTemp3",{"$nulls":5},"0x00: -60¢XC  ~  0xFE: 194¢XC, resolution: 1¢XC, offset: -60¢XC, 0xFF: invalid"]
["unsigned char",null,null,"ExletTemp",{"$nulls":5},"0x00: -60¢XC  ~  0xFE: 194¢XC, resolution: 1¢XC, offset: -60¢XC, 0xFF: invalid"]
["unsigned char",null,null,"InletTemp_1",{"$nulls":5},"0x00: -60¢XC  ~  0xFE: 194¢XC, resolution: 1¢XC, offset: -60¢XC, 0xFF: invalid"]
["unsigned char",null,null,"InletTemp_2",{"$nulls":5},"0x00: -60¢XC  ~  0xFE: 194¢XC, resolution: 1¢XC, offset: -60¢XC, 0xFF: invalid"]
["unsigned char",null,null,"InletTemp",{"$nulls":5},"0x00: -60¢XC  ~  0xFE: 194¢XC, resolution: 1¢XC, offset: -60¢XC, 0xFF: invalid"]
["unsigned char",null,null,"OutletTemp",{"$nulls":5},"0x00: -60¢XC  ~  0xFE: 194¢XC, resolution: 1¢XC, offset: -60¢XC, 0xFF: invalid"]
["unsigned int",null,null,"AlarmCode"]
["unsigned int",null,null,"FaultCode"]
["unsigned char",null,null,"SerialNumber[32]"]
["unsigned char",null,null,"FireWireIndex"]
[]
["PsuGroupData"]
["Data type",null,null,"Define",{"$nulls":5},"Comment"]
["unsigned char",null,null,"GroupPresentPsuQuantity"]
["unsigned char",null,null,"GroupOutputPowerSwitch",{"$nulls":5},"0: D.D normal OFF,  1: D.D emergency OFF,  2: D.D ON"]
["unsigned short",null,null,"GroupTargetOutputVoltage",{"$nulls":5},"abcd=abc.d volt"]
["unsigned short",null,null,"GroupTargetOutputCurrent",{"$nulls":5},"abcd=abc.d amp"]
["unsigned short",null,null,"GroupAvailableCurrent",{"$nulls":5},"abcd=abc.d amp"]
["unsigned int",null,null,"GroupAvailablePower",{"$nulls":5},"Watt"]
["unsigned short",null,null,"GroupPresentOutputVoltage",{"$nulls":5},"abcd=abc.d volt"]
["unsigned short",null,null,"GroupPresentOutputCurrent",{"$nulls":5},"abcd=abc.d amp"]
["struct PsuModuleData",null,null,"PsuModule[MAX_PSU_QUANTITY]"]
[]
["PsuData"]
["Data type",null,null,"Define",{"$nulls":5},"Comment"]
["unsigned char",null,null,"SystemPresentPsuQuantity"]
["struct PsuGroupData",null,null,"PsuGroup[4]"]
["unsigned char",null,null,"GroupCount"]
["unsigned char",null,null,"SelfTest_Comp",{"$nulls":5},"0 : none, other : complete"]

{"sheet":"Chademo","index":8,"n_rows":84,"n_cols":10,"rows_kept":84,"cut":false,"hidden":false,"merged":[[43,0,43,2],[43,3,43,8],[43,9,43,20],[1,0,1,2],[1,3,1,8],[1,9,1,20],[0,0,0,20],[12,0,12,2],[13,0,13,2],[4,0,4,2],[4,3,4,8],[4,9,4,20],[5,0,5,2],[5,3,5,8],[5,9,5,20],[2,0,2,2],[2,3,2,8],[2,9,2,20],[3,0,3,2],[3,3,3,8],[3,9,3,20],[8,0,8,2],[8,3,8,8],[8,9,8,20],[9,0,9,2],[9,3,9,8],[9,9,9,20],[6,0,6,2],[6,3,6,8],[6,9,6,20],[7,0,7,2],[7,3,7,8],[7,9,7,20],[15,0,15,2],[15,3,15,8],[15,9,15,20],[16,0,16,2],[16,3,16,8],[16,9,16,20],[10,0,10,2],[10,3,10,8],[10,9,10,20],[11,0,11,2],[11,3,11,8],[30,0,30,2],[30,3,30,8],[14,0,14,2],[12,3,12,8],[13,3,13,8],[14,3,14,8],[11,9,14,20],[22,0,22,2],[23,0,23,2],[24,0,24,2],[25,0,25,2],[26,0,26,2],[27,0,27,2],[19,3,19,8],[31,3,31,8],[17,0,17,2],[17,3,17,8],[29,0,29,2],[29,3,29,8],[29,9,29,20],[32,3,32,8],[20,3,20,8],[21,3,21,8],[22,3,22,8],[23,3,23,8],[24,3,24,8],[25,3,25,8],[26,3,26,8],[27,3,27,8],[18,0,18,2],[18,3,18,8],[17,9,28,20],[19,0,19,2],[20,0,20,2],[21,0,21,2],[44,9,44,20],[34,0,34,2],[35,0,35,2],[36,0,36,2],[37,0,37,2],[41,0,41,2],[41,3,41,8],[41,9,41,20],[42,0,42,2],[42,3,42,8],[42,9,42,20],[39,0,39,2],[39,3,39,8],[39,9,39,20],[40,0,40,2],[40,3,40,8],[40,9,40,20],[35,3,35,8],[36,3,36,8],[37,3,37,8],[30,9,37,20],[38,0,38,2],[38,3,38,8],[38,9,38,20],[61,3,61,8],[67,3,67,8],[77,3,77,8],[78,3,78,8],[51,3,51,8],[52,3,52,8],[28,3,28,8],[28,0,28,2],[58,0,58,2],[58,3,58,8],[31,0,31,2],[32,0,32,2],[33,0,33,2],[68,0,68,2],[47,0,47,2],[47,3,47,8],[53,0,53,2],[53,3,53,8],[57,0,57,2],[57,3,57,8],[33,3,33,8],[34,3,34,8],[44,0,44,2],[44,3,44,8],[47,9,47,20],[48,0,48,2],[48,3,48,8],[48,9,48,20],[45,0,45,20],[46,0,46,2],[46,3,46,8],[46,9,46,20],[49,0,49,2],[49,3,49,8],[53,9,53,20],[50,0,50,2],[51,0,51,2],[52,0,52,2],[50,3,50,8],[49,9,52,20],[56,0,56,2],[56,3,56,8],[56,9,56,20],[57,9,58,20],[54,0,54,2],[54,3,54,8],[54,9,54,20],[55,0,55,2],[55,3,55,8],[55,9,55,20],[80,0,80,20],[81,0,81,2],[81,3,81,8],[81,9,81,20],[63,3,63,8],[64,3,64,8],[65,3,65,8],[67,9,76,20],[74,3,74,8],[75,3,75,8],[76,3,76,8],[76,0,76,2],[68,3,68,8],[69,3,69,8],[70,3,70,8],[71,3,71,8],[72,3,72,8],[82,9,82,20],[59,0,59,2],[59,3,59,8],[59,9,59,20],[79,0,79,2],[79,3,79,8],[79,9,79,20],[60,0,60,2],[61,0,61,2],[67,0,67,2],[77,0,77,2],[60,9,60,20],[77,9,77,20],[78,9,78,20],[69,0,69,2],[62,0,62,2],[63,0,63,2],[64,0,64,2],[66,3,66,8],[61,9,66,20],[65,0,65,2],[62,3,62,8],[78,0,78,2],[60,3,60,8],[85,9,85,20],[86,0,86,2],[86,3,86,8],[86,9,86,20],[83,0,83,2],[83,3,83,8],[83,9,83,20],[84,0,84,2],[84,3,84,8],[84,9,84,20],[73,3,73,8],[70,0,70,2],[71,0,71,2],[72,0,72,2],[73,0,73,2],[74,0,74,2],[75,0,75,2],[85,0,85,2],[85,3,85,8],[82,0,82,2],[82,3,82,8]]}
["CHAdeMOEvseData (樁端)"]
["Data type",null,null,"Define",{"$nulls":5},"Comment"]
["unsigned char",null,null,"SelfTest_Comp"]
["unsigned char",null,null,"version[16]",{"$nulls":5},"Chademo firmware version"]
["unsigned char",null,null,"SupportDynamicControl",{"$nulls":5},"bit0=1:supported"]
["unsigned char",null,null,"SupportHighCurrent",{"$nulls":5},"bit1=1:supported"]
["unsigned short",null,null,"AvailableOutputVoltage",{"$nulls":5},"0~600(V) (unit:1V)"]
["unsigned short",null,null,"AvailableOutputCurrent"]
["unsigned short",null,null,"ThresholdVoltage",{"$nulls":5},"0~600(V) (unit:1V)"]
["unsigned char",null,null,"ConnectorTemperatureP",{"$nulls":5},"-40~215(degC) (unit:degC) //value 0=-40\t[NISSAN customized]"]
["unsigned char",null,null,"ConnectorTemperatureN",{"$nulls":5},"-40~215(degC) (unit:degC) //value 0=-41\t[NISSAN customized]"]
["unsigned char",null,null,"ProtocolVersion",{"$nulls":5},"0~255\n0x00: CHAdeMO specification 0.9 and earlier\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t0x01: CHAdeMO specification 0.9 and 0.9.1\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t0x02: CHAdeMO specification 1.0.0, 1.0.1, 1.1 and 1.2"]
[]
[]
[]
["unsigned short",null,null,"PresentOutputVoltage",{"$nulls":5},"0~600(V) (unit:1V)"]
["unsigned short",null,null,"PresentOutputCurrent"]
["unsigned char",null,null,"EvseDetection",{"$nulls":5},"bit0=0:not charging state now\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit0=1:charging state now\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit1=0:EVSE normal\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit1=1:EVSE error\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit2=0:Not Energizing state\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit2=1:Energizing state\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit3=0:No Battery incompatibility\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit3=1:Battery incompatibility\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit4=0:No Charging system error\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit4=1:Charging system error\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit5=0:No Charging stop control\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit5=1:Charging stop control"]
{"$rows_empty":11}
["unsigned short",null,null,"RemainChargingTime",{"$nulls":5},"10(sec.)~255(min.)\t(Unit:sec)"]
["unsigned char",null,null,"HighPowerCondition",{"$nulls":5},"bit0=0:Present charging current H¡¦118.3,H¡¦118.4¡¨ is less than or equal to rated current of a charging cable\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit0=1:Present charging current H¡¦118.3,H¡¦118.4¡¨ is exceeds to rated current of a charging cable\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit1=1:charging cable Cooling function Operating Installed\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit2=1:charging cable Current limiting function\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit3=1:charging connector Cooling function Operating\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit4=1:charging connector Current limiting function Installed\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit5=1:charging connector Over-temperature protection Installed\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit6=1:Functional safety Applied"]
{"$rows_empty":7}
["unsigned int",null,null,"MaxiGroupPower",{"$nulls":5},"XXXXXXXX (Unit:Watt)depend on which group to be used"]
["unsigned int",null,null,"MaxiGroupCurrent",{"$nulls":5},"XXXXXXXX (unit:1A)depend on which group to be used"]
["unsigned short",null,null,"ApplyOutputVoltage",{"$nulls":5},"0~600(V) (unit:1V)"]
["unsigned short",null,null,"ElapseChargingTime",{"$nulls":5},"(Unit:sec)"]
["unsigned short",null,null,"ElapseEnergy",{"$nulls":5},"(Unit:10xkWh)"]
["unsigned char",null,null,"EvboardStatus",{"$nulls":5},"0 : init"]
[]
["CHAdeMOEvData (車端)"]
["Data type",null,null,"Define",{"$nulls":5},"Comment"]
["unsigned char",null,null,"SupportDynamicControl",{"$nulls":5},"bit0=1:supported"]
["unsigned char",null,null,"SupportHighCurrent",{"$nulls":5},"bit0=1:supported"]
["unsigned char",null,null,"MiniChargeCurrent",{"$nulls":5},"0~200(A) (unit:1A)\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t0x00: request for current equivalent to 1.5kW\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t0x01: no request\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\t0x02: request of 1A and following are the same rule"]
[]
[]
[]
["unsigned short",null,null,"MaxiBatteryVoltage",{"$nulls":5},"0~600(V) (unit:1V)"]
["unsigned short",null,null,"MaxiChargingTime",{"$nulls":5},"10(sec.)~255(min.)\t(Unit:sec)"]
["unsigned char",null,null,"EstimatChargingTime",{"$nulls":5},"0~254(min.)\t(Unit:sec)"]
["unsigned short",null,null,"TotalBatteryCapacity",{"$nulls":5},"0.1~6553.5(kWh)\t(unit:0.1 kWh)"]
["unsigned char",null,null,"ProtocolVersion",{"$nulls":5},"0~255\n0x02: CHAdeMO specification ver.1.2"]
[]
["unsigned short",null,null,"TargetBatteryVoltage",{"$nulls":5},"0~600(V) (unit:1V)"]
["unsigned short",null,null,"ChargingCurrentRequest",{"$nulls":5},"0~200(A) (unit:1A)"]
["unsigned char",null,null,"BatteryAlarm",{"$nulls":5},">0:alarm\nbit0=1:Battery overvoltage\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit1=1:Battery undervoltage\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit2=1:Battery current deviation error\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit3=1:High battery temperature\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit4=1:Battery voltage deviation error"]
[]
[]
[]
[]
[]
["unsigned char",null,null,"EvDetection",{"$nulls":5},"bit0=0:Vehicle charging disabled,\t(stop charging)\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit0=1:Vehicle charging enabled,\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit1=0:¡§Parking¡¨ position\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit1=1:other position\t\t\t\t(stop charging)\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit2=0:Charging system normal\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit2=1:Charging system error\t\t(stop charging)\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit3=0:EV contactor close or during welding detection\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit3=1:EV contactor open or termination of welding detection (stop charging)\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit4=0:No stop request before charging\n\t\t\t\t\t\t\t\t\t\t\t\t\t\t\tbit4=1:Normal stop request before charging\t(stop charging)"]
{"$rows_empty":9}
["unsigned char",null,null,"SOC",{"$nulls":5},"0~100(%) (unit:%)"]
["unsigned char",null,null,"Communicating",{"$nulls":5},"it is true if receive EV CAN message within every 1500ms"]
[]
["CHAdeMOData"]
["Data type",null,null,"Define",{"$nulls":5},"Comment"]
["struct CHAdeMOEvData",null,null,"ev[CHAdeMO_QUANTITY]"]
["struct CHAdeMOEvseData ",null,null,"evse[CHAdeMO_QUANTITY]"]

{"sheet":"OCPP","index":9,"n_rows":39,"n_cols":12,"rows_kept":39,"cut":false,"hidden":false,"merged":[[0,0,0,18],[1,11,1,18],[2,11,93,18],[16,9,16,10],[17,9,17,10],[18,9,18,10],[2,0,2,2],[2,3,2,8],[2,9,2,10],[3,0,3,2],[3,3,3,8],[3,9,3,10],[1,0,1,2],[1,3,1,8],[1,9,1,10],[6,0,6,2],[6,3,6,8],[6,9,6,10],[7,0,7,2],[7,3,7,8],[7,9,7,10],[4,0,4,2],[4,3,4,8],[4,9,4,10],[5,0,5,2],[5,3,5,8],[5,9,5,10],[10,0,10,2],[10,3,10,8],[10,9,10,10],[11,0,11,2],[11,3,11,8],[11,9,11,10],[8,0,8,2],[8,3,8,8],[8,9,8,10],[9,0,9,2],[9,3,9,8],[9,9,9,10],[14,0,14,2],[14,3,14,8],[14,9,14,10],[15,0,15,2],[15,3,15,8],[15,9,15,10],[12,0,12,2],[12,3,12,8],[12,9,12,10],[13,0,13,2],[13,3,13,8],[13,9,13,10],[25,9,25,10],[26,9,26,10],[27,9,27,10],[28,9,28,10],[29,9,29,10],[30,9,30,10],[19,9,19,10],[20,9,20,10],[21,9,21,10],[22,9,22,10],[23,9,23,10],[24,9,24,10],[39,9,39,10],[40,9,40,10],[41,9,41,10],[42,9,42,10],[43,9,43,10],[31,9,31,10],[32,9,32,10],[33,9,33,10],[34,9,34,10],[35,9,35,10],[36,9,36,10],[50,9,50,10],[51,9,51,10],[52,9,52,10],[53,9,53,10],[54,9,54,10],[55,9,55,10],[44,9,44,10],[45,9,45,10],[46,9,46,10],[47,9,47,10],[48,9,48,10],[49,9,49,10],[62,9,62,10],[63,9,63,10],[64,9,64,10],[65,9,65,10],[66,9,66,10],[67,9,67,10],[56,9,56,10],[57,9,57,10],[58,9,58,10],[59,9,59,10],[60,9,60,10],[61,9,61,10],[76,9,76,10],[77,9,77,10],[78,9,78,10],[79,9,79,10],[68,9,68,10],[69,9,69,10],[70,9,70,10],[71,9,71,10],[72,9,72,10],[73,9,73,10],[92,9,92,10],[93,9,93,10],[94,9,94,10],[16,0,16,2],[17,0,17,2],[18,0,18,2],[19,0,19,2],[20,0,20,2],[21,0,21,2],[22,0,22,2],[86,9,86,10],[87,9,87,10],[88,9,88,10],[89,9,89,10],[90,9,90,10],[91,9,91,10],[80,9,80,10],[81,9,81,10],[82,9,82,10],[83,9,83,10],[84,9,84,10],[85,9,85,10],[74,9,74,10],[75,9,75,10],[57,0,57,2],[58,0,58,2],[16,3,16,8],[17,3,17,8],[18,3,18,8],[19,3,19,8],[20,3,20,8],[48,0,48,2],[49,0,49,2],[50,0,50,2],[51,0,51,2],[52,0,52,2],[53,0,53,2],[42,0,42,2],[43,0,43,2],[44,0,44,2],[45,0,45,2],[46,0,46,2],[47,0,47,2],[35,0,35,2],[36,0,36,2],[38,0,38,2],[39,0,39,2],[40,0,40,2],[21,3,21,8],[22,3,22,8],[23,3,23,8],[24,3,24,8],[25,3,25,8],[26,3,26,8],[54,0,54,2],[55,0,55,2],[56,0,56,2],[41,0,41,2],[29,0,29,2],[30,0,30,2],[31,0,31,2],[32,0,32,2],[33,0,33,2],[34,0,34,2],[23,0,23,2],[24,0,24,2],[25,0,25,2],[26,0,26,2],[27,0,27,2],[28,0,28,2],[33,3,33,8],[34,3,34,8],[35,3,35,8],[38,3,38,8],[36,3,36,8],[37,0,37,10],[27,3,27,8],[28,3,28,8],[29,3,29,8],[30,3,30,8],[31,3,31,8],[32,3,32,8],[38,9,38,10]]}
["OCPP16Data"]
["Data type",null,null,"Define",{"$nulls":5},"Comment",null,"union"]
["unsigned char",null,null,"OcppServerURL[512]",{"$nulls":7},"union\n\t\t{\n\t\t\tunsigned char CpMsgValue[CHAdeMO_QUANTITY + CCS_QUANTITY + GB_QUANTITY];\n\t\t\tstruct\n\t\t\t{\n\t\t\t\t//CpMsgValue[0]\n\t\t\t\tunsigned char DataTransferReq:1;\t//bit 0,\n\t\t\t\tunsigned char DataTransferConf:1;\t//bit 1,\n\t\t\t\tunsigned char StartTransactionReq:1; //bit 2,\n\t\t\t\tunsigned char StartTransactionConf:1;\t//bit 3,\n\t\t\t\tunsigned char StopTransactionReq:1;\t//bit 4,\n\t\t\t\tunsigned char StopTransactionConf:1;\t//bit 5,\n\t\t\t\tunsigned char :2;\t//bit 6,7 , reserved\n\t\t\t} bits[CHAdeMO_QUANTITY + CCS_QUANTITY + GB_QUANTITY];\n\t\t}CpMsg;\nunion\n\t\t{\n\t\t\t//Operations Initiated by Sequence Point\n\t\t\tunsigned char SpMsgValue[1];\n\t\t\tstruct\n\t\t\t{\n\t\t\t\t//SpMsgValue[0]\n\t\t\t\tunsigned char BootNotificationReq :1;\t//bit 0,\n\t\t\t\tunsigned char BootNotificationConf :1;\t//bit 1,\n\t\t\t\tunsigned char AuthorizeReq :1; //bit 2,\n\t\t\t\tunsigned char AuthorizeConf :1;\t//bit 3,\n\t\t\t\tunsigned char DiagnosticsStatusNotificationReq :1;\t//bit 4,\n\t\t\t\tunsigned char DiagnosticsStatusNotificationConf :1;\t//bit 5,\n\t\t\t\tunsigned char FirmwareStatusNotificationReq :1; //bit 6,\n\t\t\t\tunsigned char FirmwareStatusNotificationConf :1; //bit 7,\n\t\t\t} bits;\n\t\t} SpMsg;\n\n\t\tunion\n\t\t{\n\t\t\t//Operations Initiated by Central System\n\t\t\tunsigned char CsMsgValue[3 * (CHAdeMO_QUANTITY + CCS_QUANTITY + GB_QUANTITY)];\n\t\t\tstruct\n\t\t\t{\n\t\t\t\t//CsMsgValue[0]\n\t\t\t\tunsigned char CancelReservationReq :1;\t//bit 0,\n\t\t\t\tunsigned char CancelReservationConf :1;\t//bit 1,\n\t\t\t\tunsigned char ChangeAvailabilityReq :1; //bit 2,\n\t\t\t\tunsigned char ChangeAvailabilityConf :1;\t//bit 3,\n\t\t\t\tunsigned char ReserveNowReq :1;\t//bit 4,\n\t\t\t\tunsigned char ReserveNowConf :1;\t//bit 5,\n\t\t\t\tunsigned char SetChargingProfileReq :1;\t//bit 6,\n\t\t\t\tunsigned char SetChargingProfileConf :1;\t//bit 7,\n\t\t\t\t//CsMsgValue[1]\n\t\t\t\tunsigned char TriggerMessageReq :1;\t//bit 0,\n\t\t\t\tunsigned char TriggerMessageConf :1;\t//bit 1,\n\t\t\t\tunsigned char UnlockConnectorReq :1; //bit 2,\n\t\t\t\tunsigned char UnlockConnectorConf :1;\t//bit 3,\n\t\t\t\tunsigned char RemoteStartTransactionReq :1;\t//bit 4,\n\t\t\t\tunsigned char RemoteStartTransactionConf :1; //bit 5,\n\t\t\t\tunsigned char RemoteStopTransactionReq :1;\t//bit 6,\n\t\t\t\tunsigned char RemoteStopTransactionConf :1;\t//bit 7,\n\t\t\t\t//CsMsgValue[2]\n\t\t\t\tunsigned char ClearChargingProfileReq :1;\t//bit 0,\n\t\t\t\tunsigned char ClearChargingProfileConf :1;\t//bit 1,\n\t\t\t\tunsigned char DataTransferReq :1; //bit 2,\n\t\t\t\tunsigned char DataTransferConf :1;\t//bit 3,\n\t\t\t\tunsigned char GetCompositeScheduleReq :1;\t//bit 4,\n\t\t\t\tunsigned char GetCompositeScheduleConf :1;\t//bit 5,\n\t\t\t\tunsigned char :2;\t//bit 6,7\n\t\t\t} bits[CHAdeMO_QUANTITY + CCS_QUANTITY + GB_QUANTITY];\n\t\t}CsMsg;\n\n\t\tunion\n\t\t{\n\t\t\t//Operations Initiated by Main System\n\t\t\tunsigned char MsMsgValue[2];\n\t\t\tstruct\n\t\t\t{\n\t\t\t\t//CsMsgValue[0]\n\t\t\t\tunsigned char ChangeConfigurationReq :1;\t//bit 0,\n\t\t\t\tunsigned char ChangeConfigurationConf :1;\t//bit 1,\n\t\t\t\tunsigned char ClearCacheReq :1;\t//bit 2,\n\t\t\t\tunsigned char ClearCacheConf :1;\t//bit 3,\n\t\t\t\tunsigned char GetConfigurationReq :1;\t//bit 4,\n\t\t\t\tunsigned char GetConfigurationConf :1;\t//bit 5,\n\t\t\t\tunsigned char UpdateFirmwareReq :1;\t//bit 6,\n\t\t\t\tunsigned char UpdateFirmwareConf :1;\t//bit 7,\n\t\t\t\t//CsMsgValue[1]\n\t\t\t\tunsigned char GetDiagnosticsReq :1;\t//bit 0,\n\t\t\t\tunsigned char GetDiagnosticsConf :1;\t//bit 1,\n\t\t\t\tunsigned char GetLocalListVersionReq :1; //bit 2,\n\t\t\t\tunsigned char GetLocalListVersionConf :1;\t//bit 3,\n\t\t\t\tunsigned char ResetReq :1; //bit 4,\n\t\t\t\tunsigned char ResetConf :1;\t//bit 5,\n\t\t\t\tunsigned char SendLocalListReq :1;\t//bit 6,\n\t\t\t\tunsigned char SendLocalListConf :1;\t//bit 7,\n\t\t\t} bits;\n\t\t} MsMsg;"]
["unsigned char",null,null,"ChargeBoxId[128]"]
["unsigned char",null,null,"OcppConnStatus"]
["struct StructBootNotification",null,null,"BootNotification"]
["struct StructHeartbeat",null,null,"Heartbeat"]
["struct StructAuthorize",null,null,"Authorize"]
["struct StructStartTransaction",null,null,"StartTransaction[CHAdeMO_QUANTITY+ CCS_QUANTITY + GB_QUANTITY]"]
["struct StructStopTransaction",null,null,"StopTransaction[CHAdeMO_QUANTITY+ CCS_QUANTITY + GB_QUANTITY]"]
["struct StructStatusNotification",null,null,"StatusNotification[CHAdeMO_QUANTITY+ CCS_QUANTITY + GB_QUANTITY]"]
["struct StructCancelReservation",null,null,"CancelReservation[CHAdeMO_QUANTITY+ CCS_QUANTITY + GB_QUANTITY]"]
["struct StructChangeAvailability",null,null,"ChangeAvailability[CHAdeMO_QUANTITY+ CCS_QUANTITY + GB_QUANTITY]"]
["struct StructChangeConfiguration",null,null,"ChangeConfiguration"]
["struct StructClearCache\t",null,null,"ClearCache"]
["struct StructClearChargingProfile",null,null,"ClearChargingProfile[CHAdeMO_QUANTITY+ CCS_QUANTITY + GB_QUANTITY]"]
["struct StructDataTransfer",null,null,"DataTransfer[CHAdeMO_QUANTITY+ CCS_QUANTITY + GB_QUANTITY]"]
["struct StructDiagnosticsStatusNotification",null,null,"DiagnosticsStatusNotification"]
["struct StructFirmwareStatusNotification\t",null,null,"FirmwareStatusNotification"]
["struct StructGetCompositeSchedule",null,null,"GetCompositeSchedule[CHAdeMO_QUANTITY+ CCS_QUANTITY + GB_QUANTITY]"]
["struct StructGetConfiguration",null,null,"GetConfiguration"]
["struct StructGetDiagnostics\t",null,null,"GetDiagnostics"]
["struct StructGetLocalListVersion",null,null,"GetLocalListVersion"]
["struct StructMeterValues",null,null,"MeterValues[CHAdeMO_QUANTITY+ CCS_QUANTITY + GB_QUANTITY]"]
["struct StructRemoteStartTransaction\t",null,null,"RemoteStartTransaction[CHAdeMO_QUANTITY+ CCS_QUANTITY + GB_QUANTITY]"]
["struct StructRemoteStopTransaction",null,null,"RemoteStopTransaction[CHAdeMO_QUANTITY+ CCS_QUANTITY + GB_QUANTITY]"]
["struct StructReserveNow",null,null,"ReserveNow[CHAdeMO_QUANTITY+ CCS_QUANTITY + GB_QUANTITY]"]
["struct StructReset",null,null,"Reset"]
["struct StructSendLocalList",null,null,"SendLocalList"]
["struct StructSetChargingProfile\t",null,null,"SetChargingProfile[CHAdeMO_QUANTITY+ CCS_QUANTITY + GB_QUANTITY]"]
["struct StructTriggerMessage\t",null,null,"TriggerMessage[CHAdeMO_QUANTITY+ CCS_QUANTITY + GB_QUANTITY]"]
["struct StructUnlockConnector",null,null,"UnlockConnector[CHAdeMO_QUANTITY+ CCS_QUANTITY + GB_QUANTITY]"]
["struct StructUpdateFirmware",null,null,"UpdateFirmware"]
["struct OCPP16ConfigurationTable\t",null,null,"ConfigurationTable"]
["struct StructChargingProfile",null,null,"CHAdeMOChargingProfile[CHAdeMO_QUANTITY]"]
["struct StructChargingProfile",null,null,"CcsChargingProfile[CCS_QUANTITY]"]
[]
[]
["Data type",null,null,"Define",{"$nulls":5},"Comment"]