{"text_format":"2","workbook":"xlsx","n_sheets":6,"sheets":["Revision","System","Charging","Network","Backend","AC_CCS"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Revision","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[[2,3,5,5]]}
[]
[]
[null,null,null,"System Configuration and Information Table"]
[]
[]
[]
[]
[null,null,"Revision History"]
[null,null,"Rev","Date","Description","Editor"]
[null,null,"01","2018/11/05","First issue","Vern Chang"]
[null,null,"02","2019/01/21","add \"PhaseLossPolicy\", \"LocalWhiteCard[10]\"","Vern Chang"]
[null,null,"03","2019/03/06","add Fan module, relay control module, CSU Primary version info","Vern Chang"]
[null,null,"04","2019/03/07","add dual charging connector info in charging sheet, eth1 info","Vern Chang"]
[null,null,"05","2019/06/14","1. remove 'SystemStatus' in SysInfoData structure(System page)                           2. add 5 parameters: 'SystemStatus'、'Index' 、'Type'、'type_index'、'EvBatterytargetCurrent' in ChargingInfoData structure( Charging page)\n","Kathy Yeh"]
[null,null,"06","2019/12/12","1. Ccs1PlugInTimes & Ccs2PlugInTimes disable on AC model\n2. CcsConnectorTemp move to Chargin information","Folus Wen"]
[null,null,"07","2020/01/07","System status contant define add","Folus Wen"]
[null,null,"08","2020/01/08","modify system status contant define","Alston Lin"]
[null,null,"09","2020/01/22","System->AuthorisationMode item cancel (Phihong backend & Phihong RFID)","Folus Wen"]
[null,null,"10","2020/01/31","Backend->Add OrderCharging for remote charging\nCharging->Add IsAvailable for check connector is enable or disable\nSystem->Add ReAssignedFlag for record how to change max to average charging step\nSystem->Add MainChargingMode for check charging mode of charger\nSystem->Add RatingCurrent for limit MaxChargingCurrent reference","Alston Lin"]
[null,null,"11","2020/02/06","Charging-> \"SystemStatus\" case 19:single run changed to 19:update","Eason Yang"]
[null,null,"12","2020/03/27","System->Version informatrion add LED control module","Folus Wen"]
[null,null,"13","2020/05/15","Add AC_CCS sheet","Edward Lien"]
[null,null,"14","2020/05/27","Refine AC_CCS sheet","Joseph Chiu"]
[null,null,"15","2020/05/27","[AC_CCS] Fixing resolution to unit.","Joseph Chiu"]
[null,null,"16","2020/05/27","[AC_CCS] Fixing MeterID info.","Joseph Chiu"]
[null,null,"17","2020/06/03","[AC_CCS] Adding EVOperation (for BPT, i.e. Bidirectional Power Transfer)","Joseph Chiu"]
[null,null,"18","2020/06/03","[AC_CCS] Adding EVChargeProgress, CpSetPWMDuty, CpSetStateE, CpPresentPWMDuty, CpPresentState, CpPositiveVoltage, CpNegativeVoltage","Joseph Chiu"]
[null,null,"19","2020/06/08","change CsuAlarmStatusCode uint16_t => uint32_t","Edward Lien"]
[null,null,"20","2020/06/09","Add CCS receive socket counter uint32_t for heart beat use ","Edward Lien"]
[null,null,"21","2020/06/11","1. [AC_CCS] Modifying R/W permission of the following variables\n    - EVCCID\n    - EVSEModelName\n    - CCSAlarmStatusCode\n    - PaymentOptions\n    - EVSEMaxCurrent\n    - EVSEMinCurrent\n2. [AC_CCS] Changing Variable Name (CCSSocketCount => CcsHeartBeat)\n3. [AC_CCS] Adding  EVSEPresentCurrent, AcOutputRelayStatus, AvailableChargingPower\n4. [AC_CCS] Modifying Name\n    - EVSENominalVoltage => GridVoltage (float)","Joseph Chiu"]
[null,null,22,"2020/06/12","1.change GridVoltage[3], EVSEPresentCurrent[3] for 3 phase.","Edward Lien"]
[null,null,"23","2020/06/15","1. [AC_CCS] Adding \"EVSENotification\"","Joseph Chiu"]

{"sheet":"System","index":1,"n_rows":56,"n_cols":27,"rows_kept":56,"cut":false,"hidden":false,"merged":[[36,0,36,2],[36,3,36,11],[36,12,36,13],[36,14,36,16],[36,17,36,19],[36,20,36,21],[36,22,36,25],[27,22,27,25],[29,0,29,2],[29,3,29,11],[29,12,29,13],[29,14,29,16],[29,17,29,19],[29,20,29,21],[29,22,29,25],[28,12,28,13],[28,14,28,16],[35,0,35,2],[35,3,35,11],[35,12,35,13],[35,14,35,16],[35,17,35,19],[35,20,35,21],[35,22,35,25],[37,3,37,11],[37,12,37,13],[37,14,37,16],[37,17,37,19],[37,20,37,21],[37,22,37,25],[34,14,34,16],[34,17,34,19],[34,20,34,21],[34,22,34,25],[34,12,34,13],[0,20,0,21],[0,22,0,25],[2,0,2,2],[2,3,2,11],[2,12,2,13],[2,14,2,16],[2,17,2,19],[2,20,2,21],[2,22,2,25],[0,0,0,2],[0,3,0,11],[0,12,0,13],[0,14,0,16],[0,17,0,19],[1,0,1,25],[22,0,22,2],[22,3,22,11],[22,12,22,13],[22,14,22,16],[22,17,22,19],[22,20,22,21],[22,22,22,25],[21,0,21,25],[6,0,6,2],[6,3,6,11],[6,12,6,13],[7,22,7,25],[8,0,8,2],[8,3,8,11],[8,12,8,13],[8,14,8,16],[8,17,8,19],[8,20,8,21],[8,22,8,25],[6,14,6,16],[6,17,6,19],[6,20,6,21],[6,22,6,25],[7,0,7,2],[38,22,38,25],[38,0,38,2],[38,3,38,11],[38,12,38,13],[38,14,38,16],[38,17,38,19],[38,20,38,21],[32,22,32,25],[33,0,33,2],[33,3,33,11],[33,12,33,13],[33,14,33,16],[33,17,33,19],[33,20,33,21],[33,22,33,25],[32,0,32,2],[32,3,32,11],[32,12,32,13],[37,0,37,2],[32,14,32,16],[32,17,32,19],[32,20,32,21],[34,0,34,2],[34,3,34,11],[46,12,46,13],[46,14,46,16],[46,17,46,19],[46,20,46,21],[46,22,46,25],[45,0,45,2],[45,3,45,11],[45,12,45,13],[45,14,45,16],[45,17,45,19],[45,20,45,21],[41,3,41,11],[41,12,41,13],[41,14,41,16],[41,17,41,19],[47,22,47,25],[48,0,48,2],[48,3,48,11],[48,12,48,13],[48,14,48,16],[48,17,48,19],[48,20,48,21],[48,22,48,25],[47,0,47,2],[47,3,47,11],[47,12,47,13],[47,14,47,16],[47,17,47,19],[47,20,47,21],[42,20,42,21],[42,22,42,25],[44,0,44,25],[45,22,45,25],[46,0,46,2],[46,3,46,11],[49,22,49,25],[50,0,50,2],[50,3,50,11],[50,12,50,13],[50,14,50,16],[50,17,50,19],[50,20,50,21],[50,22,50,25],[49,0,49,2],[49,3,49,11],[49,12,49,13],[49,14,49,16],[49,17,49,19],[49,20,49,21],[52,12,52,13],[52,14,52,16],[52,17,52,19],[52,20,52,21],[52,22,52,25],[51,0,51,2],[51,3,51,11],[51,12,51,13],[51,14,51,16],[51,17,51,19],[51,20,51,21],[25,0,25,2],[25,3,25,11],[25,12,25,13],[25,14,25,16],[25,17,25,19],[25,20,25,21],[25,22,25,25],[28,0,28,2],[28,3,28,11],[26,14,26,16],[26,17,26,19],[26,20,26,21],[26,22,26,25],[27,3,27,11],[27,12,27,13],[27,14,27,16],[27,17,27,19],[27,20,27,21],[23,20,23,21],[23,22,23,25],[24,0,24,2],[24,3,24,11],[31,0,31,2],[31,3,31,11],[31,12,31,13],[31,14,31,16],[31,17,31,19],[31,20,31,21],[28,17,28,19],[28,20,28,21],[28,22,28,25],[30,0,30,2],[30,3,30,11],[30,12,30,13],[30,14,30,16],[30,17,30,19],[30,20,30,21],[30,22,30,25],[27,0,27,2],[26,0,26,2],[26,3,26,11],[26,12,26,13],[5,22,5,25],[5,0,5,2],[5,3,5,11],[5,12,5,13],[5,14,5,16],[5,17,5,19],[5,20,5,21],[3,22,3,25],[4,0,4,2],[4,3,4,11],[4,12,4,13],[4,14,4,16],[4,17,4,19],[4,20,4,21],[4,22,4,25],[3,0,3,2],[3,3,3,11],[3,12,3,13],[3,14,3,16],[3,17,3,19],[3,20,3,21],[7,3,7,11],[7,12,7,13],[7,14,7,16],[7,17,7,19],[7,20,7,21],[9,22,9,25],[10,0,10,2],[10,3,10,11],[10,12,10,13],[10,14,10,16],[10,17,10,19],[10,20,10,21],[10,22,10,25],[9,0,9,2],[9,3,9,11],[9,12,9,13],[9,14,9,16],[9,17,9,19],[9,20,9,21],[24,17,24,19],[24,20,24,21],[24,22,24,25],[31,22,31,25],[23,0,23,2],[23,3,23,11],[40,0,40,25],[11,22,11,25],[12,0,12,2],[12,3,12,11],[12,12,12,13],[12,14,12,16],[12,17,12,19],[12,20,12,21],[12,22,12,25],[11,0,11,2],[11,3,11,11],[11,12,11,13],[11,14,11,16],[11,17,11,19],[11,20,11,21],[23,12,23,13],[23,14,23,16],[23,17,23,19],[20,0,20,2],[20,3,20,11],[20,12,20,13],[20,14,20,16],[20,17,20,19],[20,20,20,21],[20,22,20,25],[43,0,43,2],[43,3,43,11],[43,12,43,13],[43,14,43,16],[43,17,43,19],[43,20,43,21],[43,22,43,25],[41,0,41,2],[41,20,41,21],[41,22,41,25],[42,0,42,2],[42,3,42,11],[42,12,42,13],[42,14,42,16],[42,17,42,19],[24,12,24,13],[24,14,24,16],[19,0,19,2],[19,3,19,11],[19,12,19,13],[19,14,19,16],[19,17,19,19],[19,20,19,21],[19,22,19,25],[17,0,17,2],[17,3,17,11],[17,12,17,13],[17,14,17,16],[17,17,17,19],[17,20,17,21],[17,22,17,25],[14,14,14,16],[14,17,14,19],[14,20,14,21],[14,22,14,25],[16,0,16,25],[18,0,18,2],[18,3,18,11],[18,12,18,13],[18,14,18,16],[18,17,18,19],[18,20,18,21],[18,22,18,25],[55,0,55,2],[55,3,55,11],[55,12,55,13],[55,14,55,16],[55,17,55,19],[55,20,55,21],[55,22,55,25],[13,0,13,2],[13,3,13,11],[13,12,13,13],[13,14,13,16],[13,17,13,19],[13,20,13,21],[13,22,13,25],[15,0,15,2],[15,3,15,11],[15,12,15,13],[15,14,15,16],[15,17,15,19],[15,20,15,21],[15,22,15,25],[14,0,14,2],[14,3,14,11],[14,12,14,13],[39,0,39,2],[39,3,39,11],[39,12,39,13],[39,14,39,16],[39,17,39,19],[39,20,39,21],[39,22,39,25],[54,0,54,2],[54,3,54,11],[54,12,54,13],[54,14,54,16],[54,17,54,19],[54,20,54,21],[54,22,54,25],[53,22,53,25],[53,0,53,2],[53,3,53,11],[53,12,53,13],[53,14,53,16],[53,17,53,19],[53,20,53,21],[51,22,51,25],[52,0,52,2],[52,3,52,11]]}
["Parameter",null,null,"Description",{"$nulls":8},"Value Type",null,"Range",null,null,"Default Value",null,null,"Authority",null,"Applied Model"]
["System Information"]
["ModelName",null,null,"charger model name",{"$nulls":8},"string ",null,"64 Bytes",null,null,"(NULL)",null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysConfigData"]
["SerialNumber",null,null,"charger system serial number",{"$nulls":8},"string ",null,"64 Bytes",null,null,"(NULL)",null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysConfigData"]
["SystemId",null,null,"charger system ID",{"$nulls":8},"string ",null,"128 Bytes",null,null,"(NULL)",null,null,"R/W",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysConfigData"]
["SystemDateTime",null,null,"charger system date and time",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(RTC default)",null,null,"R/W",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysConfigData"]
["FactoryConfiguration",null,null,"charger will return the configuration to factory default if trigger",{"$nulls":8},"integer",null,"0: normal\n1: trigger",null,null,0,null,null,"R/W",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysInfoData"]
["AuthorisationMode",null,null,"charger will do user authorizing according the authorisation mode ",{"$nulls":8},"integer",null,"0: OCPP backend\n1: free mode",null,null,0,null,null,"R/W",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysConfigData"]
["DefaultLanguage",null,null,"the default language shows on the screen",{"$nulls":8},"integer",null,"0: English\n1: 繁體中文\n2: 简体中文\n3: 日本語\n4: Français\n5: Italiano\n6: Español\n7: Deutsch\n8: Nederland\n9: Norsk\n10: Suomalainen\n11: Svenska\n12: Pусский\n13: ไทย",null,null,0,null,null,"R/W",null,"□AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["InputVoltageR",null,null,"phase R input voltage",{"$nulls":8},"float ",null,"0~655.35 volt",null,null,0,null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysInfoData"]
["InputVoltageS",null,null,"phase S input voltage",{"$nulls":8},"float ",null,"0~655.35 volt",null,null,0,null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysInfoData"]
["InputVoltageT",null,null,"phase T input voltage",{"$nulls":8},"float ",null,"0 ~ 655.35 volt",null,null,0,null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysInfoData"]
["SystemFanRotaSpeed",null,null,"the rotating speed of system fan",{"$nulls":8},"integer",null,"0 ~ 65535 RPM",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["PsuFanRotaSpeed",null,null,"the rotating speed of PSU fan",{"$nulls":8},"integer",null,"0 ~ 65535 RPM",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["RfidCardNumEndian",null,null,"switch RFID card number endian",{"$nulls":8},"integer",null,"0: little endian\n1: big endian",null,null,0,null,null,"R/W",null,"■AC Net ■AC Eco ■DC"]
["RatingCurrent",null,null,"EVSE current rating value",{"$nulls":8},"integer",null,"0: Dependon Model name\n1 ~ rating value amp",null,null,0,null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysConfigData"]
["Aux. power Information"]
["AuxPower5V",null,null,"present 5V aux. power voltage from aux. power module",{"$nulls":8},"integer",null,"0 ~ 255 volt",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["AuxPower12V",null,null,"present 12V aux. power voltage from aux. power module",{"$nulls":8},"integer",null,"0 ~ 255 volt",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["AuxPower24V",null,null,"present 24V aux. power voltage from aux. power module",{"$nulls":8},"integer",null,"0 ~ 255 volt",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["AuxPower48V",null,null,"present 48V aux. power voltage from aux. power module",{"$nulls":8},"integer",null,"0 ~ 255 volt",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["Version Information"]
["CsuHwRev",null,null,"CSU board hardware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysInfoData"]
["CsuBootLoadFwRev",null,null,"CSU board bootloader firmware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysInfoData"]
["CsuKernelFwRev",null,null,"CSU board OS kernel firmware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysInfoData"]
["CsuRootFsFwRev",null,null,"CSU board root file system firmware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysInfoData"]
["CsuPrimFwRev",null,null,"CSU Primary chip firmware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysInfoData"]
["LcmHwRev",null,null,"LCM module hardware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["LcmFwRev",null,null,"LCM module firmware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["PsuHwRev",null,null,"PSU hardware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["PsuPrimFwRev",null,null,"PSU primary firmware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["PsuSecFwRev",null,null,"PSU secondary firmware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["AuxPwrHwRev",null,null,"Aux. power module hardware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["AuxPwrFwRev",null,null,"Aux. power module firmware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["FanModuleHwRev",null,null,"Fan  module hardware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["FanModuleFwRev",null,null,"Fan  module firmware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["RelayModuleHwRev",null,null,"Relay control  module hardware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["RelayModuleFwRev",null,null,"Relay control  module firmware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["TelcomModemFwRev",null,null,"the 3G/4G modem firmware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["LedModuleFwRev",null,null,"LED controle module firmware version",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["Temperature Information"]
["SystemAmbientTemp",null,null,"system ambient temperature as air intake temperature",{"$nulls":8},"integer",null," -40 ~ 215 degree C",null,null,0,null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysInfoData"]
["SystemCriticalTemp",null,null,"the temperature of critical module inside the system",{"$nulls":8},"integer",null," -40 ~ 215 degree C",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["PsuAmbientTemp",null,null,"the ambient temperature of PSU ",{"$nulls":8},"integer",null," -40 ~ 215 degree C",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["Connector Plug-in Information"]
["AcPlugInTimes",null,null,"AC connector plug-in times",{"$nulls":8},"integer",null,"0~65535",null,null,0,null,null,"RO",null,"■AC Net ■AC Eco ■DC"]
["GbPlugInTimes",null,null,"GB connector plug-in times",{"$nulls":8},"integer",null,"0~65535",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC"]
["Ccs1PlugInTimes",null,null,"CCS1 connector plug-in times",{"$nulls":8},"integer",null,"0~65535",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC"]
["Ccs2PlugInTimes",null,null,"CCS2 connector plug-in times",{"$nulls":8},"integer",null,"0~65535",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC"]
["ChademoPlugInTimes",null,null,"CHAdeMO connector plug-in times",{"$nulls":8},"integer",null,"0~65535",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC"]
[]
[]
[]
[]
["ReAssignedFlag",null,null,"to change max to average charging step",{"$nulls":8},"unsigned char",{"$nulls":4},0,null,null,"RO",null,"□AC Net □AC Eco ■DC"]
["MainChargingMode",null,null,"CHAdeMO connector plug-in times",{"$nulls":8},"unsigned char",null,"0 : Max\n1 : Average",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC"]

{"sheet":"Charging","index":2,"n_rows":28,"n_cols":27,"rows_kept":28,"cut":false,"hidden":false,"merged":[[8,0,8,2],[8,3,8,11],[8,12,8,13],[8,14,8,16],[8,17,8,19],[8,20,8,21],[8,22,8,25],[9,0,9,2],[9,3,9,11],[9,12,9,13],[9,14,9,16],[9,17,9,19],[9,20,9,21],[9,22,9,25],[7,12,7,13],[7,14,7,16],[7,17,7,19],[7,20,7,21],[7,22,7,25],[0,22,0,25],[1,0,1,25],[2,0,2,2],[2,3,2,11],[2,12,2,13],[2,14,2,16],[2,17,2,19],[2,20,2,21],[2,22,2,25],[0,0,0,2],[0,3,0,11],[0,12,0,13],[0,14,0,16],[0,17,0,19],[0,20,0,21],[3,22,3,25],[4,0,4,2],[4,3,4,11],[4,12,4,13],[4,14,4,16],[4,17,4,19],[4,20,4,21],[4,22,4,25],[3,0,3,2],[3,3,3,11],[3,12,3,13],[3,14,3,16],[3,17,3,19],[3,20,3,21],[5,22,5,25],[10,0,10,25],[11,0,11,2],[11,3,11,11],[11,12,11,13],[11,14,11,16],[11,20,11,21],[11,22,11,25],[5,0,5,2],[5,3,5,11],[5,12,5,13],[5,14,5,16],[5,17,5,19],[5,20,5,21],[11,17,11,19],[6,0,6,2],[6,3,6,11],[6,12,6,13],[6,14,6,16],[6,17,6,19],[6,20,6,21],[6,22,6,25],[7,0,7,2],[7,3,7,11],[12,22,12,25],[13,0,13,2],[13,3,13,11],[13,12,13,13],[13,14,13,16],[13,17,13,19],[13,20,13,21],[13,22,13,25],[12,0,12,2],[12,3,12,11],[12,12,12,13],[12,14,12,16],[12,17,12,19],[12,20,12,21],[14,22,14,25],[15,0,15,2],[15,3,15,11],[15,12,15,13],[15,14,15,16],[15,17,15,19],[15,20,15,21],[15,22,15,25],[14,0,14,2],[14,3,14,11],[14,12,14,13],[14,14,14,16],[14,17,14,19],[14,20,14,21],[17,3,17,11],[17,12,17,13],[17,14,17,16],[17,17,17,19],[17,20,17,21],[17,22,17,25],[16,0,16,2],[16,3,16,11],[16,12,16,13],[16,14,16,16],[16,17,16,19],[16,20,16,21],[16,22,16,25],[17,0,17,2],[18,22,18,25],[19,0,19,2],[19,3,19,11],[19,12,19,13],[19,14,19,16],[19,17,19,19],[19,20,19,21],[19,22,19,25],[18,0,18,2],[18,3,18,11],[18,12,18,13],[18,14,18,16],[18,17,18,19],[18,20,18,21],[21,0,21,2],[21,3,21,11],[21,12,21,13],[21,14,21,16],[21,17,21,19],[21,20,21,21],[21,22,21,25],[20,22,20,25],[20,0,20,2],[20,3,20,11],[20,12,20,13],[20,14,20,16],[20,17,20,19],[20,20,20,21],[22,0,22,2],[22,3,22,11],[22,12,22,13],[22,14,22,16],[22,17,22,19],[22,20,22,21],[22,22,22,25],[23,0,23,2],[23,3,23,11],[23,12,23,13],[23,14,23,16],[23,17,23,19],[23,20,23,21],[23,22,23,25],[24,0,24,2],[24,3,24,11],[24,12,24,13],[24,14,24,16],[24,17,24,19],[24,20,24,21],[24,22,24,25],[25,0,25,2],[25,3,25,11],[25,12,25,13],[25,14,25,16],[25,17,25,19],[25,20,25,21],[25,22,25,25],[27,0,27,2],[27,3,27,11],[27,12,27,13],[27,14,27,16],[27,17,27,19],[27,20,27,21],[27,22,27,25],[26,0,26,2],[26,3,26,11],[26,12,26,13],[26,14,26,16],[26,17,26,19],[26,20,26,21],[26,22,26,25]]}
["Parameter",null,null,"Description",{"$nulls":8},"Value Type",null,"Range",null,null,"Default Value",null,null,"Authority",null,"Applied Model"]
["Charging relevant parameters"]
["MaxChargingEnergy",null,null,"the maximum charging energy per charge, charger will stop charging if present output energy reach to this threshold",{"$nulls":8},"integer",null,"0: no limit\n1 ~ 65535 kWh",null,null,0,null,null,"R/W",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysConfigData"]
["MaxChargingPower",null,null,"the maximum charging power for each charge",{"$nulls":8},"integer",null,"0: rating value\n1 ~ rating value kW",null,null,0,null,null,"R/W",null,"□AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["MaxChargingCurrent",null,null,"the maximum charging current for each charge",{"$nulls":8},"integer",null,"0: rating value\n1 ~ rating value amp",null,null,0,null,null,"R/W",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysConfigData"]
["MaxChargingDuration",null,null,"the maximum charging duration for each charge",{"$nulls":8},"integer",null,"0: no limit\n1 ~ 65535 minutes",null,null,0,null,null,"R/W",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysConfigData"]
["PhaseLossPolicy",null,null,"the charger will check this setting to see if go into charging state under phase loss ",{"$nulls":8},"integer",null,"0: charging\n1: stop charging",null,null,0,null,null,"R/W",null,"□AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["LocalWhiteCard[10]",null,null,"this array stores the ID of administrator RFID card, charger will bypass the user authentication if administrator RFID card be swiped.",{"$nulls":8},"string ",null,"32 Bytes x10 ",null,null,"(NULL)",null,null,"R/W",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysConfigData"]
["CcsAuthentication",null,null,"Authentication mode in CCS charging",{"$nulls":8},"integer",null,"0: EIM\n1: EIM&PnC mixed",null,null,0,null,null,"R/W",null,"■AC Net ■AC Eco ■DC"]
["AcCcsChargingMode",null,null,"CCS charging mode in AC charging",{"$nulls":8},"integer",null,"0: BC (PWM) only\n1: BC&PLC mixed",null,null,1,null,null,"R/W",null,"■AC Net ■AC Eco ■DC"]
["Charging Information"]
["UserId",null,null,"the user use this ID to trigger charging event, it can be RFID card number, OCPP IdTag, etc.",{"$nulls":8},"string ",null,"32 Bytes",null,null,"(NULL)",null,null,"R/W",null,"■AC Net ■AC Eco ■DC",null,null,null,"SysConfigData"]
["PresentChargingVoltage",null,null,"present output voltage ",{"$nulls":8},"float ",null,"0~6553.5 volt",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"ChargingInfoData"]
["PresentChargingCurrent",null,null,"present output whole current ",{"$nulls":8},"float ",null,"0~6553.5 amp",null,null,0,null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"ChargingInfoData"]
["PresentChargingPower",null,null,"present output whole power",{"$nulls":8},"float ",null,"0~6553.5 kW",null,null,0,null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"ChargingInfoData"]
["PresentChargedEnergy",null,null,"the charged energy of this charging event ",{"$nulls":8},"float ",null,"0~6553.5 kWh",null,null,0,null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"ChargingInfoData"]
["PresentChargedDuration",null,null,"present charged duration of this charge ",{"$nulls":8},"integer",null,"0~65535 second",null,null,0,null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"ChargingInfoData"]
["RemainChargingDuration",null,null,"this value will be the less one of BMS and charger calculating value",{"$nulls":8},"integer",null,"0~65535 second",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"ChargingInfoData"]
["EvBatteryMaxVoltage",null,null,"EV battery maximum voltage",{"$nulls":8},"float ",null,"0~6553.5 volt",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"ChargingInfoData"]
["EvBatterytargetVoltage",null,null,"EV battery target voltage",{"$nulls":8},"float ",null,"0~6553.5 volt",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"ChargingInfoData"]
["EvBatterySoc",null,null,"present EV battery SOC",{"$nulls":8},"integer",null,"0~100 %",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"ChargingInfoData"]
["SystemStatus",null,null,"charger system present status",{"$nulls":8},"integer",null,"0: booting\n1: idle\n2: authorizing\n3: reassign check\n4: reassign\n5: preparing\n6: preparing for EV\n7: preparing for evse\n8: charging\n9: terminating\n10: complete\n11: alarm\n12: fault\n13: reservation\n14: booking\n15: maintain\n16: debug\n17: precharge step 0\n18:precharge step 1\n19:update",null,null,0,null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"ChargingInfoData"]
["Index",null,null,"connector Id",{"$nulls":8},"integer",null,"0 : connector 1\n1 : connector 2\n2 : connector 3\n3 : connector 4",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"ChargingInfoData"]
["Type",null,null,"model Type",{"$nulls":8},"integer",null,"0 : Chademo\n1 : CCS\n2 : GB",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"ChargingInfoData"]
["type_index",null,null,"connector index by model type",{"$nulls":8},"integer",{"$nulls":4},0,null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"ChargingInfoData"]
["EvBatterytargetCurrent",null,null,"EV battery target current",{"$nulls":8},"float ",null,"0~200(A)",null,null,0,null,null,"RO",null,"□AC Net □AC Eco ■DC",null,null,null,"ChargingInfoData"]
["CcsConnectorTemp",null,null,"the temperature of CCS connector",{"$nulls":8},"integer",null," -40 ~ 215 degree C",null,null,0,null,null,"RO",null,"■AC Net ■AC Eco ■DC",null,null,null,"ChargingInfoData"]
["IsAvailable",null,null,"Check if the connector is available or disabled",{"$nulls":8},"unsigned char",null,"0 : disable\n1 : enable",null,null,1,null,null,"RO",null,"■AC Net ■AC Eco ■DC"]

{"sheet":"Network","index":3,"n_rows":37,"n_cols":27,"rows_kept":37,"cut":false,"hidden":false,"merged":[[0,22,0,25],[4,0,4,25],[5,0,5,2],[5,3,5,11],[5,12,5,13],[5,14,5,16],[5,17,5,19],[5,20,5,21],[5,22,5,25],[1,0,1,25],[0,0,0,2],[0,3,0,11],[0,12,0,13],[0,14,0,16],[0,17,0,19],[0,20,0,21],[6,22,6,25],[7,0,7,2],[7,3,7,11],[7,12,7,13],[7,14,7,16],[7,17,7,19],[7,20,7,21],[7,22,7,25],[6,0,6,2],[6,3,6,11],[6,12,6,13],[6,14,6,16],[6,17,6,19],[6,20,6,21],[15,0,15,25],[16,0,16,2],[16,3,16,11],[8,22,8,25],[9,0,9,2],[9,3,9,11],[9,12,9,13],[9,14,9,16],[9,17,9,19],[9,20,9,21],[9,22,9,25],[8,0,8,2],[8,3,8,11],[8,12,8,13],[8,14,8,16],[8,17,8,19],[8,20,8,21],[16,12,16,13],[16,14,16,16],[16,17,16,19],[16,20,16,21],[16,22,16,25],[10,0,10,2],[10,3,10,11],[27,0,27,2],[27,3,27,11],[27,12,27,13],[27,14,27,16],[27,17,27,19],[27,20,27,21],[27,22,27,25],[25,17,25,19],[24,22,24,25],[25,0,25,2],[25,3,25,11],[25,12,25,13],[25,14,25,16],[25,20,25,21],[25,22,25,25],[24,0,24,2],[24,3,24,11],[24,12,24,13],[24,14,24,16],[24,17,24,19],[24,20,24,21],[17,0,17,2],[17,3,17,11],[17,12,17,13],[17,14,17,16],[17,17,17,19],[17,20,17,21],[17,22,17,25],[18,0,18,2],[18,3,18,11],[18,12,18,13],[18,14,18,16],[18,17,18,19],[18,20,18,21],[18,22,18,25],[23,3,23,11],[23,12,23,13],[23,14,23,16],[23,17,23,19],[23,20,23,21],[21,22,21,25],[22,0,22,2],[22,3,22,11],[22,12,22,13],[22,14,22,16],[22,17,22,19],[22,20,22,21],[22,22,22,25],[21,0,21,2],[21,3,21,11],[21,12,21,13],[21,14,21,16],[21,17,21,19],[21,20,21,21],[35,22,35,25],[35,0,35,2],[35,3,35,11],[35,12,35,13],[35,14,35,16],[35,17,35,19],[35,20,35,21],[29,22,29,25],[30,0,30,2],[30,3,30,11],[30,12,30,13],[30,14,30,16],[30,17,30,19],[30,20,30,21],[30,22,30,25],[29,0,29,2],[29,3,29,11],[29,12,29,13],[29,14,29,16],[29,17,29,19],[29,20,29,21],[34,3,34,11],[34,12,34,13],[34,14,34,16],[19,22,19,25],[31,0,31,2],[31,3,31,11],[31,12,31,13],[31,14,31,16],[31,17,31,19],[31,20,31,21],[31,22,31,25],[19,0,19,2],[19,3,19,11],[19,12,19,13],[19,14,19,16],[19,17,19,19],[19,20,19,21],[23,22,23,25],[26,0,26,25],[28,0,28,2],[28,3,28,11],[28,12,28,13],[28,14,28,16],[28,17,28,19],[28,20,28,21],[28,22,28,25],[23,0,23,2],[34,17,34,19],[34,20,34,21],[32,22,32,25],[33,0,33,2],[33,3,33,11],[33,12,33,13],[33,14,33,16],[33,17,33,19],[33,20,33,21],[33,22,33,25],[32,0,32,2],[32,3,32,11],[32,12,32,13],[32,14,32,16],[32,17,32,19],[32,20,32,21],[36,0,36,25],[2,22,2,25],[3,0,3,2],[3,3,3,11],[3,12,3,13],[3,14,3,16],[3,17,3,19],[3,20,3,21],[3,22,3,25],[2,0,2,2],[2,3,2,11],[2,12,2,13],[2,14,2,16],[2,17,2,19],[2,20,2,21],[34,22,34,25],[20,0,20,2],[20,3,20,11],[20,12,20,13],[20,14,20,16],[20,17,20,19],[20,20,20,21],[20,22,20,25],[34,0,34,2],[10,12,10,13],[10,14,10,16],[10,17,10,19],[10,20,10,21],[10,22,10,25],[11,0,11,2],[11,3,11,11],[11,12,11,13],[11,14,11,16],[11,17,11,19],[11,20,11,21],[11,22,11,25],[14,0,14,2],[14,3,14,11],[14,12,14,13],[14,14,14,16],[14,17,14,19],[14,20,14,21],[14,22,14,25],[12,0,12,2],[12,3,12,11],[12,12,12,13],[12,14,12,16],[12,17,12,19],[12,20,12,21],[12,22,12,25],[13,0,13,2],[13,3,13,11],[13,12,13,13],[13,14,13,16],[13,17,13,19],[13,20,13,21],[13,22,13,25]]}
["Parameter",null,null,"Description",{"$nulls":8},"Value Type",null,"Range",null,null,"Default Value",null,null,"Authority",null,"Applied Model"]
["Network Status"]
["InternetConn",null,null,"the status of internet connection ",{"$nulls":8},"integer",null,"0: disconnected\n1: connected",null,null,0,null,null,"RO",null,"■AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["FtpServer",null,null,"the ftp server for Phihong server to do data transimission",{"$nulls":8},"string ",null,"256 Bytes",null,null,"(NULL)",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["Ethernet Interface"]
["Eth0DhcpClient",null,null,"DHCP client will be ran via Ethernet interface 0 if enabled",{"$nulls":8},"integer",null,"0: enable\n1: disable",null,null,0,null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["Eth0MacAddress",null,null,"the Ethernet interface 0 MAC address",{"$nulls":8},"string ",null,"18 Bytes",null,null,"(NULL)",null,null,"RO",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["Eth0IpAddress",null,null,"the Ethernet interface 0 IP address",{"$nulls":8},"string ",null,"16 Bytes",null,null,"192.168.0.10",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["Eth0SubmaskAddress",null,null,"the Ethernet interface 0 submask address",{"$nulls":8},"string ",null,"16 Bytes",null,null,"255.255.255.0",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["Eth0GatewayAddress",null,null,"the Ethernet interface 0 gateway address",{"$nulls":8},"string ",null,"16 Bytes",null,null,"192.168.0.254",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["Eth1DhcpClient",null,null,"DHCP client will be ran via Ethernet interface 1 if enabled",{"$nulls":8},"integer",null,"0: enable\n1: disable",null,null,0,null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["Eth1MacAddress",null,null,"the Ethernet interface 1 MAC address",{"$nulls":8},"string ",null,"18 Bytes",null,null,"(NULL)",null,null,"RO",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["Eth1IpAddress",null,null,"the Ethernet interface 1 IP address",{"$nulls":8},"string ",null,"16 Bytes",null,null,"192.168.1.10",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["Eth1SubmaskAddress",null,null,"the Ethernet interface 1 submask address",{"$nulls":8},"string ",null,"16 Bytes",null,null,"255.255.255.0",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["Eth1GatewayAddress",null,null,"the Ethernet interface 1 gateway address",{"$nulls":8},"string ",null,"16 Bytes",null,null,"192.168.1.254",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["WiFi Module"]
["WifiMode",null,null,"the mode of WiFi module",{"$nulls":8},"integer",null,"0: disable\n1: Infrastructure client\n2: Infrastructure server\n3: Ad-Hoc",null,null,1,null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["WifiSsid",null,null,"the SSID which client want to connect or server want to establish",{"$nulls":8},"string ",null,"255 Bytes",null,null,"(NULL)",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["WifiPassword",null,null,"the password or preshare key for client to do login or server to do authorization ",{"$nulls":8},"string ",null,"128 Bytes",null,null,"(NULL)",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["WifiRssi",null,null,"the received signal strength of WiFi connection",{"$nulls":8},"integer",null," -100 ~ 0 dBm",null,null,0,null,null,"RO",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["WifiDhcpServer",null,null,"DHCP server will be ran under infrastructure server mode if enabled",{"$nulls":8},"integer",null,"0: enable\n1: disable",null,null,0,null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["WifiDhcpClient",null,null,"DHCP client will be ran via WiFi module if enabled",{"$nulls":8},"integer",null,"0: enable\n1: disable",null,null,0,null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["WifiMacAddress",null,null,"the WiFi MAC address",{"$nulls":8},"string ",null,"18 Bytes",null,null,"(NULL)",null,null,"RO",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["WifiIpAddress",null,null,"the WiFi IP address",{"$nulls":8},"string ",null,"16 Bytes",null,null,"(NULL)",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["WifiSubmaskAddress",null,null,"the WiFi submask address",{"$nulls":8},"string ",null,"16 Bytes",null,null,"(NULL)",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["WifiGatewayAddress",null,null,"the WiFi gateway address",{"$nulls":8},"string ",null,"16 Bytes",null,null,"(NULL)",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["3G/4G Module"]
["TelcomApn",null,null,"the APN which charger want to connected",{"$nulls":8},"string ",null,"256 Bytes",null,null,"(NULL)",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["TelcomRssi",null,null,"the signal strength of 3G/4G connection",{"$nulls":8},"integer",null," -100 ~ 0 dBm",null,null,0,null,null,"RO",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["TelcomChapPapId",null,null,"the login ID for CHAP/PAP authentication ",{"$nulls":8},"string ",null,"256 Bytes",null,null,"(NULL)",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["TelcomChapPapPwd",null,null,"the login password for CHAP/PAP authentication ",{"$nulls":8},"string ",null,"256 Bytes",null,null,"(NULL)",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["TelcomModemImei",null,null,"the IMEI code of this telcom modem",{"$nulls":8},"string ",null,"16 Bytes",null,null,"(NULL)",null,null,"RO",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["TelcomSimImsi",null,null,"the IMSI code of this SIM card",{"$nulls":8},"string ",null,"16 Bytes",null,null,"(NULL)",null,null,"RO",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["TelcomSimStatus",null,null,"Present SIM card status",{"$nulls":8},"integer",null,"0: no SIM card is found\n1: valid SIM card\n2: invalid SIM card",null,null,0,null,null,"RO",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["TelcomModemMode",null,null,"Present telcom system mode through this modem",{"$nulls":8},"integer",null,"0: No services\n1: CDMA \n2: GSM/GPRS\n3: WCDMA\n4: GSM/WCDMA\n5: TD_SCDMA mode\n6: Unknow",null,null,0,null,null,"RO",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["TelcomIpAddress",null,null,"the IP address got from telcom ",{"$nulls":8},"string ",null,"16 Bytes",null,null,"(NULL)",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["Bluetooth Module"]

{"sheet":"Backend","index":4,"n_rows":12,"n_cols":27,"rows_kept":12,"cut":false,"hidden":false,"merged":[[5,22,5,25],[4,12,4,13],[4,14,4,16],[4,17,4,19],[4,20,4,21],[4,22,4,25],[0,22,0,25],[1,0,1,25],[9,0,9,2],[9,3,9,11],[9,12,9,13],[9,14,9,16],[9,17,9,19],[9,20,9,21],[9,22,9,25],[6,0,6,25],[0,0,0,2],[0,3,0,11],[0,12,0,13],[0,14,0,16],[0,17,0,19],[0,20,0,21],[3,22,3,25],[7,0,7,2],[7,3,7,11],[7,12,7,13],[7,14,7,16],[7,17,7,19],[7,20,7,21],[7,22,7,25],[3,0,3,2],[3,3,3,11],[3,12,3,13],[3,14,3,16],[3,17,3,19],[3,20,3,21],[4,0,4,2],[4,3,4,11],[2,22,2,25],[11,0,11,25],[10,0,10,2],[10,3,10,11],[10,12,10,13],[10,14,10,16],[10,17,10,19],[10,20,10,21],[10,22,10,25],[2,0,2,2],[5,0,5,2],[5,3,5,11],[5,12,5,13],[5,14,5,16],[5,17,5,19],[5,20,5,21],[2,3,2,11],[2,12,2,13],[2,14,2,16],[2,17,2,19],[2,20,2,21],[8,20,8,21],[8,22,8,25],[8,0,8,2],[8,3,8,11],[8,12,8,13],[8,14,8,16],[8,17,8,19]]}
["Parameter",null,null,"Description",{"$nulls":8},"Value Type",null,"Range",null,null,"Default Value",null,null,"Authority",null,"Applied Model"]
["Common Information"]
["BackendConnTimeout",null,null,"the timeout time of the backend connection",{"$nulls":8},"integer",null,"0 ~ 86400 second",null,null,300,null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["OfflinePolicy",null,null,"the user authrization policy if disconnected from backend",{"$nulls":8},"integer",null,"0: local list\n1: Phihong RFID tag\n2: free charging\n3: no charging",null,null,0,null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["OfflineMaxChargeEnergy",null,null,"the maximum charging energy per charge when offline, charger will stop charging if present output energy reach to this threshold",{"$nulls":8},"integer",null,"0: same as MaxChargingEnergy\n1 ~ 65535 kWh",null,null,0,null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["OfflineMaxChargeDuration",null,null,"the maximum charging duration for each charge when offline",{"$nulls":8},"integer",null,"0: same as MaxChargeDuration\n1 ~ 65535 minutes",null,null,0,null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["OCPP Backend"]
["OcppConnStatus",null,null,"the connection status of OCPP backend",{"$nulls":8},"integer",null,"0: disconnected\n1: connected",null,null,0,null,null,"RO",null,"■AC Net □AC Eco ■DC",null,null,null,"SysInfoData"]
["OrderCharging",null,null,"for remote charging of OCPP method",{"$nulls":8},"char",null,"1 Bytes",null,null,0,null,null,"R/W",null,"■AC Net □AC Eco ■DC"]
["OcppServerURL",null,null,"the OCPP server which charger want to connected.\nhttp: non-secure OCPP 1.5-S\nhttps: secure OCPP 1.5-S\nws: non-secure OCPP 1.6-J\nwss: secure OCPP 1.6-J",{"$nulls":8},"string ",null,"512 Bytes",null,null,"(NULL)",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["ChargeBoxId",null,null,"the charge box ID will use to connect to OCPP server",{"$nulls":8},"string ",null,"128 Bytes",null,null,"(NULL)",null,null,"R/W",null,"■AC Net □AC Eco ■DC",null,null,null,"SysConfigData"]
["Phihong Backend"]

{"sheet":"AC_CCS","index":5,"n_rows":38,"n_cols":25,"rows_kept":38,"cut":false,"hidden":false,"merged":[[33,0,33,2],[33,3,33,11],[33,12,33,13],[33,14,33,16],[33,17,33,19],[33,20,33,21],[33,22,33,23],[33,24,33,27],[3,22,3,23],[3,17,3,19],[3,14,3,16],[3,12,3,13],[3,3,3,11],[3,0,3,2],[3,24,3,27],[19,20,19,21],[7,20,7,21],[6,20,6,21],[5,20,5,21],[4,20,4,21],[3,20,3,21],[12,3,12,11],[12,0,12,2],[14,22,14,23],[14,24,14,27],[4,22,4,23],[4,24,4,27],[4,0,4,2],[5,22,5,23],[5,17,5,19],[5,14,5,16],[5,12,5,13],[5,3,5,11],[5,0,5,2],[12,12,12,13],[12,14,12,16],[12,17,12,19],[13,12,13,13],[13,14,13,16],[13,17,13,19],[13,20,13,21],[6,17,6,19],[6,14,6,16],[11,17,11,19],[11,22,11,23],[6,12,6,13],[8,20,8,21],[10,12,10,13],[28,22,28,23],[27,0,27,2],[27,3,27,11],[27,12,27,13],[27,14,27,16],[27,17,27,19],[27,20,27,21],[27,22,27,23],[14,17,14,19],[14,14,14,16],[14,12,14,13],[14,3,14,11],[14,0,14,2],[26,22,26,23],[24,0,24,2],[24,3,24,11],[24,12,24,13],[24,14,24,16],[24,17,24,19],[24,20,24,21],[24,22,24,23],[20,0,20,2],[20,3,20,11],[20,12,20,13],[32,22,32,23],[32,24,32,27],[30,0,30,2],[30,3,30,11],[30,12,30,13],[30,14,30,16],[30,17,30,19],[30,20,30,21],[30,22,30,23],[30,24,30,27],[32,0,32,2],[32,3,32,11],[32,12,32,13],[32,14,32,16],[32,17,32,19],[32,20,32,21],[27,24,27,27],[31,0,31,2],[31,3,31,11],[31,12,31,13],[31,14,31,16],[31,17,31,19],[31,20,31,21],[31,22,31,23],[31,24,31,27],[29,0,29,2],[29,3,29,11],[29,12,29,13],[29,14,29,16],[29,17,29,19],[29,20,29,21],[29,22,29,23],[29,24,29,27],[28,24,28,27],[28,0,28,2],[28,3,28,11],[28,12,28,13],[28,14,28,16],[28,17,28,19],[28,20,28,21],[23,24,23,27],[26,24,26,27],[25,0,25,2],[25,3,25,11],[25,12,25,13],[25,14,25,16],[25,17,25,19],[25,20,25,21],[25,22,25,23],[25,24,25,27],[26,0,26,2],[26,3,26,11],[26,12,26,13],[26,14,26,16],[26,17,26,19],[26,20,26,21],[21,0,21,2],[21,3,21,11],[21,12,21,13],[21,14,21,16],[21,17,21,19],[21,20,21,21],[21,22,21,23],[21,24,21,27],[24,24,24,27],[22,0,22,2],[22,3,22,11],[22,12,22,13],[22,14,22,16],[22,17,22,19],[22,20,22,21],[22,22,22,23],[22,24,22,27],[23,0,23,2],[23,3,23,11],[23,12,23,13],[23,14,23,16],[23,17,23,19],[23,20,23,21],[23,22,23,23],[18,3,18,11],[18,12,18,13],[18,14,18,16],[18,17,18,19],[18,20,18,21],[18,22,18,23],[18,24,18,27],[20,14,20,16],[20,17,20,19],[20,20,20,21],[20,22,20,23],[20,24,20,27],[5,24,5,27],[9,0,9,2],[9,3,9,11],[9,12,9,13],[9,14,9,16],[9,17,9,19],[9,22,9,23],[9,24,9,27],[6,24,6,27],[6,22,6,23],[6,3,6,11],[6,0,6,2],[7,24,7,27],[7,0,7,2],[8,3,8,11],[8,12,8,13],[8,14,8,16],[8,17,8,19],[8,22,8,23],[9,20,9,21],[8,24,8,27],[19,0,19,2],[19,3,19,11],[19,12,19,13],[19,14,19,16],[19,17,19,19],[19,22,19,23],[10,24,10,27],[11,0,11,2],[11,3,11,11],[11,12,11,13],[10,22,10,23],[12,22,12,23],[12,24,12,27],[16,0,16,2],[16,3,16,11],[16,12,16,13],[16,14,16,16],[16,17,16,19],[10,0,10,2],[10,3,10,11],[10,14,10,16],[10,17,10,19],[15,17,15,19],[0,24,0,27],[1,0,1,27],[0,0,0,2],[0,3,0,11],[0,12,0,13],[0,14,0,16],[0,17,0,19],[0,22,0,23],[2,0,2,2],[2,3,2,11],[2,12,2,13],[2,14,2,16],[2,17,2,19],[2,22,2,23],[2,24,2,27],[0,20,0,21],[2,20,2,21],[4,3,4,11],[7,3,7,11],[7,12,7,13],[7,14,7,16],[7,17,7,19],[7,22,7,23],[8,0,8,2],[34,12,34,13],[34,0,34,2],[34,3,34,11],[34,14,34,16],[34,17,34,19],[34,20,34,21],[34,22,34,23],[4,17,4,19],[4,14,4,16],[4,12,4,13],[15,20,15,21],[10,20,10,21],[11,20,11,21],[12,20,12,21],[14,20,14,21],[17,0,17,2],[17,3,17,11],[34,24,34,27],[11,24,11,27],[19,24,19,27],[16,22,16,23],[16,24,16,27],[16,20,16,21],[13,0,13,2],[13,22,13,23],[13,24,13,27],[15,0,15,2],[15,22,15,23],[15,24,15,27],[13,3,13,11],[15,3,15,11],[15,12,15,13],[15,14,15,16],[11,14,11,16],[17,12,17,13],[17,14,17,16],[17,17,17,19],[17,20,17,21],[17,22,17,23],[17,24,17,27],[18,0,18,2],[37,0,37,2],[37,3,37,11],[37,12,37,13],[37,14,37,16],[37,17,37,19],[37,20,37,21],[37,22,37,23],[37,24,37,27],[35,0,35,2],[35,3,35,11],[35,12,35,13],[35,14,35,16],[35,17,35,19],[35,20,35,21],[35,22,35,23],[35,24,35,27],[36,0,36,2],[36,3,36,11],[36,12,36,13],[36,14,36,16],[36,17,36,19],[36,20,36,21],[36,22,36,23],[36,24,36,27]]}
["Parameter/Variable Name",null,null,"Description",{"$nulls":8},"Value Type",null,"Range",null,null,"Default Value",null,null,"Authority of CSU",null,"Authority of CCS",null,"Applied Model"]
["Common Information"]
["BatteryChargeType",null,null,"Battery charge type",{"$nulls":8},"uint8_t",null,"0x00: AC charging, 0x01: DC charging",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["PresentMsgFlowStatus",null,null,"PresentMsgFlowStatus",{"$nulls":8},"uint8_t",null,"0: Idle(wait B2 state), \n1: CM_SLAC_PARM.REQ, \n2: CM_SLAC_PARM.CNF, \n3: CM_START_ATTEN_CHAR.IND\n4: CM_MNBC_SOUND.IND, \n5: CM_ATTEN_CHAR.IND, \n6: CM_ATTEN_CHAR.RSP, \n7: CM_VALIDATE.REQ\n8: CM_VALIDATE.CNF, \n9: CM_SLAC_MATCH.REQ, \n10: CM_SLAC_MATCH.CNF, \n11: CM_AMP_MAP.REQ\n12: CM_AMP_MAP.CNF, \n13: SLACC/SDP/TCP connection,\n16: SupportedAppProtocolRequest, \n17: SupportedAppProtocolResponse, \n18: SessionSetupRequest\n19: SessionSetupResponse, \n20: ServiceDiscoveryRequest, \n21: ServiceDiscoveryResponse\n22: ServiceDetailRequest, \n23: ServiceDetailResponse\n24:ServiceAndPaymentSelectionRequest/ServiceSelectionRequest, \n25: ServiceAndPaymentSelectionResponse/ServiceSelectionResponse\n26: PaymentDetailsRequest/IdentificationDetailsRequest;, \n27: PaymentDetailsResponse/IdentificationDetailsResponse,\n28: AuthorizationRequest, \n29: AuthorizationResponse,\n30: CertificateUpdateRequest, \n31: CertificateUpdateResponse, \n32:CertificateInstallationRequest, \n33: CertificateInstallationResponse\n34: ChargeParameterDiscoveryRequest, \n35: ChargeParameterDiscoveryResponse\n36: CableCheckRequest, \n37: CableCheckResponse, \n38: PreChargeRequest, \n39: PreChargeResponse\n40: PowerDeliveryRequest start, \n41: PowerDeliveryResponse start, \n42: ChargingStatusRequest, \n43: ChargingStatusResponse\n44:CurrentDemandRequest, \n45:CurrentDemandResponse, \n46:MeteringReceiptRequest, \n47: MeteringReceiptResponse\n48: PowerDeliveryRequest end, \n49: PowerDeliveryRequest end, \n50: WeldingDetectionRequest, \n51: WeldingDetectionResponse,\n52: SessionStopRequest, \n53: SessionStopResponse\n253: Performance Timeout, \n254: Sequence Timeout, \n255: Fault",null,null,0,null,null,"RO",null,"R/W",null,"■AC Net □AC Eco □DC"]
["ChargingPermission",null,null,"Permission for the charging process",{"$nulls":8},"bool",null,"0x00: Not ready yet, stay in idle mode or go into terminating process.\n0x01: start charging process",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["ConnectorLockStatus ",null,null,"Connector lock status ",{"$nulls":8},"bool",null,"0x00: released\n0x01: locked ",null,null,0,null,null,"RO",null,"R/W",null,"■AC Net □AC Eco □DC"]
["ConnectorTemp1",null,null,"Connector temperature 1",{"$nulls":8},"float",null," unit: 1°C",null,null,0,null,null,"RO",null,"R/W",null,"■AC Net □AC Eco □DC"]
["ConnectorTemp2",null,null,"Connector temperature 2",{"$nulls":8},"float",null," unit: 1°C",null,null,0,null,null,"RO",null,"R/W",null,"■AC Net □AC Eco □DC"]
["ChargingRemainingTime",null,null,"charging remaining time",{"$nulls":8},"uint16_t",null," (0x0000: 0 sec ~ 0xFFFF: 65535 sec, resolution: 1 second)",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["Total Battery Capacity",null,null,"Total Battery Capacity",{"$nulls":8},"float",null,"unit: 1WH",null,null,0,null,null,"RO",null,"R/W",null,"■AC Net □AC Eco □DC"]
["BatteryMaximumVoltage",null,null,"Battery maximum voltage",{"$nulls":8},"float",null,"unit: 1V",null,null,0,null,null,"RO",null,"R/W",null,"■AC Net □AC Eco □DC"]
["BatteryMaximumCurrent",null,null,"Battery maximum current",{"$nulls":8},"float",null,"unit: 1A",null,null,0,null,null,"RO",null,"R/W",null,"■AC Net □AC Eco □DC"]
["EVCCID",null,null,"ID of EVCC",{"$nulls":8},"uint8_t*8",null,"12-Byte ASCII",null,null,0,null,null,"RO",null,"R/W",null,"■AC Net □AC Eco □DC"]
["EVSEID",null,null,"ID of EVSE",{"$nulls":8},"uint8_t*40",null,"40-Byte ASCII",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["CcsLibRev",null,null,"CCS library version",{"$nulls":8},"unit8_t*32",null,"32-Bytes ASCII",null,null,0,null,null,"RO",null,"R/W",null,"■AC Net □AC Eco □DC"]
["EVSEModelName",null,null,"EVSE Model Name",{"$nulls":8},"unit8_t*32",null,"32-Bytes ASCII",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["CsuAlarmStatusCode",null,null,"Stop charge event(alarm status )",{"$nulls":8},"uint32_t",null,"refer to \"Status Code Table.xlsx\"",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["CCSAlarmStatusCode",null,null,"Stop charge event(alarm status )",{"$nulls":8},"uint16_t",null,"refer to \"Status Code Table.xlsx\"",null,null,0,null,null,"RO",null,"R/W",null,"■AC Net □AC Eco □DC"]
["PaymentOptions",null,null,"Payment Options",{"$nulls":8},"uint8_t",null,"0x00: EIM\n0x01: PnC",null,null,0,null,null,"RO",null,"R/W",null,"■AC Net □AC Eco □DC"]
["EVSEMaxCurrent",null,null,"EVSE Maximum Current",{"$nulls":8},"float",null,"unit: 1A",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["EVSEMinCurrent",null,null,"EVSE Minimum Current",{"$nulls":8},"float",null,"unit: 1A",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["RCDStatus",null,null,"RCD Status",{"$nulls":8},"bool",null,"0x00: no error is detected\n0x01: an error is detected",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["GridVoltage[3]",null,null,"Grid Voltage (RMS value)",{"$nulls":8},"float",null,"unit: 1v",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["MeterID",null,null,"Meter ID",{"$nulls":8},"uint8_t*32",null,"32-Byte ASCII",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["MeterReading",null,null,"Meter Reading Value",{"$nulls":8},"float",null,"unit: 1WH",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["EVOperation",null,null,"EV Operation Mode",{"$nulls":8},"uint8_t",null,"0: Charge\n1: Discharge",null,null,0,null,null,"RO",null,"R/W",null,"■AC Net □AC Eco □DC"]
["EVChargeProgress",null,null,"EV Charge Progress",{"$nulls":8},"uint8_t",null,"0: Stop\n1: Start\n2: Renegotiate\n3: Standby ",null,null,0,null,null,"RO",null,"R/W",null,"■AC Net □AC Eco □DC"]
["CpSetPWMDuty",null,null,"Set CP PWM Duty",{"$nulls":8},"uint8_t",null,"unit: 1%\n0: 0%\n5: 5%\n100: 100%",null,null,0,null,null,"RO",null,"R/W",null,"■AC Net □AC Eco □DC"]
["CpSetStateE",null,null,"Set CP to State E",{"$nulls":8},"uint8_t",null,"0: DISABLE\n1: ENABLE",null,null,0,null,null,"RO",null,"R/W",null,"■AC Net □AC Eco □DC"]
["CpPresentPWMDuty",null,null,"CP Present PWM Duty",{"$nulls":8},"uint8_t",null,"unit: 1%",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["CpPresentState",null,null,"CP Present State",{"$nulls":8},"uint8_t",null,"1: A (12V, no PWM)\n2: B1 (9V, no PWM)\n3: B2 (9V, with PWM)\n4: C (6V, with PWM)\n5: D (3V, with PWM)\n6: E (0V, no PWM)\n7: F (-12V, no PWM)\n8: G (>12V)\n9: H  (<12V)",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["CpPositiveVoltage",null,null,"CP Present Voltage",{"$nulls":8},"float",null,"unit: 1V",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["CpNegativeVoltage",null,null,"CP Negative Voltage",{"$nulls":8},"float",null,"unit: 1V",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["CcsHeartBeat",null,null,"CCS process socket count",{"$nulls":8},"uint32_t",null,"unit: 1",null,null,0,null,null,"R/W",null,"R/W",null,"■AC Net □AC Eco □DC"]
["EVSEPresentCurrent[3]",null,null,"EVSE Present Current",{"$nulls":8},"float",null,"unit: 1A",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["OutputRelayStatus",null,null,"Output Relay Status",{"$nulls":8},"bool",null,"0: OFF\n1: ON",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["AvailableChargingPower",null,null,"EVSE Available Charging Power",{"$nulls":8},"float",null,"unit: 1KW",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]
["EVSENotification",null,null,"EVSE Notification",{"$nulls":8},"unit8",null,"0: None\n1: StopCharging\n2: ReNegotiation",null,null,0,null,null,"R/W",null,"RO",null,"■AC Net □AC Eco □DC"]