{"text_format":"2","workbook":"xlsx","n_sheets":7,"sheets":["Revision","Naming Rule","所有AC model name","所有DC model name","Customer Code Table","客戶碼","工作表1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Revision","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[[2,3,5,5]]}
[]
[]
[null,null,null,"PHIHONG EVSE Model Name Naming Rule"]
[]
[]
[]
[]
[null,null,"Revision History"]
[null,null,"Rev","Date","Description","Editor"]
[null,null,"01","2019/01/24","First issue","Vern Chang"]
[null,null,"02","2019/02/13","Second issue after discussion","Vern Chang"]
[null,null,"03","2019/03/25","Modify Naming Rule","Vincent Tsai"]
[null,null,"04","2019/05/16","1. Redefine:\n(a) DM : DC EVSE Moveable\n(b) DR : DC EVSE Roadside (Battery equipped)\n\n2. Correcting:\n(a) Ac => AC\n(b) Evse => EVSE","Joseph Chiu"]
[null,null,"05","2019/06/11","new item to connector type field","Vern Chang"]
[null,null,"06","2019/07/10","DC all models added","Audrey Chen"]
[null,null,"07","2019/09/04","DC standalone new models added","Audrey Chen"]
[null,null,"08","2019/11/05","DC standalone new models modified","Audrey Chen"]
[null,null,"09","2020/02/03","DC rack models added","Audrey Chen"]
[null,null,"10","2020/06/01","Naming rule add AC CCS2 plug","Folus Wen"]
[null,null,"11","2020/06/19","Naming rule add Type E socket","Audrey Chen"]
[null,null,"12","2020/06/15","1. Add \"D\" for Ethernet+WIFI+4G in \"network option\" field\n2. Create new sheet \"4G market matching table\" for the market of 4G application\n3. Add description in \"customization\" field","Vern Chang"]
[null,null,"13","2020/06/25","1. Add \"V\" for Liquid cooling CCS1 combo in \"Connector/Socket Type\" field\n2. Add \"F\" for Liquid cooling CCS2 combo in \"Connector/Socket Type\" field","John Ruan"]
[null,null,"14","2020/06/30","Type DR\" DC Evse Roadside: and \"Dc EVse Roadside (Battery equipped) (充電寶)\" were deleted and replaced by \"DC EVSE Power Rack\" (without cabinet)","Adason Tsai"]
[null,null,"15","2020/08/10","Naming rule add AC Meter (5 types)","Audrey Chen"]
[null,null,"16","2020/08/19","Add \"A\"  in \"network option\" field","John Ruan"]
[null,null,"17","2020/12/24","Add Name Rule \"AX\"  : Ac EVse Wall Mount excellent type\nCustomer Code Table: P0/P1","Vincent Tsai"]
[null,null,18,"2021/3/5","Add DK, DX for EVSE \nAdd T, D, K, M, N, P, R, C, W for gun ","Adason Tsai"]
[null,null,19,"2021-06-09","Add B for gun\nAdd command for U  (Suitable for REMA 200A, Amphenol 200A)","Jim Lee"]
[null,null,20,"2021-07-23","1.增加槍碼 H  WOER  GB 500A水冷\n2.增加槍碼A  WOER  GB 400A水冷","Vicki Lai"]
[null,null,21,"2021-09-16","1.取消P跟R Phoenix 500A水冷\n2. 將P碼給集電弓\n3. R碼給Phoenix CCS2 250A","Adason Tsai"]
[null,null,22,"2022-03-03","增加DH for CSU3.0簡易版","Adason Tsai"]
[null,null,23,"2022-04-06","1. 增加槍碼 Y: CCS1 150A\n2. 增加槍碼 Z: CCS2  150A","Eva Tsai"]
[null,null,24,"2022-04-14","增加槍碼S: CHAdeMO 125A Boost Mode","Clara Ou-Yang"]

{"sheet":"Naming Rule","index":1,"n_rows":106,"n_cols":61,"rows_kept":106,"cut":false,"hidden":false,"merged":[[24,21,34,27],[18,24,22,32],[1,5,1,7],[5,27,12,30],[65,10,78,27],[55,14,63,27],[36,17,53,27],[2,5,2,7],[105,3,117,27],[1,26,1,27],[2,26,2,27],[1,13,1,14],[2,13,2,14],[1,16,1,18],[2,16,2,18],[2,23,2,24],[1,23,1,24],[1,2,1,3],[2,2,2,3],[1,9,1,11],[2,9,2,11],[1,20,1,21],[2,20,2,21],[80,6,102,27]]}
[]
[null,null,"Type",null,null,"Input Configuration",null,null,null,"Safety Regulation",null,null,null,"Rated Power",null,null,"Connector/Socket Type",null,null,null,"Network Option",null,null,"Generation",null,null,"Customization"]
[null,null,"X X",null,null,"X",null,null,null,"X",null,null,null,"X1 X2 X3",null,null,"X1 X2 X3",null,null,null,"X",null,null,"X",null,null,"X X "]
{"$rows_empty":15}
[{"$nulls":24},"1  : Generation 1 (Phihong 標準RFID機種for AX)\n2  : Generation 2 (Contactless payment system機種for AX)\n3  : Generation 3 (Nayax 3in 1 payment system機種for AX)\n4  : Generation 4 (UIC 3in 1 payment system機種for AX)"]
[]
[]
[]
[]
[]
[{"$nulls":21},"0  : None\nE  : Ethernet only\nB  : Bluetooth only\nW : Ethernet + WiFi\nT   : Ethernet + 4G\nU  : Ethernet + Bluetooth\nD  : Ethernet + WiFi + 4G\nA  : Ethernet + WiFi external antenna +\n      4G                                                                 F  : WiFi only"]
{"$rows_empty":11}
[{"$nulls":17},"X1X2X3 = Connector/Socket 1, 2 and 3 from left to right\n\n0 : none\n1 : IEC 62196-2 Type 1/SAE J1772 Plug\n2 : IEC 62196-2 Type 1/SAE J1772 Socket\n3 : IEC 62196-2 Type 2 Plug\n4 : IEC 62196-2 Type 2 Socket\n5 : GB/T AC Plug\n6 : GB/T AC Socket\n7：CCS2 AC Plug\n8：Type E socket\nJ : CHAdeMO\nU : Natural cooling CCS1 combo (Suitable for REMA 200A, Amphenol 200A)\nV : Liquid cooling CCS1 combo\nE : Natural cooling CCS2 combo\nF : Liquid cooling CCS2 combo\nG : GBT DC\nT: Rema CCS1 300A\nD: Rema CCS2 300A\nK: CHadeMO 200A\nM: CCS2 80A\nN: CCS1 80A\nP: 集電弓\nR: Phoenix 250A氣冷\nC: Reserved for ChaoJi\nW: Reserved for Wireless\nB: GBT YG PT1000\nH: WOER GBT 500A\nA:WOER GBT 400A\nL: CHAdeMO 80A\nY: CCS1 150A\nZ: CCS2  150A\nS: CHAdeMO 125A Boost Mode\nNOTES1: 槍線配置AC由右到左依序排列，DC由左到右依序排列\n\ne.g., \n1JU : SAE J1772 plug + CHAdeMO + CCS1",{"$nulls":42},"ssssss"]
{"$rows_empty":18}
[{"$nulls":14},"X1X2X3 = (X1 x 10 + X2) x 10^(-1+X3)  kW\ne.g., \n190 : 1.9 kW (AC 120V with 16A)\n380 : 3.8 kW (AC 120V with 32A)\n350 : 3.5 kW (AC 220V with 16A)\n700 : 7 kW (AC 220V with 32A)\n251 : 25 kW \n301 : 30 kW\n362 : 360 kW"]
[]
[]
[]
[]
[]
[{"$nulls":50},"s"]
[]
[]
[]
[{"$nulls":10},"E  : CE / European Market\nU  : UL / North America Market\nG : GB / China Market\nC  : CNS / Taiwan Market\nJ   : JARI / Japan Market\nT   : TR25 / Singapor Market\nK  : KC / Korea Market\nB  : British / UK Market\nZ   : EV ready / French Market\nM : E + MID Meter\nP  : E + PTB certification\nI   : Z + TIC Meter pcb\nF  : Z + MID Meter\nL  : U + UL meter"]
{"$rows_empty":14}
[{"$nulls":6},"Y : 3 phase wyi-connection 4 wires + PE, 380 - 415Vac, 50Hz/60Hz\nD : 3 phase delta-connection 3 wires + PE, 200 - 240Vac, 50Hz/60Hz\nL :  2 phase 2 wires + PE, 200 - 240Vac, 50Hz/60Hz\nS : 1 phase 2 wires + PE, 220 - 240Vac, 50Hz/60Hz\nW : 3 phase wyi-connection 4 wires + PE, 380 - 480Vac, 50Hz/60Hz\nT : 1 phase 2 wires + PE, 220 - 277Vac, 50Hz/60Hz\nE : 1 Phase 2 wires + PE, 100 - 120Vac, 50Hz/60Hz\nAC Plug Type: (AC 輸入線 - 帶插頭型式)\n0 : 1 phase 2 wires + PE, CEE 7/7 plug (compatible with Type E and Type F), 220 - 240Vac, 50Hz/60Hz. (For European)\n1 : 1 phase 2 wires + PE, BS 1363 plug (Type G), 220 - 240Vac, 50Hz/60Hz. (For UK)\n2 : 1 phase 2 wires + PE, AS/NZS 3112 (Type I), 220 - 240Vac, 50Hz/60Hz. (For Australia, New Zealand)\n3 : 1 phase 2 wires + PE, GB 2099.1‐2008 and GB 1002‐2008 (Type I), 220 - 240Vac, 50Hz/60Hz. (For China)\n4 : 1 phase 2 wires + PE, IS1293 plug (Type M), 220 - 240Vac, 50Hz/60Hz. (For Indian and South African)\n5 : 2 phase 2 wires + PE, NEMA 5-15 plug (Type B), 120 Vac, 50Hz/60Hz.(For UL, TW, Japan)\n6 : 2 phase 2 wires + PE, NEMA 6-20 plug, 200 - 240Vac, 50Hz/60Hz. (For UL, TW)\n7 : 2 phase 2 wires + PE, NEMA 14-30 plug, 120 - 240Vac, 50Hz/60Hz. (For UL)\n8 : 2 phase 2 wires + PE, NEMA 14-50 plug, 120 - 240Vac, 50Hz/60Hz. (For UL)\n9 :  2 phase 2 wires + PE, NEMA 6-50 plug, 200 - 240Vac, 50Hz/60Hz. (For UL, TW)                                                                                                              A : 2 phase 2 wires + PE, NEMA 14-60 plug, 200 - 240Vac, 50Hz/60Hz. (For UL)       "]
{"$rows_empty":24}
[null,null,null,"AC : Ac EVse Cordset \nAW : Ac EVse Wallmount\nAP  : Ac EVse Pedestal\nAX  : Ac EVse Wall Mount excellent type\nDW : Dc EVse Wallmount\nDS   : Dc EVse Standalone\nDM : Dc EVse Moveable (移動)  \nDR  : Dc EVse Power Rack (without cabinet)\nDD : Dc EVse Dispenser\nDO : Dc EVse Output power cabinet\nDQ : Dc EVse Infy 30KW GB module \nDK: DC EVSE Power Rack\nDX: DC EVSE Output Communication Box (Dispenser)\nDB: Dc to Dc EVSE Output power cabinet\nDH: CSU3.0 簡易版\n"]

{"sheet":"所有AC model name","index":2,"n_rows":139,"n_cols":20,"rows_kept":139,"cut":false,"hidden":false,"merged":[[4,12,4,14],[4,17,4,18],[5,5,5,6],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,4,6],[4,9,4,11]]}
[]
[]
[null,"AC Charger Model Name List"]
[]
[null,"Item \nNo","Established\nDate","Customer","Description","Type",null,"Input \nConfiguration","Safety \nRegulation","Rated Power",null,null,"Connector/\nSocket Type",null,null,"Network \nOption","Generation","Customization",null,"-RW"]
[{"$nulls":5},"X1 X2",null,"X3","X4","X5","X6","X7","X8","X9","X10","X11","X12","X13","X14"]
[null,1,"2019-03-24","飛宏","美規基礎版","A","W","L","U",7,7,0,0,0,1,0,1,"P",0,"-RW"]
[null,2,"2019-03-24","飛宏","美規連網版","A","W","L","U",7,7,0,0,0,1,"E",2,"P",0,"-RW"]
[null,3,"2019-03-24","飛宏","美規WI-FI版","A","W","L","U",7,7,0,0,0,1,"W",2,"P",0,"-RW"]
[null,4,"2019-03-24","飛宏","美規4G版","A","W","L","U",7,7,0,0,0,1,"T",2,"P",0,"-RW"]
[null,5,"2020-04-25","拓連","美規WI-FI版白色","A","W","L","U",7,7,0,0,0,1,"W",2,"N",0,"-RW"]
[null,6,"2020-04-25","拓連","美規WI-FI版銀色","A","W","L","U",7,7,0,0,0,1,"W",2,"N",1,"-RW"]
[null,7,"2020-04-25","拓連","美規4G版白色","A","W","L","U",7,7,0,0,0,1,"T",2,"N",0,"-RW"]
[null,8,"2020-04-25","拓連","美規4G版銀色","A","W","L","U",7,7,0,0,0,1,"T",2,"N",1,"-RW"]
[null,9,"2020-03-24","大綠","美規基礎版14-50","A","W",8,"U",7,7,0,0,0,1,0,1,"G",0,"-RW"]
[null,10,"2020-03-24","大綠","美規基礎版6-50","A","W",9,"U",7,7,0,0,0,1,0,1,"G",0,"-RW"]
[null,11,"2019-05-14","飛宏","陸規基礎版","A","W","S","G",7,7,0,0,0,5,0,1,"P",0,"-RW"]
[null,12,"2019-05-14","飛宏","陸規連網版","A","W","S","G",7,7,0,0,0,5,"E",1,"P",0,"-RW"]
[null,13,"2019-05-14","飛宏","陸規WI-FI版","A","W","S","G",7,7,0,0,0,5,"W",1,"P",0,"-RW"]
[null,14,"2019-05-14","飛宏","陸規4G版","A","W","S","G",7,7,0,0,0,5,"T",1,"P",0,"-RW"]
[null,15,"2019-05-14","拜騰","陸規藍芽基礎版","A","W","S","G",7,7,0,0,0,5,"B",1,"B",0,"-RW"]
[null,16,"2019-05-14","拜騰","陸規藍芽4G版","A","W","S","G",7,7,0,0,0,5,"T",1,"B",0,"-RW"]
[null,17,"2019-03-24","飛宏","歐規基礎版","A","W","S","E",7,7,0,0,0,3,0,1,"P",0,"-RW"]
[null,18,"2019-03-24","飛宏","歐規連網版","A","W","S","E",7,7,0,0,0,3,"E",2,"P",0,"-RW"]
[null,19,"2019-03-24","飛宏","歐規WI-FI版","A","W","S","E",7,7,0,0,0,3,"W",2,"P",0,"-RW"]
[null,20,"2019-03-24","飛宏","歐規4G版","A","W","S","E",7,7,0,0,0,3,"T",2,"P",0,"-RW"]
[null,21,"2019-10-18","飛宏","日規基礎版","A","W","S","J",6,0,0,0,0,1,0,1,"P",0,"-RW"]
[null,22,"2019-10-18","飛宏","日規連網版","A","W","S","J",6,0,0,0,0,1,"E",1,"P",0,"-RW"]
[null,23,"2019-10-18","飛宏","日規WI-FI版","A","W","S","J",6,0,0,0,0,1,"W",1,"P",0,"-RW"]
[null,24,"2019-10-18","飛宏","日規4G版","A","W","S","J",6,0,0,0,0,1,"T",1,"P",0,"-RW"]
[null,25,"2019-12-01","飛宏","台規基礎版","A","W","S","C",7,7,0,0,0,1,0,1,"P",0,"-RW"]
[null,26,"2019-12-01","飛宏","台規連網版","A","W","S","C",7,7,0,0,0,1,"E",1,"P",0,"-RW"]
[null,27,"2019-12-01","飛宏","台規WI-FI版","A","W","S","C",7,7,0,0,0,1,"W",1,"P",0,"-RW"]
[null,28,"2019-12-01","飛宏","台規4G版","A","W","S","C",7,7,0,0,0,1,"T",1,"P",0,"-RW"]
[null,29,"2019-12-01","拓連","台規WI-FI版白色","A","W","S","C",7,7,0,0,0,1,"W",1,"N",0,"-RW"]
[null,30,"2019-12-01","拓連","台規WI-FI版銀色","A","W","S","C",7,7,0,0,0,1,"W",1,"N",1,"-RW"]
[null,31,"2020-10-27","飛宏","美規基礎版14-50","A","W",8,"U",7,7,0,0,0,1,0,1,"P",0,"-RW"]
[null,32,"2020-10-27","飛宏","美規基礎版6-50","A","W",9,"U",7,7,0,0,0,1,0,1,"P",0,"-RW"]
[null,33,"2020-10-29","Zenobe","歐規AP63連網版_43KW*2","E","A",8,7,3,"E",3,"E","F",8,"Z","B",2,null,"-RW"]
[null,34,"2020-11-06","拓連","台規WI-FI版銀色Volvo絲印","A","W","S","C",7,7,0,0,0,1,"W",1,"N",2,"-RW"]
[null,35,"2020-11-30","飛宏","新加坡基礎版","A","W","S","T",7,7,0,0,0,3,0,1,"P",0,"-RW"]
[null,36,"2020-11-30","飛宏","新加坡連網版","A","W","S","T",7,7,0,0,0,3,"E",2,"P",0,"-RW"]
[null,37,"2020-11-30","飛宏","新加坡WiFi版","A","W","S","T",7,7,0,0,0,3,"W",2,"P",0,"-RW"]
[null,38,"2020-11-30","飛宏","新加坡4G版","A","W","S","T",7,7,0,0,0,3,"T",2,"P",0,"-RW"]
[null,39,"2020-12-24","飛宏","美規48A基礎版WiFi版無螢幕","A","X","L","U",1,1,0,0,0,1,"W",1,"P",0,"-RW"]
[null,40,"2020-12-24","飛宏","美規48A基礎版4G版無螢幕","A","X","L","U",1,1,0,0,0,1,"D",1,"P",0,"-RW"]
[null,41,"2020-12-24","飛宏","美規48高階版WiFi版帶螢幕","A","X","L","U",1,1,0,0,0,1,"W",1,"P",1,"-RW"]
[null,42,"2020-12-24","飛宏","美規48高階版4G版帶螢幕","A","X","L","U",1,1,0,0,0,1,"D",1,"P",1,"-RW"]
[null,43,"2020-12-24","飛宏","美規48A高階版4G版帶螢幕\nContactless Payment System","A","X","L","U",1,1,0,0,0,1,"D",2,"P",1,"-RW"]
[null,44,"2020-12-24","飛宏","美規48A高階版4G版帶螢幕\nNayax Payment System","A","X","L","U",1,1,0,0,0,1,"D",3,"P",1,"-RW"]
[null,45,"2020-12-24","飛宏","美規48A高階版4G版帶螢幕\nUIC Payment System","A","X","L","U",1,1,0,0,0,1,"D",4,"P",1,"-RW"]
[null,46,"2021-01-20","飛宏","美規基礎版無Logo","A","W","L","U",7,7,0,0,0,1,0,1,"P",1,"-RW"]
[null,47,"2021-01-20","飛宏","美規連網版無Logo","A","W","L","U",7,7,0,0,0,1,"E",2,"P",1,"-RW"]
[null,48,"2021-01-20","飛宏","美規WI-FI版無Logo","A","W","L","U",7,7,0,0,0,1,"W",2,"P",1,"-RW"]
[null,49,"2021-01-20","飛宏","美規4G版無Logo","A","W","L","U",7,7,0,0,0,1,"T",2,"P",1,"-RW"]
[null,50,"2021-01-20","飛宏","美規基礎版14-50無Logo","A","W",8,"U",7,7,0,0,0,1,0,1,"P",1,"-RW"]
[null,51,"2021-01-20","飛宏","美規基礎版6-50無Logo","A","W",9,"U",7,7,0,0,0,1,0,1,"P",1,"-RW"]
[null,52,"2021-02-19","UB","美規基礎版6-50 Bosch版","A","W",9,"U",7,7,0,0,0,1,0,1,"C",0,"-RW"]
[null,53,"2021-03-08","UB","美規基礎版14-50 Bosch版","A","W",8,"U",7,7,0,0,0,1,0,1,"C",0,"-RW"]
[null,54,"2021-03-08","UB","美規基礎版wifi Bosch版","A","W","L","U",7,7,0,0,0,1,"W",2,"C",0,"-RW"]
[null,55,"2021-03-18","Lewden","歐規基礎版 Lewden","A","W","S","E",7,7,0,0,0,3,0,1,"L",0,"-RW"]
[null,56,"2021-03-18","Lewden","歐規WIFI版 Lewden","A","W","S","E",7,7,0,0,0,3,"W",2,"L",0,"-RW"]
[null,57,"2021-03-24","charge lab","美規無Logo charge lab 聯網版本","A","W","L","U",7,7,0,0,0,1,"E",2,"A",0,"-RW"]
[null,58,"2021-03-24","charge lab","美規無Logo charge lab WIFI版本","A","W","L","U",7,7,0,0,0,1,"W",2,"A",0,"-RW"]
[null,59,"2021-03-24","charge lab","美規無Logo charge lab 4G版本","A","W","L","U",7,7,0,0,0,1,"T",2,"A",0,"-RW"]
[null,60,"2021-05-14","拓連","歐規WI-FI版銀色面蓋 泰文說明書","A","W","S","E",7,7,0,0,0,3,"W",2,"N",1,"-RW"]
[null,61,"2021-05-14","車麻吉","台規WI-FI版皮卡充面蓋","A","W","S","C",7,7,0,0,0,1,"W",1,"M",0,"-RW"]
[null,62,"2021-05-14","拓連","歐規WI-FI版銀色面蓋 英文說明書","A","W","S","E",7,7,0,0,0,3,"W",2,"N",2,"-RW"]
[null,63,"2021-10-14","飛宏","台規基礎版無Logo","A","W","S","C",7,7,0,0,0,1,0,1,"P",1,"-RW"]
[null,64,"2021-10-14","飛宏","台規連網版無Logo","A","W","S","C",7,7,0,0,0,1,"E",1,"P",1,"-RW"]
[null,65,"2021-10-14","飛宏","台規WiFi版無Logo","A","W","S","C",7,7,0,0,0,1,"W",1,"P",1,"-RW"]
[null,66,"2021-10-14","飛宏","台規4G版無Logo","A","W","S","C",7,7,0,0,0,1,"T",1,"P",1,"-RW"]
[null,67,"2021-10-14","飛宏","歐規基礎版無Logo","A","W","S","E",7,7,0,0,0,3,0,1,"P",1,"-RW"]
[null,68,"2021-10-14","飛宏","歐規連網版無Logo","A","W","S","E",7,7,0,0,0,3,"E",2,"P",1,"-RW"]
[null,69,"2021-10-14","飛宏","歐規WiFi版無Logo","A","W","S","E",7,7,0,0,0,3,"W",2,"P",1,"-RW"]
[null,70,"2021-10-14","飛宏","歐規4G版無Logo","A","W","S","E",7,7,0,0,0,3,"T",2,"P",1,"-RW"]
[null,71,"2021-10-19","飛宏","美規基礎版無Logo 7.5米槍","A","W","L","U",7,7,0,0,0,1,0,1,"P",2,"-RW"]
[null,72,"2021-10-19","飛宏","美規連網版無Logo 7.5米槍","A","W","L","U",7,7,0,0,0,1,"E",2,"P",2,"-RW"]
[null,73,"2021-10-19","飛宏","美規WiFi版無Logo 7.5米槍","A","W","L","U",7,7,0,0,0,1,"W",2,"P",2,"-RW"]
[null,74,"2021-10-19","飛宏","美規4G版無Logo 7.5米槍","A","W","L","U",7,7,0,0,0,1,"T",2,"P",2,"-RW"]
[null,75,"2021-11-22","TOG","TOG客製化 基礎版本","A","W","L","U",7,7,0,0,0,1,0,1,"T",1,"-RW"]
[null,76,"2021-11-22","TOG","TOG客製化 WiFi版本","A","W","L","U",7,7,0,0,0,1,"W",2,"T",1,"-RW"]
[null,77,"2021-11-22","TOG","TOG客製化 4G版本","A","W","L","U",7,7,0,0,0,1,"T",2,"T",1,"-RW"]
[null,78,"2021-11-22","PHA Shell","美規殼牌客製化4G版","A","W","L","U",7,7,0,0,0,1,"T",2,"Ｏ",1,"-RW"]
[null,79,"2021-11-22","PHA Shell","美規殼牌客製化4G版 7.5米槍線","A","W","L","U",7,7,0,0,0,1,"T",2,"Ｏ",2,"-RW"]
[null,80,"2021-11-24","TOG","TOG客製化 WiFi版本","A","X","L","U",1,1,1,0,0,1,"W",1,"T",1,"-RW"]
[null,81,"2021-11-24","TOG","TOG客製化 4G版本","A","X","L","U",1,1,1,0,0,1,"D",1,"T",1,"-RW"]
[null,82,"2021-11-29","PHEU Shell","Shell EU 基礎版","A","W","S","E",7,7,0,0,0,3,0,1,"O",1,"-RW"]
[null,83,"2021-11-29","PHEU Shell","Shell EU 連網版","A","W","S","E",7,7,0,0,0,3,"E",2,"O",1,"-RW"]
[null,84,"2021-11-29","PHEU Shell","Shell EU WiFi版","A","W","S","E",7,7,0,0,0,3,"W",2,"O",1,"-RW"]
[null,85,"2021-11-29","PHEU Shell","Shell EU 4G版","A","W","S","E",7,7,0,0,0,3,"T",2,"O",1,"-RW"]
[null,86,"2021-12-28","拓連","拓連客製化 WiFi版本","A","X","S","C",1,1,1,0,0,1,"W",1,"N",1,"-RW"]
[null,87,"2021-12-28","飛宏","台規48高階WiFi版帶螢幕","A","X","S","C",1,1,1,0,0,1,"W",1,"P",1,"-RW"]
[null,88,"2021-12-28","飛宏","歐規三相32基礎WiFi版無螢幕槍線版","A","X","Y","E",2,2,1,0,0,3,"W",1,"P",0,"-RW"]
[null,89,"2021-12-28","飛宏","歐規三相32基礎WiFi版無螢幕母座版","A","X","Y","E",2,2,1,0,0,4,"W",1,"P",0,"-RW"]
[null,90,"2021-12-28","飛宏","歐規三相32高階WiFi+4G版+MID電表帶螢幕槍線版","A","X","Y","M",2,2,1,0,0,3,"D",1,"P",0,"-RW"]
[null,91,"2021-12-28","飛宏","歐規三相32高階WiFi+4G版+MID電表帶螢幕母座版","A","X","Y","M",2,2,1,0,0,4,"D",1,"P",0,"-RW"]
[null,92,"2021-12-28","飛宏","歐規三相32法國高階WiFi+4G版+MID電表帶螢幕TypeE槍線版","A","X","Y","M",2,2,1,0,0,3,"D",2,"P",0,"-RW"]
[null,93,"2021-12-28","飛宏","歐規三相32法國高階WiFi+4G版+MID電表帶螢幕TypeE母座版","A","X","Y","M",2,2,1,0,0,4,"D",2,"P",0,"-RW"]
[null,94,"2022-01-14","PHA Shell","Shell美規48A基礎版WiFi版無螢幕","A","X","L","U",1,1,1,0,0,1,"W",1,"O",0,"-RW"]
[null,95,"2022-01-14","PHA Shell","Shell美規48A基礎版4G版無螢幕","A","X","L","U",1,1,1,0,0,1,"D",1,"O",0,"-RW"]
[null,96,"2022-01-14","PHA Shell","Shell美規48高階版WiFi版帶螢幕","A","X","L","U",1,1,1,0,0,1,"W",1,"O",1,"-RW"]
[null,97,"2022-01-14","PHA Shell","Shell美規48高階版4G版帶螢幕","A","X","L","U",1,1,1,0,0,1,"D",1,"O",1,"-RW"]
[null,98,"2022-01-14","飛宏","美規48A基礎版WiFi版無螢幕_7m槍線","A","X","L","U",1,1,1,0,0,1,"W",1,"P",3,"-RW"]
[null,99,"2022-01-14","飛宏","美規48A基礎版4G版無螢幕_7m槍線","A","X","L","U",1,1,1,0,0,1,"D",1,"P",3,"-RW"]
[null,100,"2022-01-14","飛宏","美規48高階版WiFi版帶螢幕_7m槍線","A","X","L","U",1,1,1,0,0,1,"W",1,"P",4,"-RW"]
[null,101,"2022-01-14","飛宏","美規48高階版4G版帶螢幕_7m槍線","A","X","L","U",1,1,1,0,0,1,"D",1,"P",4,"-RW"]
[null,102,"2022-02-22","WAT","歐規三相32基礎WiFi版無螢幕槍線版 WAT印刷","A","X","Y","E",2,2,1,0,0,3,"W",1,"Ｗ",0,"-RW"]
[null,103,"2022-02-22","WAT","歐規三相32基礎WiFi版無螢幕槍線版 Ford印刷","A","X","Y","E",2,2,1,0,0,3,"W",1,"Ｗ",2,"-RW"]
[null,104,"2022-02-22","WAT","歐規基礎版WAT印刷","A","W","S","E",7,7,0,0,0,3,0,1,"W",0,"-RW"]
[null,105,"2022-02-22","WAT","歐規聯網版WAT印刷","A","W","S","E",7,7,0,0,0,3,"E",2,"W",0,"-RW"]
[null,106,"2022-02-22","WAT","歐規WiFi版WAT印刷","A","W","S","E",7,7,0,0,0,3,"W",2,"W",0,"-RW"]
[null,107,"2022-02-22","WAT","歐規4G版WAT印刷","A","W","S","E",7,7,0,0,0,3,"T",2,"W",0,"-RW"]
[null,108,"2022-02-22","Noodoe","美規Wifi連網版 拓連標準白額頭","A","X","L","U",1,1,1,0,0,1,"W",1,"N",4,"-RW"]
[null,109,"2022-02-22","WAT","歐規三相32A槍線版 WAT印刷 連網版","E","A",4,4,3,"E",3,"E","F",8,"W",2,null,null,"-RW"]
[null,110,"2022-03-10","飛宏","歐規32A三相五線歐規雙母座+RFID+RCD TYPE B+WiFi","E","A",4,4,2,"E",3,"E","F",3,"P",2,null,null,"-RW"]
[null,111,"2022-03-10","飛宏","歐規32A三相五線歐規雙槍線+RFID+RCD TYPE B+WiFi","E","A",4,4,3,"E",3,"E","F",3,"P",2,null,null,"-RW"]
[null,112,"2022-03-10","飛宏","歐規63A三相五線歐規雙槍線+RFID+RCD TYPE B+WiFi","E","A",8,7,3,"E",3,"E","F",3,"P",2,null,null,"-RW"]
[null,113,"2022-03-11","PHEU Shell","Shell EU 基礎版 7M","A","W","S","E",7,7,0,0,0,3,0,1,"O",2,"-RW"]
[null,114,"2022-03-11","PHEU Shell","Shell EU 連網版 7M","A","W","S","E",7,7,0,0,0,3,"E",2,"O",2,"-RW"]
[null,115,"2022-03-11","PHEU Shell","Shell EU WiFi版 7M","A","W","S","E",7,7,0,0,0,3,"W",2,"O",2,"-RW"]
[null,116,"2022-03-11","PHEU Shell","Shell EU 4G版 7M","A","W","S","E",7,7,0,0,0,3,"T",2,"O",2,"-RW"]
[null,117,"2022-03-17","WAT","歐規三相32 高階WiFi+4G版+MID電表帶螢幕槍線版 WAT印刷","A","X","Y","M",2,2,1,0,0,3,"D",1,"W",0,"-RW"]
[null,118,"2022-03-17","PHEU Shell","歐規三相32基礎WiFi版無螢幕槍線版 7M","A","A","A","A","A","A","A","A","A","A","A","A","A","A","-RW"]
[null,119,"2022-03-17","PHEU Shell","歐規三相32基礎WiFi版無螢幕母座版 7M","A","A","A","A","A","A","A","A","A","A","A","A","A","A","-RW"]
[null,120,"2022-03-17","PHEU Shell","歐規三相32 高階WiFi+4G版+MID電表帶螢幕槍線版 7M","A","A","A","A","A","A","A","A","A","A","A","A","A","A","-RW"]
[null,121,"2022-03-17","PHEU Shell","歐規三相32 高階WiFi+4G版+MID電表帶螢幕母座版 7M","A","A","A","A","A","A","A","A","A","A","A","A","A","A","-RW"]
[null,122,"2022-03-17","PHEU Shell","歐規三相32高階WiFi+4G版+MID電表帶螢幕TypeE槍線版 7M","A","A","A","A","A","A","A","A","A","A","A","A","A","A","-RW"]
[null,123,"2022-03-17","PHEU Shell","歐規三相32高階WiFi+4G版+MID電表帶螢幕TypeE母座版 7M","A","A","A","A","A","A","A","A","A","A","A","A","A","A","-RW"]
[null,124,"2022-03-29","飛宏","歐規63A三相五線歐規雙槍線+RFID+RCD TYPE B + WiFi 7.5M","E","A",8,7,3,"E",3,"E","F",3,"P",5,null,null,"-RW"]
[null,125,"2022-03-29","飛宏","歐規63A三相五線歐規雙槍線+RFID+RCD TYPE B + 4G 7.5M","E","A",8,7,3,"E",3,"E","F",5,"P",5,null,null,"-RW"]
[null,126,"2022-03-29","飛宏","歐規63A三相五線歐規雙槍線+RFID+RCD TYPE B + Lan 7.5M","E","A",8,7,3,"E",3,"E","F",8,"P",5,null,null,"-RW"]
[null,127,"2022-04-27","飛宏","日規16A纜線盒 OTP版 ITT PSE 20A 日規AC Cord","E","A",3,5,2,"A",1,"J","M",1,"P",2,null,null,"-RW"]
[null,128,"2022-04-27","飛宏","日規16A纜線盒 大綠無包材版  ITT PSE 20A 日規AC Cord","E","A",3,5,2,"A",1,"J","M",1,"P",1,null,null,"-RW"]
[null,129,"2022-04-28","Noodoe","美規Wifi連網版 拓連標準黑額頭","A","X","L","U",1,1,1,0,0,1,"W",1,"N",2,"-RW"]
[null,130,"2022-04-28","Noodoe","美規4G+Wifi連網版 拓連標準黑額頭","A","X","L","U",1,1,1,0,0,1,"D",1,"N",2,"-RW"]
[null,131,"2022-06-09","Encgarging","日規4G版 客製化版本","A","W","S","J",6,0,0,0,0,1,"T",1,"E",0,"-RW"]
[null,132,"2022-06-16","SWTCH","美規AX48 WiFi版 客製化前面蓋印刷Logo ","A","X","L","U",1,1,1,0,0,1,"W",1,"S",1,"-RW"]
[null,133,"2022-06-16","SWTCH","美規AX48 4G版 客製化前面蓋印刷Logo ","A","X","L","U",1,1,1,0,0,1,"D",1,"S",1,"-RW"]

{"sheet":"所有DC model name","index":3,"n_rows":318,"n_cols":21,"rows_kept":318,"cut":false,"hidden":false,"merged":[[5,1,5,4],[3,9,3,11],[3,12,3,14],[58,17,58,18],[220,20,227,20],[3,17,3,18],[3,1,4,1],[3,2,4,2],[3,4,4,4],[3,3,4,3],[4,5,4,6],[3,5,3,6],[285,1,285,4],[290,1,290,4],[228,20,229,20],[59,17,59,18],[139,1,139,4]]}
[]
[null,"DC Charger Model Name List"]
[]
[null,"Item \nNo","Established\nDate","Customer","Description","Type",null,"Input \nConfiguration","Safety \nRegulation","Rated Power",null,null,"Connector/\nSocket Type",null,null,"Network \nOption","Generation","Customization",null,"-RW","請備註客製化或特殊需求"]
[{"$nulls":5},"X1 X2",null,"X3","X4","X5","X6","X7","X8","X9","X10","X11","X12","X13","X14"]
[null,"Standalone"]
[null,null,"2019-02-20","Phihong","60KW 黑白機 F-750 CSU2.0_CE","D","S","Y","E",6,0,1,"J",0,"E","T",1,"P","H","-RW"]
[null,null,"2019-07-10","Phihong","60KW 黑白機 F-750U CSU2.0_UL","D","S","W","U",6,0,1,"J",0,"U","T",1,"P","H","-RW"]
[]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_CE","D","S","Y","E",6,0,1,"J",4,"U","E",2,"P","H","-RW"]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_CE","D","S","Y","E",6,0,1,"J",4,"U","W",2,"P","H","-RW"]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_CE","D","S","Y","E",6,0,1,"J",4,"U","T",2,"P","H","-RW"]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_CE","D","S","Y","E",6,0,1,"J",4,"E","E",2,"P","H","-RW"]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_CE","D","S","Y","E",6,0,1,"J",4,"E","W",2,"P","H","-RW"]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_CE","D","S","Y","E",6,0,1,"J",4,"E","T",2,"P","H","-RW"]
[]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_UL","D","S","W","E",6,0,1,"J",1,"U","E",2,"P","H","-RW"]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_UL","D","S","W","E",6,0,1,"J",1,"U","W",2,"P","H","-RW"]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_UL","D","S","W","E",6,0,1,"J",1,"U","T",2,"P","H","-RW"]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_UL","D","S","W","E",6,0,1,"J",1,"E","E",2,"P","H","-RW"]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_UL","D","S","W","E",6,0,1,"J",1,"E","W",2,"P","H","-RW"]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_UL","D","S","W","E",6,0,1,"J",1,"E","T",2,"P","H","-RW"]
[]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_UL","D","S","W","U",6,0,1,"J",1,"U","E",2,"P","H","-RW"]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_UL","D","S","W","U",6,0,1,"J",1,"U","W",2,"P","H","-RW"]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_UL","D","S","W","U",6,0,1,"J",1,"U","T",2,"P","H","-RW"]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_UL","D","S","W","U",6,0,1,"J",1,"E","E",2,"P","H","-RW"]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_UL","D","S","W","U",6,0,1,"J",1,"E","W",2,"P","H","-RW"]
[null,null,"2019-11-06","Phihong","60KW立柱 Infy PSU CSU3.0_UL","D","S","W","U",6,0,1,"J",1,"E","T",2,"P","H","-RW"]
[]
[null,null,"2019-11-26","Phihong","60KW立柱 Infy PSU CSU3.0_CE","D","S","Y","E",6,0,1,"J",0,"E","T",2,"P","H","-RW"]
[null,null,"2019-11-26","Phihong","60KW立柱 Infy PSU CSU3.0_UL","D","S","W","U",6,0,1,"J",0,"U","T",2,"P","H","-RW"]
[]
[null,null,"2019-05-28","沙崙瑞助","30KW 黑白機 F-750","D","S","Y","C",3,0,1,"J",0,"U","E",1,"P","H","-RW"]
[]
[]
[null,null,"2019-05-28","Plugit","180KW Plugit Power Rack F-750","D","S","Y","E",1,8,2,"E",0,"G",0,1,"L",0,"-RW"]
[null,null,"2019-05-28","Plugit","210KW Plugit Power Rack F-750","D","S","Y","E",2,1,2,"E",0,"G",0,1,"L",0,"-RW"]
[null,null,"2019-05-28","Plugit","210KW Plugit Power Rack F-750","D","S","Y","E",2,1,2,"G",0,"E",0,1,"L",0,"-RW"]
[null,null,"2019-09-04","Plugit","180KW Plugit Power Rack","D","S","Y","E",1,8,2,0,0,"E",0,1,"L",0,"-RW"]
[null,null,"2019-12-04","Plugit","360KW Plugit Power Rack system","D","S","Y","E",3,6,2,0,0,"E",0,1,"L",0,"-RW"]
[null,null,"2020-02-03","Plugit","180KW Plugit Power Rack Infy","D","S","Y","E",1,8,2,0,0,"E",0,2,"L",0,"-RW"]
[null,null,"2020-02-03","Plugit","360KW Plugit Power Rack system Infy","D","S","Y","E",3,6,2,0,0,"E",0,2,"L",0,"-RW"]
[]
[null,null,"2019-11-05","Phihong","120KW CSU3.0_CE","D","S","Y","E",1,2,2,"J",4,"E","T",2,"P","H","-RW"]
[null,null,null,"Phihong","120KW CSU3.0_CE","D","S","Y","E",1,2,2,"J",4,"E","W",2,"P","H","-RW"]
[null,null,null,"Phihong","120KW CSU3.0_CE","D","S","Y","E",1,2,2,"J",4,"E","E",2,"P","H","-RW"]
[]
[null,null,"2019-12-17","Phihong","120KW CSU3.0_CE","D","S","Y","E",1,2,2,"J",0,"E","T",2,"P","H","-RW"]
[null,null,null,"Phihong","120KW CSU3.0_CE","D","S","Y","E",1,2,2,"J",0,"E","W",2,"P","H","-RW"]
[null,null,null,"Phihong","120KW CSU3.0_CE","D","S","Y","E",1,2,2,"J",0,"E","E",2,"P","H","-RW"]
[null,null,null,"Phihong","180KW一體式雙槍","D","S","Y","G",1,8,2,"G",0,"G","T",1,"D","H","-RW"]
[null,null,null,"Phihong","80KW Standalone CNS, 380Vac/750Vdc","D","S","Y","C",8,0,1,"G",0,"G","T",1,"D","H","-RW"]
[null,null,null,"Phihong","120KW Standalone CNS, 380Vac/750Vdc","D","S","Y","C",1,2,2,"G",0,"G","T",1,"D","H","-RW"]
[null,null,null,"Phihong","180KW Standalone CNS, 380Vac/750Vdc","D","S","Y","C",1,8,2,"G",0,"G","T",1,"D","H","-RW"]
[null,null,null,"BYTON","60KW單槍/拜騰","D","S","Y","G",6,0,1,"G",0,"G","T",1,"B","T","-RW"]
[null,null,null,"Phihong","160KW一體式雙槍（達宏樁標準品）","D","S","Y","G",1,6,2,"G",0,"G","T",1,"D","H","-RW"]
[null,null,null,"Phihong","160KW分體式雙槍/達宏樁（主柜）","D","D","Y","G",1,6,2,"G","G","D","T",1,"D","H","W"]
[null,null,null,"VOLVO","20KW Movable GB, 380Vac/750Vdc","D","M","Y","G",2,0,1,0,0,"G","E",1,"VLV",null,"-RW"]
[null,null,null,"VOLVO","60KW Movable GB, 380Vac/750Vdc","D","M","Y","G",6,0,1,"G",0,0,"E",1,"VLV",null,"-RW"]
[null,null,null,"Phihong","60KW Standalone CCS1+GB, 380Vac/750Vdc.","D","S","Y","G",6,0,1,"U",0,"G","T",1,"D","H","-RW"]
[null,null,null,"Phihong","180KW Standalone CNS, 380Vac/750Vdc","D","S","Y","C",1,8,2,"G",0,"G","T",1,"D","H","-RW"]
[null,null,null,"Phihong","60KW/一體式雙槍","D","S","Y","G",6,0,1,"G",0,"G","E",1,"C","P","-RW"]
[null,null,"2020-01-09","Phihong","120KW Standalone GB, 380Vac/750Vdc","D","S","Y","G",1,2,2,"G",0,"G","T",3,"D","H","-RW"]
[null,null,null,"Phihong","60KW Standalone CCS1+GB, 380Vac/750Vdc.","D","S","Y","G",6,0,1,"U",0,"G","T",1,"D","H","W"]
[null,null,"2020-03-05","Phihong","80KW Standalone GB, 380Vac/750Vdc","D","S","Y","G",8,0,1,"G",0,"G","T",3,"D","H","-RW"]
[null,null,"2020-04-06","Phihong","60KW  Standalone GB, 380Vac/750Vdc","D","S","Y","G",6,0,1,0,0,"G","T",1,"D","H","W"]
[null,null,"2020-04-14","Phihong","160KW Standalone GB, 380Vac/750Vdc","D","S","Y","G",1,6,2,"G",0,"G","T",3,"D","H","-RW"]
[null,null,"2020-07-10","Phihong","60KW Standalone   GB, 380Vac/750Vdc.","D","S","Y","G",6,0,1,0,0,"G","T",1,"D","H","-RW"]
[null,null,"2020-07-10","Phihong","120KW Standalone GB+GB, 380Vac/750Vdc","D","S","Y","G",1,2,2,"G",0,"G","T",1,"D","H","-RW"]
[null,null,"2020-05-15","Phihong","60KW Standalone GB+GB, 380Vac/750Vdc.","D","S","Y","G",6,0,1,"G",0,"G","T",1,"D","H","-RW"]
[null,null,"2020-01-07","Phihong","120KW Standalone CHAdeMO+CCS2, 380Vac/750Vdc.","D","S","Y","E",1,2,2,"J",0,"E","T",3,"P","H","-RW"]
[null,null,"2020-01-07","Phihong","120KW Standalone CHAdeMO+CCS1, 380Vac/750Vdc.","D","S","W","U",1,2,2,"J",0,"U","T",3,"P","H","-RW"]
[null,null,"2020-01-07","Phihong","150KW Standalone CHAdeMO+CCS2, 380Vac/750Vdc","D","S","Y","E",1,5,2,"J",0,"E","T",3,"P","H","-RW"]
[null,null,"2020-01-07","Phihong","150KW Standalone CHAdeMO+CCS1, 380Vac/750Vdc.","D","S","W","U",1,5,2,"J",0,"U","T",3,"P","H","-RW"]
[null,null,"2020-01-07","Phihong","180KW Standalone CHAdeMO+CCS2, 380Vac/750Vdc.","D","S","Y","E",1,8,2,"J",0,"E","T",3,"P","H","-RW"]
[null,null,"2020-01-07","Phihong","180KW Standalone CHAdeMO+CCS1, 380Vac/750Vdc","D","S","W","U",1,8,2,"J",0,"U","T",3,"P","H","-RW"]
[null,null,"2020-01-10","Phihong","180KW Standalone CCS2, 380Vac/750Vdc","D","S","Y","E",1,8,2,0,0,"E","T",3,"P","H","-RW"]
[null,null,"2020-03-05","Phihong","150KW Standalone GB+CCS1, 380Vac/750Vdc.","D","S","Y","E",1,5,2,"G",0,"U","T",3,"P","H","-RW"]
[null,null,"2020-05-06","Phihong","120KW Standalone CCS2+CCS2, 380Vac/750Vdc","D","S","Y","E",1,2,2,"E",0,"E","T",3,"P","H","-RW"]
[null,null,"2020-05-13","Phihong","180KW Standalone GB+CCS2, 380Vac/750Vdc","D","S","Y","E",1,8,2,"G",0,"E","T",3,"P","H","-RW"]
[null,null,"2020-05-13","Phihong","180KW Standalone GB+CCS1, 380Vac/750Vdc","D","S","W","U",1,8,2,"G",0,"U","T",3,"P","H","-RW"]
[null,null,"2020-05-13","Phihong","180KW Standalone CCS2, 380Vac/750Vdc","D","S","Y","E",1,8,2,0,0,"E","T",3,"P","H","-RW"]
[null,null,"2020-05-13","Phihong","180KW Standalone CCS1, 380Vac/750Vdc","D","S","W","U",1,8,2,0,0,"U","T",3,"P","H","-RW"]
[null,null,"2020-07-14","Phihong","90KW Standalone CHA+CCS2, 380Vac/950Vdc","D","S","Y","E",9,0,1,"J",0,"E","D",3,"P","H","-RW"]
[null,null,"2020-07-14","Phihong","90KW Standalone CHA+CCS1, 380Vac/950Vdc","D","S","W","U",9,0,1,"J",0,"U","D",3,"P","H","-RW"]
[null,null,"2020-07-14","Phihong","150KW Standalone CCS2+CCS2, 380Vac/950Vdc","D","S","Y","E",1,5,2,"E",0,"E","D",3,"P","H","-RW"]
[null,null,"2020-07-14","Phihong","150KW Standalone GB+CCS2, 380Vac/950Vdc","D","S","Y","E",1,5,2,"G",0,"E","D",3,"P","H","-RW"]
[null,null,"2020-08-17","Phihong","120KW Standalone GB+CCS1,380Vac/950Vdc","D","S","Y","E",1,2,2,"G",0,"U","D",3,"P","H","-RW"]
[null,null,"2020-08-17","Phihong","120KW Standalone GB+CCS1,380Vac/950Vdc","D","S","W","U",1,2,2,"G",0,"U","D",3,"P","H","-RW"]
[null,null,"2020-10-21","Phihong","120KW Standalone CHAdeMO+CCS2, 380Vac/950Vdc.","D","S","Y","E",1,2,2,"J",0,"E","D",3,"P","H","-RW"]
[null,null,"2020-10-21","Phihong","120KW Standalone CHAdeMO+CCS1, 380Vac/950Vdc.","D","S","W","U",1,2,2,"J",0,"U","D",3,"P","H","-RW"]
[null,null,"2020-10-21","Phihong","150KW Standalone CHAdeMO+CCS2, 380Vac/950Vdc","D","S","Y","E",1,5,2,"J",0,"E","D",3,"P","H","-RW"]
[null,null,"2020-10-21","Phihong","150KW Standalone CHAdeMO+CCS1, 380Vac/950Vdc.","D","S","W","U",1,5,2,"J",0,"U","D",3,"P","H","-RW"]
[null,null,"2020-10-21","Phihong","180KW Standalone CHAdeMO+CCS2, 380Vac/950Vdc.","D","S","Y","E",1,8,2,"J",0,"E","D",3,"P","H","-RW"]
[null,null,"2020-10-21","Phihong","180KW Standalone CHAdeMO+CCS1, 380Vac/950Vdc","D","S","W","U",1,8,2,"J",0,"U","D",3,"P","H","-RW"]
[null,null,"2020-10-21","Phihong","180KW Standalone CCS2, 380Vac/950Vdc","D","S","Y","E",1,8,2,0,0,"E","D",3,"P","H","-RW"]
[null,null,"2020-10-21","Phihong","150KW Standalone GB+CCS1, 380Vac/950Vdc.","D","S","Y","E",1,5,2,"G",0,"U","D",3,"P","H","-RW"]
[null,null,"2020-10-21","Phihong","120KW Standalone CCS2+CCS2, 380Vac/950Vdc","D","S","Y","E",1,2,2,"E",0,"E","D",3,"P","H","-RW"]
[null,null,"2020-10-21","Phihong","180KW Standalone GB+CCS2, 380Vac/950Vdc","D","S","Y","E",1,8,2,"G",0,"E","D",3,"P","H","-RW"]
[null,null,"2020-10-21","Phihong","180KW Standalone GB+CCS1, 380Vac/950Vdc","D","S","W","U",1,8,2,"G",0,"U","D",3,"P","H","-RW"]
[null,null,"2020-10-21","Phihong","180KW Standalone CCS2, 380Vac/950Vdc","D","S","Y","E",1,8,2,0,0,"E","D",3,"P","H","-RW"]
[null,null,"2020-10-21","Phihong","180KW Standalone CCS1, 380Vac/950Vdc","D","S","W","U",1,8,2,0,0,"U","D",3,"P","H","-RW"]
[null,null,"2020-11-04","Zenobe","120KW Standalone CCS2+CCS2, 380Vac/950Vdc","D","S","Y","E",1,2,2,"E",0,"E","D",3,"Z","B","-RW"]
[null,null,"2020-11-23","Phihong","90KW Standalone CCS2+CCS2, 380Vac/950Vdc","D","S","Y","E",9,0,1,"E",0,"E","D",3,"P","H","-RW"]
[null,null,"2020-12-02","Phihong","180KW Standalone CHA+CHA, 380Vac/950Vdc","D","S","Y","E",1,8,2,"J",0,"J","D",3,"P","H","-RW"]
[null,null,"2020-10-22","Phihong","180KW Standalone CHA+CCS2, 380Vac/950Vdc","D","S","Y","E",1,8,2,"J",0,"E","D",4,"P","H","-RW"]
[null,null,"2020-11-20","Phihong","150KW Standalone CHA+CCS2, 380Vac/750Vdc","D","S","Y","E",1,5,2,"J",0,"E","D",4,"P","H","-RW"]
[null,null,"2020-11-20","Phihong","90KW Standalone CHA+CCS2, 380Vac/750Vdc","D","S","Y","E",9,0,1,"J",0,"E","D",4,"P","H","-RW"]
[null,null,"2020-10-22","Phihong","120KW Standalone CHA+CCS2, 380Vac/750Vdc","D","S","Y","E",1,2,2,"J",0,"E","D",4,"P","H","-RW"]
[null,null,"2020-12-04","Phihong","180KW Standalone CHA+CHA, 380Vac/950Vdc","D","S","Y","E",1,8,2,"J",0,"J","D",3,"P","H","-RW"]
[null,null,"2022-05-24","Noodoe","EVSE DS 3P,480Vac UL 120kW J0U","D","S","W","U",1,2,2,"J",0,"U","D",5,"N",0,"-RW","D5擴容機(擴增至180)"]
[null,null,"2022-05-24","Noodoe","EVSE DS 3P,380-415Vac CNS 120kW J0E","D","S","Y","C",1,2,2,"U",0,"E","D",5,"N",0,"-RW","D5擴容機(擴增至180)"]
[null,null,"2022-05-27","Phihong","EVSE DS 3P,380-415Vac CNS 120kW U0U","D","S","Y","C",1,2,2,"U",0,"U","D",5,"P","H","-RW","D5擴容機(擴增至180)"]
[null,null,"2022-05-27","Phihong","EVSE DS 3P,380-415Vac CNS 120kW U0E","D","S","Y","C",1,2,2,"U",0,"E","D",5,"P","H","-RW","D5擴容機(擴增至180)"]
[null,null,"2022-06-01","Phihong","EVSE DS 3P,380-415Vac CNS 150KW U00","D","S","Y","C",1,5,2,"U",0,0,"D",5,"P","H","-RW","D5擴容機(擴增至180)"]
[null,null,"2022-06-06","Phihong","EVSE DS 3P,380-415Vac CNS 120KW J0U","D","S","Y","C",1,2,2,"J",0,"U","D",5,"P","H","-RW","D5擴容機(擴增至180)"]
[null,null,"2022-06-06","Phihong","EVSE DS 3P,380-415Vac CNS 150KW J0U","D","S","Y","C",1,5,2,"J",0,"U","D",5,"P","H","-RW","D5擴容機(擴增至180)"]
[null,null,"2022-06-06","Phihong","EVSE DS 3P,380-415Vac CNS 150KW U0E","D","S","Y","C",1,5,2,"U",0,"E","D",5,"P","H","-RW","D5擴容機(擴增至180)"]
[null,null,"2022-06-06","Phihong","EVSE DS 3P,380-415Vac CNS 90KW J0U","D","S","Y","C",9,0,1,"J",0,"U","D",5,"P","H","-RW","D5擴容機(擴增至180)"]
[null,null,"2022-06-06","Phihong","EVSE DS 3P,380-415Vac CNS 90KW U0U","D","S","Y","C",9,0,1,"U",0,"U","D",5,"P","H","-RW","D5擴容機(擴增至180)"]
{"$rows_empty":9}
[null,"Wallbox"]
[null,null,"2019-04-16","Phihong","25KW Wallbox","D","W","Y","E",2,5,1,"J",0,"E","T",1,"P","H","-RW"]
[null,null,null,"Phihong","25KW Wallbox","D","W","W","U",2,5,1,"J",0,"U","T",1,"P","H","-RW"]
[null,null,null,"Phihong","25KW Wallbox","D","W","Y","C",2,5,1,"J",0,"U","T",1,"P","H","-RW"]
[null,null,null,"Phihong","25KW Wallbox","D","W","S","U",2,5,1,"J",0,"U","T",1,"P","H","-RW"]
[]
[null,null,"2019-11-08","Phihong","30KW Wallbox (US)","D","W","W","U",3,0,1,"J",0,"U","T",1,"P","H","-RW"]
[null,null,null,"Phihong","30KW Wallbox (EU)","D","W","Y","E",3,0,1,"J",0,"E","T",1,"P","H","-RW"]
[]
[null,"Movable"]
[null,null,"2019-05-28","Phihong","30KW Movable F-750","D","M","Y","E",3,0,1,"E",0,0,"T",1,"P","H","-RW"]
[null,null,null,"Phihong","30KW Movable F-750","D","M","Y","E",3,0,1,"G",0,0,"T",1,"P","H","-RW"]
[null,null,"2019-10-25","Phihong","30KW Movable Infy PSU CSU3.0_CE","D","M","Y","E",3,0,1,"E",0,0,0,2,"P","H","-RW"]
[null,null,"2019-10-25","Phihong","30KW Movable Infy PSU CSU3.0_CE","D","M","Y","E",3,0,1,"E",0,0,"E",2,"P","H","-RW"]
[null,null,"2019-10-25","Phihong","30KW Movable Infy PSU CSU3.0_CE","D","M","Y","E",3,0,1,"E",0,0,"W",2,"P","H","-RW"]
[null,null,"2019-10-25","Phihong","30KW Movable Infy PSU CSU3.0_CE","D","M","Y","E",3,0,1,"E",0,0,"T",2,"P","H","-RW"]
[null,null,"2019-10-25","Phihong","30KW Movable Infy PSU CSU3.0_UL","D","M","W","U",3,0,1,"U",0,0,0,2,"P","H","-RW"]
[null,null,"2019-10-25","Phihong","30KW Movable Infy PSU CSU3.0_UL","D","M","W","U",3,0,1,"U",0,0,"E",2,"P","H","-RW"]
[null,null,"2019-10-25","Phihong","30KW Movable Infy PSU CSU3.0_UL","D","M","W","U",3,0,1,"U",0,0,"W",2,"P","H","-RW"]
[null,null,"2019-10-25","Phihong","30KW Movable Infy PSU CSU3.0_UL","D","M","W","U",3,0,1,"U",0,0,"T",2,"P","H","-RW"]
[]
[]
[null,null,null,"Phihong","30KW Movable Infy PSU CSU3.0_CE","D","M","Y","E",3,0,1,"J",0,0,"W",2,"P","H","-RW"]
[null,null,null,"Phihong","30KW Movable Infy PSU CSU3.0_CE","D","M","Y","E",3,0,1,"J",0,0,"T",2,"P","H","-RW"]
[null,null,null,"Phihong","30KW Movable Infy PSU CSU3.0_UL","D","M","W","U",3,0,1,"J",0,0,"E",2,"P","H","-RW"]
[null,null,null,"Phihong","30KW Movable Infy PSU CSU3.0_UL","D","M","W","U",3,0,1,"J",0,0,"W",2,"P","H","-RW"]
[null,null,null,"Phihong","30KW Movable Infy PSU CSU3.0_UL","D","M","W","U",3,0,1,"J",0,0,"T",2,"P","H","-RW"]
[]
[null,null,"2020-06-19","麗寶","30KW Movable CSU3.0_GB (Ethernet+WiFi)","D","M","Y","C",3,0,1,"G",0,0,"W",2,"P","H","-RW"]
[]
[null,null,"2020-07-20","Phihong","30KW Movable CSU3.0_CE (Ethernet + WiFi + 4G)","D","M","Y","E",3,0,1,"E",0,0,"D",2,"P","H","-RW"]
[null,null,null,"Phihong","30KW Movable CSU3.0_UL (Ethernet + WiFi + 4G)","D","M","W","U",3,0,1,"U",0,0,"D",2,"P","H","-RW"]
[]
[null,null,"2021-01-07","Porsche","EVSE DM 3P, 380-415Vac CNS 30KW U00 PS","D","M","Y","C",3,0,1,"U",0,0,"D",2,"P","S","-RW"]
[null,null,null,"e4You","EVSE DM 3P, 380-415Vac CE 30KW E00 e4","D","M","Y","E",3,0,1,"E",0,0,"D",2,"e",4,"-RW"]
[]
[null,null,"2020-09-23","Phihong","EVSE DO 3P, 380-415Vac CNS 360kW 000 PH","D","O","Y","C",3,6,2,0,0,0,"D",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 380-415Vac CNS 360kW V0U PH","D","D","Y","C",3,6,2,"V",0,"U","E",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 380-415Vac CNS 360kW J0U PH","D","D","Y","C",3,6,2,"J",0,"U","E",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 380-415Vac CNS 360kW G00 PH","D","D","Y","C",3,6,2,"G",0,0,"E",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 380-415Vac CNS 360kW J00 PH","D","D","Y","C",3,6,2,"J",0,0,"E",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 380-415Vac CNS 360kW U00 PH","D","D","Y","C",3,6,2,"U",0,0,"E",2,"P","H","-RW"]
[null,null,null,"Phihong"]
[null,null,null,"Phihong","EVSE DO 3P, 380-415Vac CE 360kW 000 PH","D","O","Y","E",3,6,2,0,0,0,"D",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 380-415Vac CE 360kW F0E PH","D","D","Y","E",3,6,2,"F",0,"E","E",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 380-415Vac CE 360kW E0E PH","D","D","Y","E",3,6,2,"E",0,"E","E",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 380-415Vac CE 360kW J0E PH","D","D","Y","E",3,6,2,"J",0,"E","E",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 380-415Vac CE 360kW G00 PH","D","D","Y","E",3,6,2,"G",0,0,"E",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 380-415Vac CE 360kW J00 PH","D","D","Y","E",3,6,2,"J",0,0,"E",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 380-415Vac CE 360kW E00 PH","D","D","Y","E",3,6,2,"E",0,0,"E",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 380-415Vac CE 360kW G0G PH","D","D","Y","E",3,6,2,"G",0,"G","E",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 380-415Vac CE 360kW G0E PH","D","D","Y","E",3,6,2,"G",0,"E","E",2,"P","H","-RW"]
[null,null,null,"Phihong"]
[null,null,null,"Phihong","EVSE DO 3P, 480Vac UL 360kW 000 PH","D","O","W","U",3,6,2,0,0,0,"D",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 480Vac UL 360kW V0U PH","D","D","W","U",3,6,2,"V",0,"U","E",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 480Vac UL 360kW J0U PH","D","D","W","U",3,6,2,"J",0,"U","E",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 480Vac UL 360kW G00 PH","D","D","W","U",3,6,2,"G",0,0,"E",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 480Vac UL 360kW J00 PH","D","D","W","U",3,6,2,"J",0,0,"E",2,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 480Vac UL 360kW U00 PH","D","D","W","U",3,6,2,"U",0,0,"E",2,"P","H","-RW"]
[null,null,null,"Phihong"]
[null,null,null,"Phihong","EVSE DO 3P, 380-415Vac CNS 180kW 000 AD","D","O","Y","C",1,8,2,0,0,0,"D",2,"A","D","-RW"]
[null,null,null,"Phihong","EVSE DD 3P, 380-415Vac CNS 180kW V0U AD","D","D","Y","C",1,8,2,"V",0,"U","E",2,"A","D","-RW"]
[null,null,"2020-11-03","Plugit","EVSE DR 3P,380-415Vac 180KW EEE PL","D","S","Y","E",1,8,2,"E","E","E",0,2,"L",1,"-RW"]
[null,null,null,"Phihong","EVSE DR 3P,380-415Vac 180KW E0E PH","D","R","Y","E",1,8,2,"E",0,"E","D",2,"P","H","-RW"]
[null,null,"2020-11-10","Phihong","EVSE DW 3P, 380-415Vac CE 30KW E00 PH","D","W","Y","E",3,0,1,"E",0,0,"D",1,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DW 3P, 480Vac UL 30KW U00 PH","D","W","W","U",3,0,1,"U",0,0,"D",1,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DW 3P, 380-415Vac CNS 30KW U00 PH","D","W","Y","C",3,0,1,"U",0,0,"D",1,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DW 3P, 380-415Vac CNS 30KW J0U PH","D","W","Y","C",3,0,1,"J",0,"U","D",1,"P","H","-RW"]
[]
[]
[]
[]
[]
[null,null,"2021/28","Phihong","EVSE DW 3P, 480Vac UL 30KW U00 CP, 7m","D","W","W","U",3,0,1,"U",0,0,"D",1,"C","P","-RW"]
[null,null,"2021-02-25","e4You","EVSE DK 3P, 380Vac CE 180KW 000 E4","D","K","Y","E",1,8,2,0,0,0,"D",1,"E",4,"-RW"]
[null,null,"2021-02-25","e4You","COMBox DX 1P, 220Vac CE 180KW E00 E4","D","X","Y","E",1,8,2,"E",0,0,"E",1,"E",4,"-RW"]
[null,null,"2021-05-25","Phihong","EVSE DK 3P, 380Vac CE 150KW 000 Parallel","D","K","Y","E",1,5,2,0,0,0,"D",1,"P","H","-RW"]
[null,null,null,"e4You","COMBox DX 1P, 220Vac CE 180KW E00 W/ LED","D","X","Y","E",1,8,2,"E",0,0,"E",1,"E",4,"-RW"]
[null,null,null,"Phihong","COMBox DX 1P, 220Vac CE 180KW E00 W/O LED","D","X","Y","E",1,8,2,"E",0,0,"E",2,"P","H","-RW"]
[null,null,null,"Phihong","COMBox DX 1P, 220Vac CE 360KW 000 W/O case","D","X","Y","E",3,6,2,"P",0,0,"E",1,"P","H","-RW"]
[null,null,"2021-09-03","Phihong","EVSE DR 3P,380Vac 240KW E0E PH","D","R","Y","E",2,4,2,"E",0,"E","D",2,"P","H","-RW"]
[null,null,null,"Phihong","COMBox DX 1P, 220Vac CE 180KW E00 W/ LED","D","X","Y","E",1,8,2,"E",0,0,"E",1,"P","H","-RW"]
[null,null,"2021-12-21","Phihong","COMBox DX 1P, 220Vac CE 360KW 000 W/ case & LED","D","X","Y","E",3,6,2,"P",0,0,"E",2,"P","H","-RW"]
[null,null,"2021-12-21","Phihong","EVSE DK 3P, 380Vac CE 180KW 000 Parallel","D","K","Y","E",1,8,2,0,0,0,"D",1,"P","H","-RW"]
[null,null,null,"Phihong","EVSE DR 3P,380Vac 180KW E0E PH","D","R","Y","E",1,8,2,"E",0,"E","D",2,"P","H","-RW"]
[null,null,"2022-02-07","Phihong","EVSE DR 3P,380Vac 150KW E0E PH","D","R","Y","E",1,5,2,"E",0,"E","D",2,"P","H","-RW"]
[null,null,"2022-02-07","Phihong","EVSE DR 3P,380Vac 120KW E0E PH","D","R","Y","E",1,2,2,"E",0,"E","D",2,"P","H","-RW"]
[null,null,"2022-02-07","Phihong","EVSE DR 3P,380Vac 90KW E0E PH","D","R","Y","E",9,0,1,"E",0,"E","D",2,"P","H","-RW"]
[]
[null,null,null,"Phihong"]
[null,null,"2021-03-26","4M w/o PH logo","DS60 CCS1 Dual","D","S","W","U",6,0,1,"U",0,"U","D",2,"P","N","-RW","美分白牌原則:\n1. Cabinet無logo絲印 \n2. Model label 無logo\n3. User manual無logo \n4. UI Display 無Logo\n5. 樁內貼紙不變更\n6. DW30 建Anphenol  65A的槍\n7. DS60 需安規更新後才能使用Anphenol 150A的槍, 目前仍是Rema"]
[null,null,null,"4M w/o PH logo","DS60 CCS1+CHAdeMO","D","S","W","U",6,0,1,"J",0,"U","D",2,"P","N","-RW"]
[null,null,null,"7M w/o PH logo","DS60 CCS1 Dual","D","S","W","U",6,0,1,"U",0,"U","D",2,"N",7,"-RW"]
[null,null,null,"7M w/o PH logo","DS60 CCS1+CHAdeMO","D","S","W","U",6,0,1,"J",0,"U","D",2,"N",7,"-RW"]
[null,null,"2021-03-29","4M w/o PH logo","EVSE DW 3P, 480Vac UL 30KW J0U, No logo, 4m","D","W","W","U",3,0,1,"J",0,"U","D",1,"P","N","-RW"]
[null,null,null,"4M w/o PH logo","EVSE DW 3P, 480Vac UL 30KW J0U, No logo, 7m","D","W","W","U",3,0,1,"J",0,"U","D",1,"N",7,"-RW"]
[null,null,null,"7M w/o PH logo","EVSE DW 3P, 480Vac UL 30KW U00, No logo, 4m","D","W","W","U",3,0,1,"U",0,0,"D",1,"P","N","-RW"]
[null,null,null,"7M w/o PH logo","EVSE DW 3P, 480Vac UL 30KW U00, No logo, 7m","D","W","W","U",3,0,1,"U",0,0,"D",1,"N",7,"-RW"]
[null,null,"2021-04-13","US LED","EVSE DW 3P, 480Vac UL 30KW U00 UD, 4m","D","W","W","U",3,0,1,"U",0,0,"D",1,"U","D","-RW","1. Customer Logo painting on cabinet\n2. Customer Model label (different ETL no.)\n3. 增加Carton label\n4. 槍Rema"]
[null,null,"2021-04-15","US LED","EVSE DW 3P, 480Vac UL 30KW J0U UD, 4m","D","W","W","U",3,0,1,"J",0,"U","D",1,"U","D","-RW"]
[null,null,"2021-04-13","Bosch","EVSE DW 3P, 480Vac UL 30KW U00 C, 4m","D","W","W","U",3,0,1,"U",0,0,"D",1,"C",0,"-RW","Bosch 客製化: TBD\n先依美分白牌準備, 槍先備Rema"]
[null,null,"2021-06-04","Phihong","EVSE DW 3P, 480Vac CE 30KW M00 80A PH","D","W","Y","E",3,0,1,"M",0,0,"D",1,"P","H","-RW","Phoenix 80A CCS2"]
[null,null,"2021-06-04","Phihong","EVSE DW 3P, 480Vac CE 30KW J0M 80A PH","D","W","Y","E",3,0,1,"J",0,"M","D",1,"P","H","-RW","CHAdeMO+Phoenix 80A CCS2"]
[null,null,"2021-06-04","Phihong","EVSE DW 3P, 480Vac UL 30KW N00 80A PH","D","W","W","U",3,0,1,"N",0,0,"D",1,"P","H","-RW","Phoenix 80A CCS1"]
[null,null,"2021-06-04","Phihong","EVSE DW 3P, 480Vac UL 30KW J0N 80A PH","D","W","W","U",3,0,1,"J",0,"N","D",1,"P","H","-RW","CHAdeMO+Phoenix 80A CCS1"]
[null,null,"2021-06-04","Phihong","EVSE DM 3P, 380-415Vac CE 30KW M00 80A PH","D","M","Y","E",3,0,1,"M",0,0,"D",2,"P","H","-RW","Phoenix 80A CCS2"]
[null,null,"2021-06-04","Phihong","EVSE DM 3P, 380-415Vac CE 30KW N00 80A PH","D","M","Y","E",3,0,1,"N",0,0,"D",2,"P","H","-RW","Phoenix 80A CCS1"]
[null,null,"2021-06-08","w/o PH logo","EVSE DM 3P, 480Vac UL 30KW E00 60A No logo","D","M","W","U",3,0,1,"E",0,0,"D",2,"P","N","-RW"]
[null,null,"2021-06-22","Zenobe","EVSE DM  3P, 480Vac CE 30KW E00 60A ZB","D","M","Y","E",3,0,1,"E",0,0,"D",2,"Z","B","-RW","搭 Phoenix CCS2"]
[null,null,"2021-08-12","Phihong","EVSE DW 3P, 480Vac UL 30KW N00 80A PH","D","W","Y","C",3,0,1,"N",0,0,"D",1,"P","H","-RW","Phoenix 80A CCS1"]
[null,null,"2021-08-12","Phihong","EVSE DW 3P, 480Vac UL 30KW J0N 80A PH","D","W","Y","C",3,0,1,"J",0,"N","D",1,"P","H","-RW","CHAdeMO+Phoenix80A CCS1"]
[null,null,"2021-08-12","Phihong","EVSE DM 3P, 480Vac UL 30KW N00 80A PH","D","M","Y","C",3,0,1,"N",0,0,"D",2,"P","H","-RW","Phoenix 80A CCS1"]
[null,null,"2021-09-15","Noodoe","EVSE DW 3P,380-415Vac YC 30KW J0U N0, 5M","D","W","Y","C",3,0,1,"J",0,"U","D",1,"N",0,"-RW","搭 Amphenol CCS1+SUMIOTOMO CHAdeMO,5M"]
[null,null,"2021-09-15","Noodoe","EVSE DW 3P,380-415Vac YC 30KW J0U N1, 7.5M","D","W","Y","C",3,0,1,"J",0,"U","D",1,"N",1,"-RW","搭 Amphenol CCS1+SUMIOTOMO CHAdeMO,7.5M"]
[null,null,"2021-11-23","Noodoe","EVSE DW 3P,380-415Vac YC 30KW U0E N0, 5M","D","W","Y","C",3,0,1,"U",0,"E","D",1,"N",0,"-RW","搭 Amphenol CCS1+CCS2,5M"]
[null,null,"2021-12-01","TOG","EVSE DW 3P, 480Vac UL 30KW U00 60A,4.5M TOG","D","W","W","U",3,0,1,"U",0,0,"D",1,"T","G","-RW","CCS1,4.5M"]
[null,null,"2021-12-01","TOG","EVSE DW 3P, 480Vac UL 30KW J0U 60A,4.5M TOG","D","W","W","U",3,0,1,"J",0,"U","D",1,"T","G","-RW","CCS1,4.5M"]
[null,null,"2021-12-01","TOG","EVSE DW 3P, 480Vac UL 30KW U00 60A,7M TOG","D","W","W","U",3,0,1,"U",0,0,"D",1,"T",7,"-RW","CHAdeMO+CCS1,7M"]
[null,null,"2021-12-01","TOG","EVSE DW 3P, 480Vac UL 30KW J0U 60A,7M TOG","D","W","W","U",3,0,1,"J",0,"U","D",1,"T",7,"-RW","CHAdeMO+CCS1,7M"]
[null,null,"2021-12-06","SHELL","EVSE DW 3P, 480Vac CE 30KW E00 60A,4.5M SHELL","D","W","Y","E",3,0,1,"E",0,0,"D",1,"O","L","-RW","CCS2,4.5M"]
[null,null,"2021-12-06","SHELL","EVSE DW 3P, 480Vac CE 30KW J0E 60A,4.5M SHELL","D","W","Y","E",3,0,1,"J",0,"E","D",1,"O","L","-RW","CHAdeMO+CCS2,4.5M"]
[null,null,"2021-12-06","SHELL","EVSE DW 3P, 480Vac UL 30KW U00 60A,4.5M SHELL","D","W","W","U",3,0,1,"U",0,0,"D",1,"O","L","-RW","CCS1,4.5M"]
[null,null,"2021-12-06","SHELL","EVSE DW 3P, 480Vac UL 30KW J0U 60A,4.5M SHELL","D","W","W","U",3,0,1,"J",0,"U","D",1,"O","L","-RW","CHAdeMO+CCS1,4.5M"]
[null,null,"2021-12-06","SHELL","EVSE DM 3P, 480Vac CE 30KW E00 60A,4.5M SHELL","D","M","Y","E",3,0,1,"E",0,0,"D",2,"O","L","-RW","CCS2,4.5M"]
[null,null,"2021-12-06","SHELL","EVSE DM 3P, 480Vac CE 30KW J00 60A,4.5M SHELL","D","M","Y","E",3,0,1,"J",0,0,"D",2,"O","L","-RW","CHAdeMO,4.5M"]
[null,null,"2021-12-06","SHELL","EVSE DM 3P, 480Vac UL 30KW U00 60A,4.5M SHELL","D","M","W","U",3,0,1,"U",0,0,"D",2,"O","L","-RW","CCS1,4.5M"]
[null,null,"2021-12-06","SHELL","EVSE DM 3P, 480Vac UL 30KW J00 60A,4.5M SHELL","D","M","W","U",3,0,1,"J",0,0,"D",2,"O","L","-RW","CHAdeMO,4.5M"]
[null,null,"2021-12-14","PHIHONG","EVSE DW 3P, 380-415Vac CNS 30KW U0E 60A,4.5M","D","M","Y","C",3,0,1,"U",0,"E","D",1,"P","H","-RW","CCS1+CCS2,4.5M"]
[null,null,"2021-12-15","FLOOX","EVSE DW 3P, 380-415Vac CE 30KW M00 80A,4.5M","D","W","Y","E",3,0,1,"M",0,0,"D",1,"F","L","-RW","CCS2,80A,4.5M"]
[null,null,"2021-12-15","FLOOX","EVSE DW 3P, 380-415Vac CE 30KW J0M 80A,4.5M","D","W","Y","E",3,0,1,"J",0,"M","D",1,"F","L","-RW","CHAdeMO+CCS2,80A,4.5M"]
[null,null,"2021-12-15","FLOOX","EVSE DM 3P, 380-415Vac CE 30KW M00 80A,4.5M","D","M","Y","E",3,0,1,"M",0,0,"D",2,"F","L","-RW","CCS2,80A,4.5M"]
[null,null,"2022-02-17","Phihong","EVSE DW 3P, 380-415Vac YC 30KW J0E 60A,4.5M","D","W","Y","C",3,0,1,"J",0,"E","D",1,"P","H","-RW","CHAdeMO+CCS2 ,60A, 5M"]
[null,null,"2022-02-17","SHELL","EVSE DW 3P, 380-415Vac CE 30KW E00 60A,7.5M SHELL","D","W","Y","E",3,0,1,"E",0,0,"D",1,"O",7,"-RW","CCS2, 60A,7.5M"]
[null,null,"2022-02-23","SHELL","EVSE DW 3P, 380-415Vac CE 30KW M00 80A,7.5M SHELL","D","W","Y","E",3,0,1,"M",0,0,"D",1,"O",7,"-RW","CCS2, 80A,7.5M,Phoenix"]
[null,null,"2022-02-23","WAT","EVSE DW 3P, 380-415Vac CE 30KW M00 80A,4.5M WAT","D","W","Y","E",3,0,1,"M",0,0,"D",1,"W",0,"-RW","CCS2, 80A,4.5M,Phoenix"]
[null,null,"2022-02-23","WAT Ford","EVSE DW 3P, 380-415Vac CE 30KW M00 80A,4.5M WAT Ford","D","W","Y","E",3,0,1,"M",0,0,"D",1,"W",2,"-RW","CCS2, 80A,4.5M,Phoenix"]
[null,null,"2022-03-01","SHELL","EVSE DW 3P,380-415Vac CE 30KW J0M 80A,7.5M SHELL","D","W","Y","E",3,0,1,"J",0,"M","D",1,"O",7,"-RW","CHAdeMO+CCS2,80A,7.5M"]
[null,null,"2022-03-01","SHELL","EVSE DW 3P,380-415Vac CE 30KW J0M 60A,7.5M SHELL","D","W","Y","E",3,0,1,"J",0,"E","D",1,"O",7,"-RW","CHAdeMO+CCS2,60A,7.5M"]
[null,null,"2022-03-07","Vone(視一科技)","EVSE DW 3P,380-415Vac YC 30KW U0E 60A, 4.5M","D","W","Y","C",3,0,1,"U",0,"E","D",1,"V","N","-RW","CCS1/CCS2, 60A,4.5M"]
[null,null,"2022-03-16","WAT","EVSE DW 3P, 380-415Vac CE 30KW J0M 80A,4.5M WAT","D","W","Y","E",3,0,1,"J",0,"M","D",1,"W",0,"-RW","CHAdeMO+CCS2,80A,4.5M Phoenix"]
[null,null,"2022-03-16","WAT","EVSE DW 3P, 380-415Vac CE 30KW M00 80A,4.5M WAT","D","M","Y","E",3,0,1,"M",0,0,"D",2,"W",0,"-RW","CCS2,80A,4.5M"]
[null,null,"2022-03-16","WAT Ford","EVSE DW 3P, 380-415Vac CE 30KW J0M 80A,4.5M WAT Ford","D","W","Y","E",3,0,1,"J",0,"M","D",1,"W",2,"-RW","CHAdeMO+CCS2,80A,4.5M Phoenix"]
[null,null,"2022-03-16","WAT Ford","EVSE DW 3P, 380-415Vac CE 30KW M00 80A,4.5M WAT Ford","D","M","Y","E",3,0,1,"M",0,0,"D",2,"W",2,"-RW","CCS2,80A,4.5M"]
[null,null,"2022-03-30","Vone(視一科技)","EVSE DW 30, 380-415Vac CE 30KW U0E 80A,4.5M Vone","D","W","Y","C",3,0,1,"N",0,"M","D",1,"V","N","-RW","CCS1/CCS2, 80A,4.5M"]
[null,null,"2022-05-03","SHELL","EVSE DW 30,480Vac UL 30KW U00,7M SHELL","D","W","W","U",3,0,1,"U",0,0,"D",1,"O",7,"-RW","CCS1,60A,7M"]
[null,null,"2022-05-03","SHELL","EVSE DW 30,480Vac UL 30KW J0U,7M SHELL","D","W","W","U",3,0,1,"J",0,"U","D",1,"O",7,"-RW","CCS1,CHAdeMO,60A 7M"]
[null,null,"2022-05-03","Phihong","EVSE DW 30, 480Vac UL 30KW U00,7M,white","D","W","W","U",3,0,1,"U",0,0,"D",1,"W","S","-RW","CCS1,60A,7M/no logo/white"]
[null,null,"2022-05-03","Phihong","EVSE DW 30, 480Vac UL 30KW J0U,7M,white","D","W","W","U",3,0,1,"J",0,"U","D",1,"W","S","-RW","CHAdeMO+CCS1,60A,7M/no logo/white"]
[null,null,"2022-05-03","Phihong","EVSE DW 30, 480Vac UL 30KW U00,4.5M,white","D","W","W","U",3,0,1,"U",0,0,"D",1,"W","N","-RW","CCS1,60A,5M/no logo/white"]
[null,null,"2022-05-03","Phihong","EVSE DW 30, 480Vac UL 30KW J0U,4.5M,white","D","W","W","U",3,0,1,"J",0,"U","D",1,"W","N","-RW","CHAdeMO+CCS1,60A,5M/no logo/white"]
[null,null,"2022-05-09","Phihong","EVSE DM 30, 480Vac UL 30KW U00,4.5M,white","D","M","W","U",3,0,1,"U",0,0,"D",2,"W","N","-RW","CCS1,60A,5M/no logo/white"]
[null,null,"2022-06-02","BERGER","EVSE DM 3P, 380-415Vac CE 30KW M00","D","M","Y","E",3,0,1,"M",0,0,"D",2,"B","E","-RW","CCS2,80A,4.5M Phoenix"]
[null,null,"2022-06-08","BOSCH","EVSE DM 3P,480Vac UL 30KW U00,BOSCH","D","M","W","U",3,0,1,"U",0,0,"D",2,"C",0,"-RW","CCS1 60A,4.5M Amphenol"]
[]
[]
[null,"DB-- Dc to Dc EVSE  "]
[null,null,"2021-11-04","TCC","EVSE DB 1P,220~240Vac CNS 180kW 000 TC","D","B","Y","C",1,8,2,0,0,0,"D",1,"T","C","-RW","Dc to Dc EVse Output power cabinet, 包模"]
[null,null,"2021-11-04","TCC","EVSE DB 1P,220~240Vac CNS 120kW 000 TC","D","B","Y","C",1,2,2,0,0,0,"D",1,"T","C","-RW","Dc to Dc EVse Output power cabinet, 包模"]
[null,null,"2021-11-04","TCC","EVSE DD 1P,220~240Vac CNS 180kW V0E TC","D","D","Y","C",0,0,0,"V",0,"E","E",1,"T","C","-RW","精誠讀卡機-客供、包模"]
[null,null,"2021-11-04","TCC","EVSE DD 1P,220~240Vac CNS 180kW V0E TC","D","D","Y","C",0,0,0,"V",0,"E","E",2,"T","C","-RW","RFID、包模"]
[null,"UU 360 >標準品/白牌 髮絲/LOGO/   UL/CE"]
[null,null,"2021-11-05","UU","EVSE DO 3P,220~240Vac CNS 360kW 000 UU","D","O","Y","C",3,6,2,0,0,0,"D",2,"U","U","-RW"]
[null,null,"2021-11-05","UU","EVSE DD 3P,220~240Vac CNS 360kW V0E UU","D","D","Y","C",3,6,2,"V",0,"U","E",2,"U","U","-RW"]
[null,null,"2021-11-05","UU","EVSE DD 3P,220~240Vac CNS 360kW F0E UU","D","D","Y","C",3,6,2,"F",0,"E","E",2,"U","U","-RW"]
[null,null,"2021-11-04","PN","EVSE DO 3P,220~240Vac UL 360kW 000 PN","D","O","W","U",3,6,2,0,0,0,"D",3,"P","N","-RW","UL 飾板 (髮絲紋);標準機(Without logo)"]
[null,null,"2021-11-04","PH","EVSE DO 3P,220~240Vac UL 360kW 000 PH","D","O","W","U",3,6,2,0,0,0,"D",3,"P","H","-RW","UL 飾板 (髮絲紋);標準機(With logo)"]
[null,null,"2021-11-04","PN","EVSE DO 3P,220~240Vac UL 360kW 000 PN","D","O","W","U",3,6,2,0,0,0,"D",2,"P","N","-RW","UL 飾板 (無髮絲紋)標準機(Without logo)"]
[null,null,"2021-11-04","PH","EVSE DO 3P,220~240Vac UL 360kW 000 PH","D","O","W","U",3,6,2,0,0,0,"D",2,"P","H","-RW","UL 飾板 (無髮絲紋)標準機(With logo)"]
[null,null,"2021-11-04","PN","EVSE DO 3P,220~240Vac CE 360kW 000 PN","D","O","Y","E",3,6,2,0,0,0,"D",3,"P","N","-RW","CE 飾板 (髮絲紋);標準機(Without logo)"]
[null,null,"2021-11-04","PH","EVSE DO 3P,220~240Vac CE 360kW 000 PH","D","O","Y","E",3,6,2,0,0,0,"D",3,"P","H","-RW","CE  飾板 (髮絲紋);標準機(With logo)"]
[null,null,"2021-11-04","PN","EVSE DO 3P,220~240Vac CE 360kW 000 PN","D","O","Y","E",3,6,2,0,0,0,"D",2,"P","N","-RW","CE  飾板 (無髮絲紋)標準機(Without logo)"]
[null,null,"2021-11-04","PH","EVSE DO 3P,220~240Vac CE 360kW 000 PH","D","O","Y","E",3,6,2,0,0,0,"D",2,"P","H","-RW","UL 飾板 (無髮絲紋)標準機(With logo)"]
[null,null,"2021-11-05","PN","EVSE DD 3P,220~240Vac UL 360kW V0U PN","D","D","W","U",3,6,2,"V",0,"U","E",3,"P","N","-RW","UL 飾板 (髮絲紋);標準機(Without logo)"]
[null,null,"2021-11-05","PH","EVSE DD 3P,220~240Vac UL 360kW V0U PH","D","D","W","U",3,6,2,"V",0,"U","E",3,"P","H","-RW","UL 飾板 (髮絲紋);標準機(With logo)"]
[null,null,"2021-11-05","PN","EVSE DD 3P,220~240Vac UL 360kW V0U PN","D","D","W","U",3,6,2,"V",0,"U","E",2,"P","N","-RW","UL 飾板 (無髮絲紋)標準機(Without logo)"]
[null,null,"2021-11-05","PH","EVSE DD 3P,220~240Vac UL 360kW V0U PH","D","D","W","U",3,6,2,"V",0,"U","E",2,"P","H","-RW","UL 飾板 (無髮絲紋)標準機(With logo)"]
[null,null,"2021-11-05","PN","EVSE DD 3P,220~240Vac CE 360kW K0D PN","D","D","Y","E",3,6,2,"K",0,"D","E",3,"P","N","-RW","CE 飾板 (髮絲紋);標準機(Without logo)"]
[null,null,"2021-11-05","PH","EVSE DD 3P,220~240Vac CE 360kW K0D PH","D","D","Y","E",3,6,2,"K",0,"D","E",3,"P","H","-RW","CE  飾板 (髮絲紋);標準機(With logo)"]
[null,null,"2021-11-05","PN","EVSE DD 3P,220~240Vac CE 360kW K0D PN","D","D","Y","E",3,6,2,"K",0,"D","E",2,"P","N","-RW","CE  飾板 (無髮絲紋)標準機(Without logo)"]
[null,null,"2021-11-05","PH","EVSE DD 3P,220~240Vac CE 360kW K0D PH","D","D","Y","E",3,6,2,"K",0,"D","E",2,"P","H","-RW","UL 飾板 (無髮絲紋)標準機(With logo)"]
[null,null,"2021-11-05","PN","EVSE DD 3P,220~240Vac UL 360kW K0T PN","D","D","W","U",3,6,2,"K",0,"T","E",3,"P","N","-RW","UL 飾板 (髮絲紋);標準機(Without logo)"]
[null,null,"2021-11-05","PH","EVSE DD 3P,220~240Vac UL 360kW K0T PH","D","D","W","U",3,6,2,"K",0,"T","E",3,"P","H","-RW","UL 飾板 (髮絲紋);標準機(With logo)"]
[null,null,"2021-11-05","PN","EVSE DD 3P,220~240Vac UL 360kW K0T PN","D","D","W","U",3,6,2,"K",0,"T","E",2,"P","N","-RW","UL 飾板 (無髮絲紋)標準機(Without logo)"]
[null,null,"2021-11-05","PH","EVSE DD 3P,220~240Vac UL 360kW K0T PH","D","D","W","U",3,6,2,"K",0,"T","E",2,"P","H","-RW","UL 飾板 (無髮絲紋)標準機(With logo)"]
[null,null,"2021-11-05","PN","EVSE DD 3P,220~240Vac CE 360kW F0G PN","D","D","Y","E",3,6,2,"F",0,"E","E",3,"P","N","-RW","CE 飾板 (髮絲紋);標準機(Without logo)"]
[null,null,"2021-11-05","PH","EVSE DD 3P,220~240Vac CE 360kW F0G PH","D","D","Y","E",3,6,2,"F",0,"E","E",3,"P","H","-RW","CE  飾板 (髮絲紋);標準機(With logo)"]
[null,null,"2021-11-05","PN","EVSE DD 3P,220~240Vac CE 360kW F0G PN","D","D","Y","E",3,6,2,"F",0,"E","E",2,"P","N","-RW","CE  飾板 (無髮絲紋)標準機(Without logo)"]
[null,null,"2021-11-05","PH","EVSE DD 3P,220~240Vac CE 360kW F0G PH","D","D","Y","E",3,6,2,"F",0,"E","E",2,"P","H","-RW","UL 飾板 (無髮絲紋)標準機(With logo)"]

{"sheet":"Customer Code Table","index":4,"n_rows":13,"n_cols":4,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Code","Customer","Product Category"]
[null,"PH","Phihong","AC, DC"]
[null,"L","Plugit","DC"]
[null,"P0 ","Phihong standard","AW"]
[null,"N0, N1","Noodoe","AW"]
[null,"B0","BYTON","AW"]
[null,"AD","Audi","DC"]
[null,"P0 ","Phihong 標準機種無螢幕","AX"]
[null,"P1","Phihong 標準機種帶螢幕","AX"]
[null,"TC","TCC ","Dc to Dc"]
[null,"HD"," Hyundai ","AC (纜線盒)"]

{"sheet":"客戶碼","index":5,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[]}
["舊機種","新機種","備註",{"$nulls":4},"PHP機種客制碼"]
["KW 敬穩","PH:  飛宏",{"$nulls":5},"法絲紋系列"]
["M 敏實","N: 拓連/ N1:拓連7.5M",{"$nulls":5},"TOG"]
["S 新筑","B: 拜騰",{"$nulls":5},"標準槍線長度5M=>TG"]
["F 恆譽","P0: Phihong standard",{"$nulls":5},"槍線長度7M=>T7"]
["K 立凱","AD: Audi",{"$nulls":5},"槍線長度10M=>TX"]
["B 百城","PL: Plugit",{"$nulls":5},"槍線長度5M+7M=>T0"]
["Y 雲杉","E4:E4You",{"$nulls":5},"SHELL"]
["J: 江能","CP: Cypress Power","2021-02-08",null,"　","標準品Phihong logo","無logo","標準槍線長度5M=OL"]
["E: 巴斯巴","C0:Bosch","2021-04-13",null,"　","後兩碼客戶碼","後兩碼客戶碼","槍線長度7M=O7"]
["P:飛宏","PN: 白牌4m槍線 DC","2021-03-29",null,"4m槍線","PH","PN","槍線長度10M=OX"]
["D: 森達","P7: 飛宏7m槍線 DC","2021-03-29",null,"7m槍線","P7","N7","槍線長度5M+7M=O0"]
["N: 能科","N7: 白牌7m槍線 DC","2021-03-29",null,"10m槍線","PX","NX","ZB（歐洲市場）"]
["BM 北汽","PX: 飛宏10m槍線 DC","2021-03-29",null,"無logo位置",null,"Cabinet, \nmodel label, \nuser manual, \nUI Display","標準槍線長度5M=ZB"]
["BS 藍天 - 單屏","NX: 白牌10m槍線 DC","2021-03-29",{"$nulls":4},"槍線長度7M=Z7"]
["BK 藍天 - 彩屏","UD: US LED","2021-04-13",{"$nulls":4},"槍線長度10M=ZX"]
["GW 長城","TC :台泥",44504,{"$nulls":4},"槍線長度5M+7M=Z0"]
["CX遼寧城鄉供電","T: TOG","2021-11-22",{"$nulls":4},"ZB（澳洲市場）"]
["TW 儲贏","O: Oil","2021-11-22",{"$nulls":4},"標準槍線長度5M=ZA"]
["WD 威思頓","FL:Floox","2021-12-15",{"$nulls":4},"槍線長度7M=A7"]
["GH 國宏","KE: KED","2022-02-10",{"$nulls":4},"槍線長度10M=AX"]
["JN 京能","W0/W1/W2/W3 : WAT","2022-02-16",{"$nulls":4},"槍線長度5M+7M=A0"]
["FX 富士康","VN:芮億(視一科技)","2022-03-07",{"$nulls":4},"拓連：N0"]
["DZ 山西大众电控设备厂","WN: 美規白牌白機櫃5M槍","2022-04-01",{"$nulls":4},"CL:  CL"]
["PA 大連松下 ","WS:美規白牌白機櫃7M槍","2022-04-01",{"$nulls":4},"E4YOU:  E4"]
[null,"HD-  Hyundai 現代汽車","2022-05-04",{"$nulls":4},"E4YOU不裝槍線：E0"]
[null,"Berger: BE","2022-06-01",{"$nulls":4},"德E: DE"]
[]
[]
["BD: 北斗",null,"PDM查無此客戶"]
["L:飛宏低階版"]
["I - 網路販賣"]
["M: MORGAN"]
["GM: GEELY MORGAN版"]
["JS - 舉視"]
["EM: 凱勝"]
["FT - 富田"]
["JN - 京能"]
["EM - 凱勝"]
["SM - 日月潭 "]
["SS 重庆盛时达汽车"]
["BY- 比亞迪"]
["ND - 拓連科技 "]
["S - 暫定BOM"]
["WM - 威马"]
["DL - 迪卡農"]
["MG: 大綠"]
["BD- 比亞迪(BYD)"]
["HD-  Hyundai 現代汽車"]

{"sheet":"工作表1","index":6,"n_rows":11,"n_cols":10,"rows_kept":11,"cut":false,"hidden":false,"merged":[[8,2,8,5],[9,2,9,5],[10,2,10,5]]}
[null,"2021/May/26"]
[null,"DK編碼"]
[null,"機種名","槍數","Output Relay","Max. output","Current","單槍","單+單","雙槍","雙+雙"]
[null,"DKYE152000D1PH","單",2,"150~240KW","500A","V","V"]
[null,"DKYE152000D2PH","雙",6,"150~240KW","500A","V","V","V","V"]
[]
[null,"DX"]
[null,"Model Name"]
[null,"DXYE182E00E1PH","250A With LED tower at bottom side"]
[null,"DXYE182E00E2PH","250A, Without LED tower"]
[null,"DXYE362E00E1PH","500A, without relay"]