{"text_format":"2","workbook":"xlsx","n_sheets":6,"sheets":["Revision","Naming Rule","所有AC model name","所有DC model name","Customization","工作表2"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Revision","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[[2,3,5,5]]}
[]
[]
[null,null,null,"PHIHONG EVSE Model Name Naming Rule"]
[]
[]
[]
[]
[null,null,"Revision History"]
[null,null,"Rev","Date","Description","Editor"]
[null,null,"01","2019/01/24","First issue","Vern Chang"]
[null,null,"02","2019/02/13","Second issue after discussion","Vern Chang"]
[null,null,"03","2019/03/25","Modify Naming Rule","Vincent Tsai"]
[null,null,"04","2019/05/16","1. Redefine:\n(a) DM : DC EVSE Moveable\n(b) DR : DC EVSE Roadside (Battery equipped)\n\n2. Correcting:\n(a) Ac => AC\n(b) Evse => EVSE","Joseph Chiu"]
[null,null,"05","2019/06/11","new item to connector type field","Vern Chang"]
[null,null,"06","2019/07/10","DC all models added","Audrey Chen"]

{"sheet":"Naming Rule","index":1,"n_rows":96,"n_cols":61,"rows_kept":96,"cut":false,"hidden":false,"merged":[[18,24,22,28],[95,3,105,27],[61,10,70,27],[51,14,59,27],[72,6,93,27],[24,21,30,27],[32,17,49,27],[5,27,12,32],[1,26,1,27],[2,26,2,27],[1,13,1,14],[2,13,2,14],[1,16,1,18],[2,16,2,18],[2,23,2,24],[1,23,1,24],[1,2,1,3],[2,2,2,3],[1,9,1,11],[2,9,2,11],[1,20,1,21],[2,20,2,21],[1,5,1,7],[2,5,2,7]]}
[]
[null,null,"Type",null,null,"Input Configuration",null,null,null,"Safety Regulation",null,null,null,"Rated Power",null,null,"Connector/Socket Type",null,null,null,"Network Option",null,null,"Generation",null,null,"Customization"]
[null,null,"X X",null,null,"X",null,null,null,"X",null,null,null,"X1 X2 X3",null,null,"X1 X2 X3",null,null,null,"X",null,null,"X",null,null,"X1 X2 "]
[]
[]
[{"$nulls":27},"X1= Customer Name, X2 : Customization\n\nP0: Phihong Standard"]
{"$rows_empty":12}
[{"$nulls":24},"1  : Generation 1\n2  : Generation 2 \n3  : Generation 3\n4  : Generation 4"]
[]
[]
[]
[]
[]
[{"$nulls":21},"0  : None  (w/o Ethernet, w/o RFID)\nR  : None  (* Include RFID)\nE  : Ethernet only (* Include RFID)\nB  : Bluetooth only (* Include RFID) \nW : Ethernet + WiFi (* Include RFID)\nT   : Ethernet + 4G (* Include RFID)\nU  : Ethernet + Bluetooth (* Include RFID)\n"]
{"$rows_empty":7}
[{"$nulls":17},"X1X2X3 = Connector/Socket 1, 2 and 3 from left to right\n\n0 : none\n1 : IEC 62196-2 Type 1/SAE J1772 Plug\n2 : IEC 62196-2 Type 1/SAE J1772 Socket\n3 : IEC 62196-2 Type 2 Plug\n4 : IEC 62196-2 Type 2 Socket\n5 : GB/T AC Plug\n6 : GB/T AC Socket\nJ : CHAdeMO\nU : CCS1 combo\nE : CCS2 combo\nG : GBT DC\nD :  GBT DC x 2 \n\ne.g., \n1JU : SAE J1772 plug + CHAdeMO + CCS1\nGGD :  GBT DC x 4",{"$nulls":42},"ssssss"]
{"$rows_empty":18}
[{"$nulls":14},"X1X2X3 = (X1 x 10 + X2) x 10^(-1+X3)  kW\ne.g., \n190 : 1.9 kW (AC 120V with 16A)\n310 : 3.1 kW (AC 240V with 13A)\n380 : 3.8 kW (AC 240V with 16A)\n770 : 7.7 kW (AC 240V with 32A)\n251 : 25 kW \n301 : 30 kW\n362 : 360 kW"]
[]
[]
[]
[]
[]
[{"$nulls":50},"s"]
[]
[]
[]
[{"$nulls":10},"E  : CE / European Market\nU  : UL / North America Market\nG : GB / China Market\nC  : CNS / Taiwan Market\nJ   : JARI / Japan Market\nT   : TR25 / Singapor Market\nK  : KC / Korea Market\nB  : British / UK Market\nZ   : EV ready / French Market\n"]
{"$rows_empty":10}
[{"$nulls":6},"Hardwire Type:\nY : 3 phase wyi-connection 4 wires + PE,  380 - 415Vac, 50Hz/60Hz ; [ Note.3 phase 5 wires = L1(R) / L2(S) / L3(T) / N / PE ]\nD : 3 phase delta-connection 3 wires + PE, 200 - 240Vac, 50Hz/60Hz ; [ Note. 3 phase 4 wires = L1(R) / L2(S) / L3(T) / PE ]\nL :  2 phase 2 wires + PE, 200 - 240Vac, 50Hz/60Hz  ; [ Note. 2 phase 3 wires = L1 / L2 / PE ]\nS : 1 phase 2 wires + PE, 220 - 240Vac, 50Hz/60Hz ; [ Note. 1 phase 3 wires = L / N / PE ]\nW : 3 phase wyi-connection 4 wires + PE, 380 - 480Vac, 50Hz/60Hz ; [ Note. 3 phase 5 wires = L1(R) / L2(S) / L3(T) / N / PE ]\nT : 1 phase 2 wires + PE, 220 - 277Vac, 50Hz/60Hz ; [ Note. 1 phase 3 wires = L1or L2 or L3 / N / PE ]\nF : 2 phase 2 wires + PE, 120 - 240Vac, 50Hz/60Hz. ; [ Note. 2 phase 3 wires = L1 / L2 / PE ]\n\nAC Plug Type:\n0 : 1 phase 2 wires + PE, CEE 7/7 plug (compatible with Type E and Type F), 220 - 240Vac, 50Hz/60Hz. (For European)\n1 : 1 phase 2 wires + PE, BS 1363 plug (Type G), 220 - 240Vac, 50Hz/60Hz. (For UK)\n2 : 1 phase 2 wires + PE, AS/NZS 3112 (Type I), 220 - 240Vac, 50Hz/60Hz. (For Australia, New Zealand)\n3 : 1 phase 2 wires + PE, GB 2099.1‐2008 and GB 1002‐2008 (Type I), 220 - 240Vac, 50Hz/60Hz. (For China)\n4 : 1 phase 2 wires + PE, IS1293 plug (Type M), 220 - 240Vac, 50Hz/60Hz. (For Indian and South African)\n5 : 2 phase 2 wires + PE, NEMA 5-15 plug (Type B), 120 Vac, 50Hz/60Hz.(For UL, TW, Japan)\n6 : 2 phase 2 wires + PE, NEMA 6-20 plug, 200 - 240Vac, 50Hz/60Hz. (For UL, TW)\n7 : 2 phase 2 wires + PE, NEMA 14-20 plug, 120 - 240Vac, 50Hz/60Hz. (For UL)\n8 : 2 phase 2 wires + PE, NEMA 14-50 plug, 120 - 240Vac, 50Hz/60Hz. (For UL)"]
{"$rows_empty":22}
[null,null,null,"AC : AC EVSE Cordset \nAW : AC EVSE Wallmount (Regular)\nAH : AC EVSE Wallmount (Luxury)-->AC32\nAP  : AC EVSE Pedestal\nDW : DC EVSE Wallmount\nDS   : DC EVSE Standalone\nDM : DC EVSE Moveable\nDR  : DC EVSE Roadside (Battery equipped)\nDD  : DC EVSE Dispenser\nDO : DC EVSE Output power cabinet\n"]

{"sheet":"所有AC model name","index":2,"n_rows":12,"n_cols":29,"rows_kept":12,"cut":false,"hidden":false,"merged":[[39,20,39,21],[40,20,40,21],[41,20,41,21],[35,4,35,6],[35,8,35,10],[35,20,35,21],[36,20,36,21],[37,20,37,21],[38,20,38,21],[33,4,33,6],[33,8,33,10],[33,20,33,21],[33,23,33,24],[34,4,34,6],[34,8,34,10],[34,20,34,21],[34,23,34,24],[31,4,31,6],[31,8,31,10],[31,20,31,21],[31,23,31,24],[32,4,32,6],[32,8,32,10],[32,20,32,21],[32,23,32,24],[29,4,29,6],[29,8,29,10],[29,20,29,21],[29,23,29,24],[30,4,30,6],[30,8,30,10],[30,20,30,21],[30,23,30,24],[27,4,27,6],[27,8,27,10],[27,20,27,21],[27,23,27,24],[28,4,28,6],[28,8,28,10],[28,20,28,21],[28,23,28,24],[25,4,25,6],[25,8,25,10],[25,20,25,21],[25,23,25,24],[26,4,26,6],[26,8,26,10],[26,20,26,21],[26,23,26,24],[23,4,23,6],[23,8,23,10],[23,20,23,21],[23,23,23,24],[24,4,24,6],[24,8,24,10],[24,20,24,21],[24,23,24,24],[21,4,21,6],[21,8,21,10],[21,20,21,21],[21,23,21,24],[22,4,22,6],[22,8,22,10],[22,20,22,21],[22,23,22,24],[19,4,19,6],[19,8,19,10],[19,20,19,21],[19,23,19,24],[20,4,20,6],[20,8,20,10],[20,20,20,21],[20,23,20,24],[17,4,17,6],[17,8,17,10],[17,20,17,21],[17,23,17,24],[18,4,18,6],[18,8,18,10],[18,20,18,21],[18,23,18,24],[15,4,15,6],[15,8,15,10],[15,20,15,21],[15,23,15,24],[16,4,16,6],[16,8,16,10],[16,20,16,21],[16,23,16,24],[13,4,13,6],[13,8,13,10],[13,20,13,21],[13,23,13,24],[14,4,14,6],[14,8,14,10],[14,20,14,21],[14,23,14,24],[11,4,11,6],[11,8,11,10],[11,20,11,21],[11,23,11,24],[12,4,12,6],[12,8,12,10],[12,20,12,21],[12,23,12,24],[9,4,9,6],[9,8,9,10],[9,20,9,21],[9,23,9,24],[10,4,10,6],[10,8,10,10],[10,20,10,21],[10,23,10,24],[7,4,7,6],[7,8,7,10],[7,20,7,21],[7,23,7,24],[8,4,8,6],[8,8,8,10],[8,20,8,21],[8,23,8,24],[5,4,5,6],[5,8,5,10],[5,20,5,21],[5,23,5,24],[6,4,6,6],[6,8,6,10],[6,20,6,21],[6,23,6,24],[3,4,3,6],[3,8,3,10],[3,20,3,21],[3,23,3,24],[4,4,4,6],[4,8,4,10],[4,20,4,21],[4,23,4,24],[1,23,1,24],[1,26,1,27],[2,1,2,2],[2,4,2,6],[2,8,2,10],[2,12,2,14],[2,16,2,18],[2,20,2,21],[2,23,2,24],[2,26,2,27],[1,1,1,2],[1,4,1,6],[1,8,1,10],[1,12,1,14],[1,16,1,18],[1,20,1,21]]}
[]
[null,"Type",null,null,"Input Configuration",null,null,null,"Safety Regulation",null,null,null,"Rated Power",null,null,null,"Connector/Socket Type",null,null,null,"Network Option",null,null,"Generation",null,null,"Customization"]
[null,"X X",null,null,"X",null,null,null,"X",null,null,null,"X1 X2 X3",null,null,null,"X1 X2 X3",null,null,null,"X",null,null,"X",null,null,"X X "]
[null,"A","W",null,"L",null,null,null,"U",null,null,null,7,0,0,null,0,0,1,null,"E",null,null,1,null,null,"P","H","簡易低價版 美規連網"]
[null,"A","W",null,"L",null,null,null,"E",null,null,null,7,0,0,null,0,0,1,null,"E",null,null,1,null,null,"P","H","簡易低價版 歐規連網"]
[null,"A","W",null,"L",null,null,null,"U",null,null,null,7,0,0,null,0,0,1,null,"E",null,null,2,null,null,"P","H","簡易中價版 美規連網"]
[null,"A","W",null,"L",null,null,null,"U",null,null,null,7,0,0,null,0,0,1,null,"W",null,null,2,null,null,"P","H","簡易中價版 美規連網 WIFI"]
[null,"A","W",null,"L",null,null,null,"U",null,null,null,7,0,0,null,0,0,1,null,"T",null,null,2,null,null,"P","H","簡易中價版 美規連網 4G"]
[null,"A","W",null,"L",null,null,null,"E",null,null,null,7,0,0,null,0,0,1,null,"E",null,null,2,null,null,"P","H","簡易中價版 歐規連網"]
[null,"A","W",null,"L",null,null,null,"E",null,null,null,7,0,0,null,0,0,1,null,"W",null,null,2,null,null,"P","H","簡易中價版 歐規連網 WIFI"]
[null,"A","W",null,"L",null,null,null,"E",null,null,null,7,0,0,null,0,0,1,null,"T",null,null,2,null,null,"P","H","簡易中價版 歐規連網 4G"]
[null,"A","P",null,"S",null,null,null,"C",null,null,null,1,6,0,null,0,0,0,null,"E",null,null,1,null,null,"J","H","巨漢工程廣告樁"]

{"sheet":"所有DC model name","index":3,"n_rows":27,"n_cols":20,"rows_kept":27,"cut":false,"hidden":false,"merged":[[5,1,5,4],[18,1,18,4],[23,1,23,4],[3,12,3,14],[3,17,3,18],[4,5,4,6],[3,1,4,1],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,3,6],[3,9,3,11]]}
[]
[null,"DC Charger Model Name List"]
[]
[null,"Item \nNo","Established\nDate","Customer","Description","Type",null,"Input \nConfiguration","Safety \nRegulation","Rated Power",null,null,"Connector/\nSocket Type",null,null,"Network \nOption","Generation","Customization",null,"-RW"]
[{"$nulls":5},"X1 X2",null,"X3","X4","X5","X6","X7","X8","X9","X10","X11","X12","X13","X14"]
[null,"Standalone"]
[null,null,"2019-02-20","Phihong","60KW歐規雙槍黑白機 F-750","D","S","Y","E",6,0,1,"J",0,"E","T",1,"P","H","-RW"]
[null,null,"2019-07-10","Phihong","60KW歐規雙槍黑白機 F-750","D","S","W","U",6,0,1,"J",0,"U","T",1,"P","H","-RW"]
[]
[null,null,"2019-03-14","Phihong","60KW三槍 CSU3.0 F-750-V","D","S","Y","E",6,0,1,"J",4,"E","T",2,"P","H","-RW"]
[null,null,"2019-03-14","Phihong","120KW三槍 CSU3.0 F-750-V","D","S","Y","E",1,2,2,"J",4,"E","T",2,"P","H","-RW"]
[]
[null,null,"2019-05-28","Plugit","180KW Plugit Power Rack F-750","D","S","Y","E",1,8,2,"E",0,"G",0,1,"L",0,"-RW"]
[null,null,null,"Plugit","210KW Plugit Power Rack F-750","D","S","Y","E",2,1,2,"E",0,"G",0,1,"L",0,"-RW"]
[null,null,null,"Plugit","210KW Plugit Power Rack F-750","D","S","Y","E",2,1,2,"G",0,"E",0,1,"L",0,"-RW"]
[]
[null,null,"2019-05-28","沙崙瑞助","30KW Standalone F-750","D","S","Y","C",3,0,1,"J",0,"U","E",1,"P","H","-RW"]
[]
[null,"Movable"]
[null,null,"2019-05-28","Phihong","30KW Movable F-750","D","M","Y","E",3,0,1,"E",0,0,"T",1,"P","H","-RW"]
[null,null,null,"Phihong","30KW Movable F-750","D","M","Y","E",3,0,1,"G",0,0,"T",1,"P","H","-RW"]
[]
[]
[null,"Wallbox"]
[null,null,"2019-04-16","Phihong","25KW Wallbox","D","W","Y","E",2,5,1,"J",0,"E","T",1,"P","H","-RW"]
[null,null,null,"Phihong","25KW Wallbox","D","W","W","U",2,5,1,"J",0,"U","T",1,"P","H","-RW"]
[null,null,null,"Phihong","25KW Wallbox","D","W","W","C",2,5,1,"J",0,"U","T",1,"P","H","-RW"]

{"sheet":"Customization","index":4,"n_rows":4,"n_cols":3,"rows_kept":4,"cut":false,"hidden":false,"merged":[[0,0,0,1],[1,0,1,1]]}
["Customization"]
["X1 X2 ",null,"Note."]
["X1 : Customer Name","X2 : Customization"]
["P",0,"P = Phihong Standard,  0 = Cable legth 5m, "]

{"sheet":"工作表2","index":5,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}